#N canvas 426 75 567 654 10;
#X obj 8 625 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 8 415 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 8 458 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 8 591 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 109 427 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 110 469 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 135 427 signal;
#X text 135 469 signal;
#X text 141 600 (none);
#X obj 218 196 bng 20 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 218 275 cyclone/framedelta~;
#X obj 395 269 cyclone/framedelta~;
#X obj 395 295 cyclone/phasewrap~;
#X text 111 197 start counter =>;
#X text 138 513 For each signal block \, the first sample of its output will be the first sample in the current block minus the first sample in the previous block \, the second sample of its output will be the second sample in the current block minus the second sample in the previous block \, and so on.;
#X obj 9 501 cnv 3 550 3 empty empty more_info 8 12 0 13 #dcdcdc #000000 0;
#X text 81 92 The [framedelta~] object was designed specially to compute a running phase deviation of a FFT analysis by subtracting values in each position of its previously received signal block from the current signal block. When used in a FFT subpatch \, it can keep a running phase deviation of the FFT because the FFT size is equal to the block size.;
#X obj 218 227 cyclone/count~;
#X text 199 469 - Deviation between successive FFT frames;
#X text 199 427 - The input on which the deviation will be computed;
#X text 365 217 properly check phase deviation;
#X text 391 235 with [phasewrap~];
#X obj 497 71 cyclone/dsponoff~;
#X obj 2 5 ./header framedelta~;
#X text 22 61 FFT frame deviation;
#X obj 75 281 cyclone/snapshot~ 1;
#X floatatom 75 310 11 0 0 0 - - - 12;
#X obj 218 312 cyclone/snapshot~ 1;
#X floatatom 218 341 5 0 0 0 - - - 12;
#X text 194 382 see also:;
#X obj 259 381 cyclone/frameaccum~;
#X connect 9 0 17 0;
#X connect 10 0 27 0;
#X connect 11 0 12 0;
#X connect 17 0 10 0;
#X connect 17 0 25 0;
#X connect 25 0 26 0;
#X connect 27 0 28 0;
