#N canvas 396 48 561 616 10;
#X obj 4 587 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 5 313 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 5 407 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 5 439 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 77 322 cnv 17 3 80 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X msg 299 198 write;
#X msg 229 187 clear;
#X text 133 320 signal;
#X obj 278 136 bng 25 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 278 170 cyclone/count~;
#X text 103 227 click to open text window =>;
#X text 185 338 - clear stored values and starts capturing again;
#X text 139 337 clear;
#X text 145 370 open;
#X text 184 387 - closes text window;
#X text 133 387 wclose;
#X text 184 371 - opens text window (like double clicking);
#X text 185 319 - signal to be stored in a text format;
#X text 186 536 - decimal precision (default 4);
#X text 115 447 1) symbol;
#X text 115 515 2) float;
#X text 115 535 3) float;
#X text 115 552 4) list;
#X text 133 415 (none);
#X text 185 415 - but the stored values can be copied or saved to a file;
#X text 185 447 -;
#X text 196 446 optional flag "f" for "first mode" - where collecting data stops after receiving the specified number of samples. If not given \, the default is "last mode" \, where it continues to collect data \, throwing away old values if it has received more than the specified samples, f 58;
#X text 186 516 - number of samples to store (default 4096);
#X obj 278 227 cyclone/capture~ f 64 1 0 1 2 3;
#X text 85 354 write <symbol>;
#X text 184 355 - save to file (no symbol opens dialog box);
#X text 187 554 -;
#X text 198 552 up to 10 number indices within a signal block. If no list is given \, entire block is stored, f 58;
#X text 167 138 start [count~] =>;
#X text 166 154 and clear data;
#X text 346 199 write to a text file;
#X obj 501 69 cyclone/dsponoff~;
#X obj 2 3 ./header capture~;
#X text 23 59 Store samples;
#X text 66 86 [capture~] is designed for signal debugging/investigation \, it captures samples into a text window or text file. [capture~]'s window holds limited data \, so you can capture more than you can see. If so \, write it to a text file and open elsewhere;
#X text 54 276 see also:;
#X obj 121 277 cyclone/capture;
#X obj 268 277 print~;
#X text 237 276 and;
#X obj 320 277 tabwrite~;
#X text 383 277 for vanilla alternatives;
#X connect 5 0 28 0;
#X connect 6 0 28 0;
#X connect 8 0 6 0;
#X connect 8 0 9 0;
#X connect 9 0 28 0;
