#N canvas 451 37 565 591 10;
#X obj 4 437 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 4 485 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 4 526 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 113 494 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 113 451 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 158 494 signal;
#X text 159 535 (none);
#X obj 4 558 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 185 158 hsl 180 15 1e-05 1 0 0 empty empty empty -2 -8 0 10 #dcdcdc #000000 #000000 0 1;
#X obj 182 245 cyclone/atodb~;
#X text 223 157 Linear Amplitude;
#X text 215 451 - linear amplitude value;
#X text 156 451 signal;
#X obj 182 212 sig~;
#X text 216 495 - converted dBFS amplitude value;
#X text 146 308 dBFS;
#X obj 182 187 nbx 8 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 500 69 cyclone/dsponoff~;
#X obj 4 2 header atodb~;
#X text 20 59 Linear amplitude to dBFS conversion for signals;
#X obj 182 280 cyclone/snapshot~ 1;
#X obj 182 310 nbx 9 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 361 273 The above is a Vanilla alternative, f 12;
#X obj 372 225 rmstodb~;
#X obj 372 246 -~ 100;
#X text 46 95 Use the [atodb~] to convert a signal representing a linear amplitude value to a deciBel Full Scale (dBFS) equivalent. The conversion formula is: dbFS = log10(amp) * 20 (minimum output value is -999)., f 68;
#X obj 92 371 cyclone/atodb;
#X obj 93 394 cyclone/dbtoa~;
#X text 17 385 see also:;
#X text 194 377 Plugdata users or those with ELSE can also use [else/lin2db~] as an alternative, f 41;
#X text 468 355 click:;
#X obj 470 396 open-else;
#X msg 470 375 lin2db~;
#X connect 8 0 16 0;
#X connect 9 0 20 0;
#X connect 13 0 9 0;
#X connect 16 0 13 0;
#X connect 20 0 21 0;
#X connect 23 0 24 0;
#X connect 32 0 31 0;
