#N canvas 495 44 558 614 10;
#X obj 2 334 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 486 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 518 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 81 495 cnv 17 3 17 empty empty n 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 81 344 cnv 17 3 136 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 88 149 bng 17 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 2 581 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X text 132 380 bang;
#X text 126 348 float;
#X text 126 497 float;
#X text 105 526 1) float;
#X text 105 544 2) float;
#X obj 88 254 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 123 254 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 158 254 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 193 254 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 88 199 nbx 2 14 -9 99 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 174 526 - sets number of outlets (default 1), f 60;
#N canvas 823 75 391 268 output-flag 0;
#X obj 214 26 bng 17 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 214 76 nbx 2 14 -9 99 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 214 50 random 100;
#X obj 214 168 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 249 168 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 284 168 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 319 168 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 214 136 cyclone/bucket 4 1;
#X obj 38 173 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 73 173 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 108 173 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 143 173 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 38 141 cyclone/bucket 4 0;
#X text 78 211 (default);
#X text 51 55 set as 2nd arguments;
#X text 31 195 <0> holds to next round;
#X text 204 194 <1> outputs immediately;
#X connect 0 0 2 0;
#X connect 1 0 12 0;
#X connect 1 0 7 0;
#X connect 2 0 1 0;
#X connect 7 0 3 0;
#X connect 7 1 4 0;
#X connect 7 2 5 0;
#X connect 7 3 6 0;
#X connect 12 0 8 0;
#X connect 12 1 9 0;
#X connect 12 2 10 0;
#X connect 12 3 11 0;
#X restore 450 250 pd output-flag;
#X text 138 430 l2r;
#X text 138 447 r2l;
#X text 177 430 - or 'L2R'/'ltor': sets shift from left to right (default);
#X text 177 447 - or 'R2L'/'rtol': sets shift from right to left;
#X text 90 364 set <float>;
#X text 132 464 roll;
#X text 132 413 thaw;
#X text 120 396 freeze;
#X msg 310 136 freeze;
#X msg 317 160 thaw;
#X msg 331 188 l2r;
#X msg 337 210 r2l;
#X msg 372 217 roll;
#X msg 237 172 set \$1;
#X floatatom 237 151 5 0 0 0 - - - 0;
#X obj 310 251 send bucket;
#X obj 287 174 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 140 197 r bucket;
#X text 177 348 - the input number, f 60;
#X text 177 364 - sets input value and outputs it to all outlets;
#X text 177 380 - outputs all stored values without shifting, f 60;
#X text 177 396 - suspends output \, but continues to shift input internally;
#X text 177 413 - resumes the output after being freezed, f 51;
#X text 177 464 - shifts stores values in loop (according to direction);
#X text 177 497 - numbers being passed;
#X obj 88 224 cyclone/bucket 4 1;
#X obj 88 173 random 100;
#X text 174 544 - output flag: <0> (default) holds the input and passes it on the next round \, <1> outputs the input immediately;
#X obj 3 4 header bucket;
#X text 22 62 Pass numbers from outlet to outlet;
#X text 49 87 As [bucket] is input with floats \, it outputs them shiftting from outlet to outlet in a rotational pattern (or "passing the bucket" as in a bucket brigade).;
#X obj 211 298 cyclone/cycle;
#X text 142 297 see also:;
#X obj 301 298 cyclone/spray;
#X connect 5 0 45 0;
#X connect 16 0 44 0;
#X connect 27 0 34 0;
#X connect 28 0 34 0;
#X connect 29 0 34 0;
#X connect 30 0 34 0;
#X connect 31 0 34 0;
#X connect 32 0 34 0;
#X connect 33 0 32 0;
#X connect 35 0 34 0;
#X connect 36 0 44 0;
#X connect 44 0 12 0;
#X connect 44 1 13 0;
#X connect 44 2 14 0;
#X connect 44 3 15 0;
#X connect 45 0 16 0;
