#N canvas 452 27 560 587 10;
#X declare -stdpath ./;
#X obj 4 553 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 5 461 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 5 501 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 97 472 cnv 17 3 17 empty empty n 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 167 472 signal;
#X text 155 526 2) float;
#X floatatom 159 215 5 0 0 0 - - - 0;
#X obj 159 147 vradio 15 1 0 4 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0;
#X text 177 146 none;
#X text 177 161 1st outlet;
#X text 177 177 2nd outlet;
#X text 177 193 3rd outlet;
#X obj 5 400 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 97 409 cnv 17 3 27 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 97 441 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 131 408 float/signal;
#N canvas 726 248 416 434 signal-rate 0;
#X obj 139 272 cyclone/gate~ 2;
#X obj 139 125 *~ 3;
#X obj 139 86 phasor~ 0.5;
#X text 37 22 You can set the outlet number with a signal input \, this allows gate to be controlle with sample accuracy. Signal values are truncated to integers.;
#X obj 226 234 noise~;
#X obj 136 310 output~;
#X obj 162 158 cyclone/snapshot~ 1;
#X floatatom 162 187 15 0 0 0 - - - 0;
#X obj 142 391 declare -stdpath ./;
#X connect 0 0 5 0;
#X connect 0 1 5 1;
#X connect 1 0 0 0;
#X connect 1 0 6 0;
#X connect 2 0 1 0;
#X connect 4 0 0 1;
#X connect 6 0 7 0;
#X restore 377 240 pd signal-rate;
#X text 167 441 signal;
#X text 220 441 - signal to be routed;
#X obj 159 236 cyclone/gate~ 3 1;
#X text 155 509 1) float;
#X text 220 472 - 'n' outlets for routing input signal;
#X text 221 527 - initial outlet to route to (default 0 - none);
#X text 220 507 - 'n' number of outlets (1 to 500 \, default 1);
#X text 58 89 [gate~] routes an input signal from the second inlet to one of 'n' specified outlets or none of them. If an outlet is not selected \, it outputs zero values.;
#X text 220 408 -;
#X text 231 408 outlet number to route to - values are truncated to integers and clipped from 0 to number of outlets, f 52;
#X obj 497 71 cyclone/dsponoff~;
#X text 22 61 Route a signal to 'n' outlet(s);
#X obj 3 1 ./header gate~;
#X obj 258 208 noise~;
#X obj 159 265 env~;
#X floatatom 159 286 5 0 0 0 - - - 0;
#X obj 208 265 env~;
#X floatatom 208 286 5 0 0 0 - - - 0;
#X obj 258 265 env~;
#X floatatom 258 286 5 0 0 0 - - - 0;
#X text 47 329 see also:;
#X obj 412 369 open-else;
#X msg 412 319 xgate~;
#X text 475 332 click;
#X msg 420 340 xgate2~;
#X obj 44 352 cyclone/selector~;
#X text 168 332 Plugdata users or those with ELSE can use the much better [else/xgate~] or [else/xgate~] objects instead (see also their multichannel variations)., f 38;
#X connect 6 0 19 0;
#X connect 7 0 6 0;
#X connect 19 0 31 0;
#X connect 19 1 33 0;
#X connect 19 2 35 0;
#X connect 30 0 19 1;
#X connect 31 0 32 0;
#X connect 33 0 34 0;
#X connect 35 0 36 0;
#X connect 39 0 38 0;
#X connect 41 0 38 0;
