#N canvas 319 23 563 572 10;
#X obj 2 398 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 470 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 507 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 101 408 cnv 17 3 55 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 101 481 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 2 545 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X msg 246 190 set 25;
#X msg 252 219 clear;
#X obj 184 279 bng 20 250 50 0 empty empty empty 17 7 0 10 #d0d0d0 #000000 #000000;
#X text 178 409 -;
#X text 144 409 list;
#X text 178 481 -;
#X text 145 481 bang;
#X text 112 446 set <list> -;
#X text 142 428 clear -;
#X text 193 428 clears the memory so a next input may trigger a bang;
#X obj 187 166 hsl 128 15 0 127 0 0 empty empty empty -2 -8 0 10 #dcdcdc #000000 #000000 0 1;
#X obj 184 193 nbx 4 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 184 254 cyclone/past 63.5;
#X text 169 519 - value(s) of initial threshold(s) - required (no defaults);
#X text 104 179 compare to threshold =>, f 12;
#X text 292 191 sets new threshold;
#X text 294 214 clears last input \, so a new input may trigger if >= the threshold, f 33;
#N canvas 813 130 401 324 lists 0;
#X obj 163 278 bng 20 250 50 0 empty empty empty 17 7 0 10 #d0d0d0 #000000 #000000;
#X msg 106 178 clear;
#X text 19 20 The numbers of an input list can be compared to a list of thresholds set via arguments or a "set" message \, but only if they have the same length.;
#X msg 163 155 8 256 2 512;
#X msg 186 187 8 256 1 512;
#X text 20 73 A bang is output if all elements in the list are greater than (or 'past') the corresponding thresholds. If any of the input values fall bacl equal to or below a corresponding threshold \, another bang may be output again when the values are greater.;
#X msg 201 219 set 2 128 0 256;
#X obj 163 247 cyclone/past 4 128 1 256;
#X connect 1 0 7 0;
#X connect 3 0 7 0;
#X connect 4 0 7 0;
#X connect 6 0 7 0;
#X connect 7 0 0 0;
#X restore 485 275 pd lists;
#X text 193 446 sets threshold to one or more values, f 52;
#X text 70 93 [past] bangs when an input is greater than a threshold value and the last value was below or equal to it. The input needs to fall back to a value equal or below the threshold for another bang to be output when it goes past it again.;
#X text 193 481 if input is > threshold value(s) but last input wasn't;
#X text 193 409 values to check if went past a list of thresholds, f 52;
#X text 120 519 1) list;
#X text 296 253 <-- initial threshold;
#X obj 4 2 ./header past;
#X text 24 61 Check if input increases past a threshold;
#X obj 402 362 open-else;
#X text 443 336 click;
#X text 64 347 see also:;
#X msg 402 336 above;
#X text 138 340 Plugdata users or those with ELSE can also use [else/above] as an alternative, f 40;
#X connect 6 0 18 0;
#X connect 7 0 18 0;
#X connect 16 0 17 0;
#X connect 17 0 18 0;
#X connect 18 0 8 0;
#X connect 35 0 32 0;
