#N canvas 469 23 558 588 10;
#X obj 2 384 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 463 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 507 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 94 393 cnv 17 3 36 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 94 435 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X msg 433 186 symbol bar;
#X obj 94 475 cnv 17 3 17 empty empty n 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 97 142 vradio 15 1 0 4 sdvs asfgasgf empty 0 -8 0 10 #dcdcdc #000000 #000000 0;
#X obj 2 562 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X text 144 393 bang;
#X text 138 414 float;
#X text 120 436 anything;
#X text 120 476 anything;
#X obj 190 197 nbx 3 15 -1e+37 1e+37 0 0 xfkvds asfmnv empty 0 -8 0 12 #dcdcdc #000000 #000000 0 256;
#X obj 97 212 nbx 2 15 -1e+37 1e+37 0 0 xfkvds asfmnv empty 0 -8 0 12 #dcdcdc #000000 #000000 0 256;
#X obj 190 260 nbx 3 13 -1e+37 1e+37 0 0 xfkvds asfmnv empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 143 260 nbx 3 13 -1e+37 1e+37 0 0 xfkvds asfmnv empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 97 260 nbx 3 13 -1e+37 1e+37 0 0 xfkvds asfmnv empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 186 414 - sets outlet number (0 is none), f 33;
#X text 186 436 - message to send through a specified outlet;
#X text 115 142 none;
#X text 115 157 1st;
#X text 115 172 2nd;
#X text 115 187 3rd;
#X text 51 172 outlet;
#X text 68 91 [gate] routes a message from the second inlet to one of 'n' specified outlets or none of them.;
#X text 186 393 - reports the open outlet number on the left outlet, f 52;
#X text 120 516 1) float;
#X obj 317 180 tgl 15 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000 0 1;
#X obj 317 214 cyclone/gate, f 18;
#X text 45 158 specify;
#X obj 190 280 bng 15 250 50 0 empty empty empty 17 7 0 10 #fcfcfc #000000 #000000;
#X obj 143 280 bng 15 250 50 0 empty empty empty 17 7 0 10 #fcfcfc #000000 #000000;
#X obj 97 280 bng 15 250 50 0 empty empty empty 17 7 0 10 #fcfcfc #000000 #000000;
#X obj 395 161 bng 15 250 50 0 empty empty empty 17 7 0 10 #fcfcfc #000000 #000000;
#X msg 422 157 1 2 3;
#X msg 451 214 x;
#X obj 317 262 print;
#X obj 284 180 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 334 240 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X text 120 536 2) float;
#X obj 97 234 cyclone/gate 3 1;
#X text 186 536 - sets initially open outlet (default 0 - none);
#X text 186 477 - 'n' outlets for routing any received message;
#X text 190 175 float;
#X text 405 133 other messages;
#X text 186 516 - 'n' number of outlets (1 to 100 \, default 1);
#X obj 4 3 ./header gate;
#X text 22 61 Route message to an outlet;
#X text 60 333 see also:;
#X obj 429 347 open-else;
#X msg 429 325 selector;
#X text 437 303 click:;
#X text 141 328 Plugdata users or those with ELSE can also use [else/selector] as an alternative, f 42;
#X connect 5 0 29 1;
#X connect 7 0 14 0;
#X connect 13 0 41 1;
#X connect 14 0 41 0;
#X connect 15 0 31 0;
#X connect 16 0 32 0;
#X connect 17 0 33 0;
#X connect 28 0 29 0;
#X connect 29 0 37 0;
#X connect 29 0 39 0;
#X connect 34 0 29 1;
#X connect 35 0 29 1;
#X connect 36 0 29 1;
#X connect 38 0 29 0;
#X connect 41 0 17 0;
#X connect 41 1 16 0;
#X connect 41 2 15 0;
#X connect 51 0 50 0;
