arduino-simple-tts

Loading...
Searching...
No Matches
Class Hierarchy
This inheritance list is sorted roughly, but not completely, alphabetically:
[detail level 12]

▼C simple_tts::AudioDictionaryBase | Dictionary which provides a Stream of Audio for the indicated word
C simple_tts::AudioDictionary | A dictionary which is based on in memory audio files
C simple_tts::AudioDictionarySD | A dictionary which is based on files stored on an SD card. By default we use the SdFat library. You can use the SD library with #define USE_SD before including this file
C simple_tts::AudioDictionaryURL | A dictionary which is based on audio files that can be accessed via URLs
C simple_tts::AudioDictionaryEntry | An Entry for the in Memory Audio Dictionary
C simple_tts::AudioSDEntry | An Entry for the in Memory Audio Dictionary which contains the full text
▼CAudioStream |
C simple_tts::AudioStreamFileWrapper< AudioFile > |
C simple_tts::AudioStreamFileWrapper< T > | A simple Wrapper that let's a file pretend to be a AudioStream to support the begin and end methods
C simple_tts::NumberUnitToText::DecimalInfo | Units might have different decimals. The decimal system is based on 3. But currencies have usually 2
C simple_tts::Number | Convert numbers to string and provide integer and decimals
C simple_tts::SimpleTime | Just a simple structure with the hour and minutes
▼C simple_tts::SimpleTTSBase | Common Functionality for TTS classes
C simple_tts::NumberToText | Translates a number into englich words
C simple_tts::NumberUnitToText | An extension of the Number to Text functionality which supports numbers with units of measures
C simple_tts::TimeToText | Translates a time in hour and minutes into englich words. This implementation builds upon the NumberToText class to handle the basic numbers
C simple_tts::TextToSpeech | Audio output from text via the indicated audio sink. The text components need to be prerecorded and available as audio files
C simple_tts::TextToSpeechQueue | Audio output from text via the indicated audio sink. The text components need to be prerecorded and available as audio files