  
***

# Sad Mac

<!--
<details>
<summary><p>Click/tap here to expand/collapse</p>
<p>the dropdown containing the Mac OS X 10.0 logo</p></summary>

![https://github.com/seanpm2001/WacOS/blob/master/Graphics/MacOS_X/10.0_Cheetah/MacOS10.1.png](https://github.com/seanpm2001/WacOS/blob/master/Graphics/MacOS_X/10.0_Cheetah/MacOS10.1.png)

</details>
!-->

![https://github.com/seanpm2001/WacOS/blob/master/Graphics/Sad_Mac/Sad_mac.png](https://github.com/seanpm2001/WacOS/blob/master/Graphics/Sad_Mac/Sad_mac.png)

<!-- ( **Predecessor:** [Mac OS X Public Beta](https://github.com/seanpm2001/WacOS/wiki/Mac-OS-X-Public-Beta/) | **Successor:** [Mac OS X 10.1 (Puma)](https://github.com/seanpm2001/WacOS/wiki/Mac-OS-X-10-1-Puma/) ) !-->

<!-- **This article is a modified copy of the Wikipedia article of the same subject. It needs to be rewritten to be more original.** !-->

A Sad Mac is a symbol in older-generation Apple Macintosh computers (hardware using the Old World ROM and not Open Firmware, which are those predating onboard USB), starting with the original 128K Macintosh and ending with the last NuBus-based Power Macintosh models (including the first-generation 6100, 7100, 8100, as well as the PowerBook 5300 and 1400), to indicate a severe hardware or software problem that prevented startup from occurring successfully. The Sad Mac icon is displayed, along with a set of hexadecimal codes that indicate the type of problem at startup. Different codes are for different errors. This is in place of the normal Happy Mac icon, which indicates that the startup-time hardware tests were successful. In 68k models made after the Macintosh II, the Chimes of Death are played.

Models prior to the Macintosh II crash silently and display the Sad Mac, without playing any tone. PowerPC Macs play a sound effect of a car crash, and computers equipped with the PowerPC upgrade card use the three note brass fanfare death chime (A, E-natural, and E-flat), followed by the sound of a drum, same as the Macintosh Performa 6200 and Macintosh Performa 6300.

A Sad Mac may be deliberately generated at startup by pressing the interrupt switch on Macintosh computers that had one installed, or by pressing Command and Power keys shortly after the startup chime. On some Macintoshes such as PowerBook 540c, if the user presses the command and power keys before the boot screen displays, it will play the "chimes of death". The chimes are a fraction of normal speed and there is no Sad Mac displayed.

Old World ROM Power Macintosh and PowerBook models based on the PCI architecture do not use a Sad Mac icon and will instead only play the error/car-crash sound on a hardware failure (such as missing or bad memory, unusable CPU, or similar).

Mac OS X 10.2 Jaguar and later instead use the Universal "no" symbol to denote a hardware or software error that renders the computer non-bootable.

**This description is a copy and paste from Wikipedia and needs to be rewritten to be original.**

***

## WacOS equivalent

There is no equivalent for WacOS yet.

_This article on Classic Mac OS Graphics is a stub. You can help by expanding it._

***

## Sources

[Wikipedia - Macintosh Startup](https://en.wikipedia.org/wiki/Macintosh_startup#Happy_Mac)

Other sources are needed, because Wikipedia cannot be the only source, as Wikipedia shouldn't be used as a main source. <!-- this article needs LOTS of improvement and original work to prevent it from being a copy and paste from Wikipedia. !-->

***

## Article info

**Written on:** `2021 Tuesday September 21st at 8:01 pm`

**Last revised on:** `2021 Tuesday September 21st at 8:01 pm`

**File format** `Markdown document (*.md *.mkd *.markdown)`

**Article version:** `1 (2021 Tuesday September 21st at 8:01 pm)`

***

<!-- Tools

Quick copy and paste

https://github.com/seanpm2001/WacOS/wiki/

!-->

