.\" DO NOT MODIFY THIS FILE!  It was generated by help2man 1.49.3.
.TH ARV-CAMERA-TEST-0.10 "1" "novembre 2023" "arv-camera-test-0.10 0.9.0" "User Commands"
.SH NAME
arv-camera-test-0.10 \- manual page for arv-camera-test-0.10 0.9.0
.SH DESCRIPTION
.SS "Usage:"
.IP
arv\-camera\-test\-0.10 [OPTION?]
.PP
Small utility for basic device checks.
.SS "Help Options:"
.TP
\-?, \fB\-\-help\fR
Show help options
.SS "Application Options:"
.TP
\fB\-n\fR, \fB\-\-name=\fR<camera_id>
Camera name
.TP
\fB\-f\fR, \fB\-\-frequency=\fR<Hz>
Acquisition frequency
.TP
\fB\-t\fR, \fB\-\-trigger=\fR<trigger_id>
External trigger
.TP
\fB\-o\fR, \fB\-\-software\-trigger=\fR<Hz>
Emit software trigger
.TP
\fB\-w\fR, \fB\-\-width=\fR<n_pixels>
Width
.TP
\fB\-h\fR, \fB\-\-height=\fR<n_pixels>
Height
.TP
\fB\-\-h\-binning=\fR<n_pixels>
Horizontal binning
.TP
\fB\-\-v\-binning=\fR<n_pixels>
Vertical binning
.TP
\fB\-e\fR, \fB\-\-exposure=\fR<time_us>
Exposure time
.TP
\fB\-g\fR, \fB\-\-gain=\fR<dB>
Gain (dB)
.TP
\fB\-a\fR, \fB\-\-auto\fR
Auto socket buffer size
.TP
\fB\-\-features\fR
Additional configuration as a space separated list of features
.TP
\fB\-j\fR, \fB\-\-packet\-size\-adjustment=\fR{never|always|once|on\-failure|on\-failure\-once}
Packet size adjustment
.TP
\fB\-r\fR, \fB\-\-no\-packet\-resend\fR
No packet resend
.TP
\fB\-q\fR, \fB\-\-packet\-request\-ratio\fR=\fI\,[0\/\fR..2.0]
Packet resend request limit as a frame packet ratio
.TP
\fB\-l\fR, \fB\-\-initial\-packet\-timeout=\fR<ms>
Initial packet timeout
.TP
\fB\-p\fR, \fB\-\-packet\-timeout=\fR<ms>
Packet timeout
.TP
\fB\-m\fR, \fB\-\-frame\-retention=\fR<ms>
Frame retention
.TP
\fB\-c\fR, \fB\-\-gv\-stream\-channel=\fR<id>
GigEVision stream channel id
.TP
\fB\-y\fR, \fB\-\-gv\-packet\-delay=\fR<ns>
GigEVision packet delay
.TP
\fB\-i\fR, \fB\-\-gv\-packet\-size=\fR<n_bytes>
GigEVision packet size
.TP
\fB\-s\fR, \fB\-\-usb\-mode=\fR{sync|async}
USB device I/O mode
.TP
\fB\-u\fR, \fB\-\-chunks=\fR<chunk_id>[,<chunk_id>[...]]
Chunks
.TP
\fB\-\-realtime\fR
Make stream thread realtime
.TP
\fB\-\-high\-priority\fR
Make stream thread high priority
.TP
\fB\-\-no\-packet\-socket\fR
Disable use of packet socket
.TP
\fB\-\-multipart\fR
Enable multipart payload
.TP
\fB\-\-register\-cache=\fR{disable|enable|debug}
Register cache policy
.TP
\fB\-\-range\-check=\fR{disable|enable|debug}
Range check policy
.TP
\fB\-\-access\-check=\fR{disable|enable}
Feature access check policy
.TP
\fB\-b\fR, \fB\-\-bandwidth\-limit=\fR<limit>
Desired USB3 Vision device bandwidth limit
.TP
\fB\-\-duration=\fR<s>
Test duration (s)
.TP
\fB\-\-gv\-allow\-broadcast\-discovery\-ack\fR
Allow broadcast discovery ack
.TP
\fB\-d\fR, \fB\-\-debug=\fR{<category>[:<level>][,...]|help}
Debug output selection
.TP
\fB\-v\fR, \fB\-\-version\fR
Show version
.PP
This tool configures a camera and starts video streaming, infinitely unless a duration is given.
