.\" DO NOT MODIFY THIS FILE!  It was generated by help2man 1.49.3.
.TH ARV-TOOL-0.10 "1" "novembre 2023" "arv-tool-0.10 0.9.0" "User Commands"
.SH NAME
arv-tool-0.10 \- manual page for arv-tool-0.10 0.9.0
.SH DESCRIPTION
.SS "Usage:"
.TP
arv\-tool\-0.10 [OPTION?]
command <parameters>
.PP
Small utility for basic control of a Genicam device.
.SS "Help Options:"
.TP
\fB\-h\fR, \fB\-\-help\fR
Show help options
.SS "Application Options:"
.HP
\fB\-n\fR, \fB\-\-name=\fR<pattern>
.HP
\fB\-a\fR, \fB\-\-address=\fR<device_address>
.TP
\fB\-\-register\-cache=\fR{disable|enable|debug}
Register cache policy
.TP
\fB\-\-range\-check=\fR{disable|enable|debug}
Range check policy
.TP
\fB\-\-access\-check=\fR{disable|enable}
Feature access check policy
.TP
\fB\-\-gv\-allow\-broadcast\-discovery\-ack\fR
Allow broadcast discovery ack
.TP
\fB\-t\fR, \fB\-\-time\fR
Show execution time
.HP
\fB\-d\fR, \fB\-\-debug=\fR{<category>[:<level>][,...]|help}
.TP
\fB\-v\fR, \fB\-\-version\fR
Show version
.PP
Command may be one of the following possibilities:
.TP
genicam:
dump the content of the Genicam xml data
.TP
features:
list all features
.TP
values:
list all available feature values
.TP
description [<feature>] ...:
show the full feature description
.TP
control <feature>[=<value>] ...:
read/write device features
.TP
network <setting>[=<value>]...:
read/write network settings
.PP
If no command is given, this utility will list all the available devices.
For the control command, direct access to device registers is provided using a R[address] syntax in place of a feature name.
.SH EXAMPLES
arv\-tool\-0.10 control Width=128 Height=128 Gain R[0x10000]=0x10
arv\-tool\-0.10 features
arv\-tool\-0.10 description Width Height
arv\-tool\-0.10 network mode=PersistentIP
arv\-tool\-0.10 network ip=192.168.0.1 mask=255.255.255.0 gateway=192.168.0.254
arv\-tool\-0.10 \-n Basler\-210ab4 genicam
