.\" DO NOT MODIFY THIS FILE!  It was generated by help2man 1.49.3.
.TH ARV-TEST-0.10 "1" "novembre 2023" "arv-test-0.10 0.9.0" "User Commands"
.SH NAME
arv-test-0.10 \- manual page for arv-test-0.10 0.9.0
.SH DESCRIPTION
.SS "Usage:"
.IP
arv\-test\-0.10 [OPTION?]
.PP
Automated test utillity.
.SS "Help Options:"
.TP
\fB\-h\fR, \fB\-\-help\fR
Show help options
.SS "Application Options:"
.TP
\fB\-n\fR, \fB\-\-name=\fR<pattern>
Device selection
.TP
\fB\-t\fR, \fB\-\-test=\fR<pattern>
Test selection
.TP
\fB\-c\fR, \fB\-\-configuration=\fR<path>
Alternative configuration
.TP
\fB\-i\fR, \fB\-\-iterations=\fR<n_iter>
Number of test repetitions
.TP
\fB\-s\fR, \fB\-\-usb\-mode=\fR{sync|async}
USB device I/O mode
.TP
\fB\-a\fR, \fB\-\-cache\-check\fR
Register cache check
.TP
\fB\-\-packet\-socket\fR
Enable use of packet socket
.HP
\fB\-d\fR, \fB\-\-debug=\fR{<category>[:<level>][,...]|help}
.TP
\fB\-v\fR, \fB\-\-version\fR
Show version
.PP
arv\-test is an automated test utility that tries to exercise most of the
Aravis functionalities. By default it runs all the tests on all the detected
devices, but devices and tests can be selected using a glob pattern.
.PP
A default configuration file is bundled in the executable. An alternative
one with entries specific to the camera you want to test can be specified.
