
Sample virtual server for receiving a CoA or Disconnect-Request packet.


Listen on the CoA port.

This uses the normal set of clients, with the same secret as for
authentication and accounting.





Receive a CoA request

Insert your own policies here.


Send a CoA ACK

Sample module.


Send a CoA NAK

Sample module.


Receive a Disconnect request

Insert your own policies here.


Send a Disconnect ACK

Sample module.


Send a Disconnect NAK

Sample module.

== Default Configuration

```
server coa {
	namespace = radius
	listen {
		type = CoA-Request
		type = Disconnect-Request
		transport = udp
		udp {
			ipaddr = *
			port = 3799
		}
	}
	recv CoA-Request {
		ok
	}
	send CoA-ACK {
		ok
	}
	send CoA-NAK {
		ok
	}
	recv Disconnect-Request {
		ok
	}
	send Disconnect-ACK {
		ok
	}
	send Disconnect-NAK {
		ok
	}
}
```
