REGISTERS
AX, BX, CX, DX - 16bit registers
SP - 16bit stack pointer, not accessible explicitly
PC - 16bit program counter
BP - 16bit base pointer

FLAGS
CF - carry flag
ZF - zero flag
OF - overflow flag