<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.1" unitdist="inch" unit="inch" style="lines" multiple="1" display="no" altdistance="0.01" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="no" active="no"/>
<layer number="2" name="Route2" color="1" fill="3" visible="no" active="no"/>
<layer number="3" name="Route3" color="4" fill="3" visible="no" active="no"/>
<layer number="4" name="Route4" color="1" fill="4" visible="no" active="no"/>
<layer number="5" name="Route5" color="4" fill="4" visible="no" active="no"/>
<layer number="6" name="Route6" color="1" fill="8" visible="no" active="no"/>
<layer number="7" name="Route7" color="4" fill="8" visible="no" active="no"/>
<layer number="8" name="Route8" color="1" fill="2" visible="no" active="no"/>
<layer number="9" name="Route9" color="4" fill="2" visible="no" active="no"/>
<layer number="10" name="Route10" color="1" fill="7" visible="no" active="no"/>
<layer number="11" name="Route11" color="4" fill="7" visible="no" active="no"/>
<layer number="12" name="Route12" color="1" fill="5" visible="no" active="no"/>
<layer number="13" name="Route13" color="4" fill="5" visible="no" active="no"/>
<layer number="14" name="Route14" color="1" fill="6" visible="no" active="no"/>
<layer number="15" name="Route15" color="4" fill="6" visible="no" active="no"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="no" active="no"/>
<layer number="17" name="Pads" color="2" fill="1" visible="no" active="no"/>
<layer number="18" name="Vias" color="2" fill="1" visible="no" active="no"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="no" active="no"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="no" active="no"/>
<layer number="21" name="tPlace" color="16" fill="1" visible="no" active="no"/>
<layer number="22" name="bPlace" color="14" fill="1" visible="no" active="no"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="no" active="no"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="no" active="no"/>
<layer number="25" name="tNames" color="7" fill="1" visible="no" active="no"/>
<layer number="26" name="bNames" color="7" fill="1" visible="no" active="no"/>
<layer number="27" name="tValues" color="7" fill="1" visible="no" active="no"/>
<layer number="28" name="bValues" color="7" fill="1" visible="no" active="no"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="no"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="no"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="no"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="no"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="no"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="no"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="no"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="no"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="no"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="no"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="no" active="no"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="no" active="no"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="no" active="no"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="no" active="no"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="no" active="no"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="no"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="no"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="no"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="no"/>
<layer number="48" name="Document" color="7" fill="1" visible="no" active="no"/>
<layer number="49" name="Reference" color="7" fill="1" visible="no" active="no"/>
<layer number="50" name="dxf" color="7" fill="1" visible="no" active="no"/>
<layer number="51" name="tDocu" color="6" fill="1" visible="no" active="no"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="no" active="no"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="no" active="no"/>
<layer number="57" name="tCAD" color="7" fill="1" visible="no" active="no"/>
<layer number="59" name="tCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="60" name="bCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="88" name="SimResults" color="9" fill="1" visible="yes" active="yes"/>
<layer number="89" name="SimProbes" color="9" fill="1" visible="yes" active="yes"/>
<layer number="90" name="Modules" color="5" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="no" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
<layer number="99" name="SpiceOrder" color="7" fill="1" visible="yes" active="yes"/>
<layer number="100" name="Muster" color="7" fill="1" visible="no" active="no"/>
<layer number="101" name="Patch_Top" color="12" fill="4" visible="no" active="no"/>
<layer number="102" name="Vscore" color="7" fill="1" visible="no" active="no"/>
<layer number="103" name="tMap" color="7" fill="1" visible="no" active="no"/>
<layer number="104" name="Name" color="16" fill="1" visible="no" active="no"/>
<layer number="105" name="tPlate" color="7" fill="1" visible="no" active="no"/>
<layer number="106" name="bPlate" color="7" fill="1" visible="no" active="no"/>
<layer number="107" name="Crop" color="7" fill="1" visible="no" active="no"/>
<layer number="108" name="tplace-old" color="10" fill="1" visible="no" active="no"/>
<layer number="109" name="ref-old" color="11" fill="1" visible="no" active="no"/>
<layer number="110" name="fp0" color="7" fill="1" visible="no" active="no"/>
<layer number="111" name="LPC17xx" color="7" fill="1" visible="no" active="no"/>
<layer number="112" name="tSilk" color="7" fill="1" visible="no" active="no"/>
<layer number="113" name="IDFDebug" color="4" fill="1" visible="no" active="no"/>
<layer number="114" name="Badge_Outline" color="7" fill="1" visible="no" active="no"/>
<layer number="115" name="ReferenceISLANDS" color="7" fill="1" visible="no" active="no"/>
<layer number="116" name="Patch_BOT" color="9" fill="4" visible="no" active="no"/>
<layer number="117" name="PM_Ref" color="7" fill="1" visible="yes" active="yes"/>
<layer number="118" name="Rect_Pads" color="7" fill="1" visible="no" active="no"/>
<layer number="119" name="PF_Ref" color="7" fill="1" visible="yes" active="yes"/>
<layer number="120" name="WFL_Ref" color="7" fill="1" visible="yes" active="yes"/>
<layer number="121" name="_tsilk" color="7" fill="1" visible="no" active="no"/>
<layer number="122" name="_bsilk" color="7" fill="1" visible="no" active="no"/>
<layer number="123" name="tTestmark" color="7" fill="1" visible="no" active="no"/>
<layer number="124" name="bTestmark" color="7" fill="1" visible="no" active="no"/>
<layer number="125" name="_tNames" color="7" fill="1" visible="no" active="no"/>
<layer number="126" name="_bNames" color="7" fill="1" visible="no" active="no"/>
<layer number="127" name="_tValues" color="7" fill="1" visible="no" active="no"/>
<layer number="128" name="_bValues" color="7" fill="1" visible="no" active="no"/>
<layer number="129" name="Mask" color="7" fill="1" visible="no" active="no"/>
<layer number="131" name="tAdjust" color="7" fill="1" visible="no" active="no"/>
<layer number="132" name="bAdjust" color="7" fill="1" visible="no" active="no"/>
<layer number="144" name="Drill_legend" color="7" fill="1" visible="no" active="no"/>
<layer number="150" name="Notes" color="7" fill="1" visible="no" active="no"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="no" active="no"/>
<layer number="152" name="_bDocu" color="7" fill="1" visible="no" active="no"/>
<layer number="153" name="FabDoc1" color="7" fill="1" visible="no" active="no"/>
<layer number="154" name="FabDoc2" color="7" fill="1" visible="no" active="no"/>
<layer number="155" name="FabDoc3" color="7" fill="1" visible="no" active="no"/>
<layer number="199" name="Contour" color="7" fill="1" visible="no" active="no"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="no" active="no"/>
<layer number="201" name="201bmp" color="2" fill="10" visible="no" active="no"/>
<layer number="202" name="202bmp" color="3" fill="10" visible="no" active="no"/>
<layer number="203" name="203bmp" color="4" fill="10" visible="no" active="no"/>
<layer number="204" name="204bmp" color="5" fill="10" visible="no" active="no"/>
<layer number="205" name="205bmp" color="6" fill="10" visible="no" active="no"/>
<layer number="206" name="206bmp" color="7" fill="10" visible="no" active="no"/>
<layer number="207" name="207bmp" color="8" fill="10" visible="no" active="no"/>
<layer number="208" name="208bmp" color="9" fill="10" visible="no" active="no"/>
<layer number="209" name="209bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="210" name="210bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="211" name="211bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="212" name="212bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="213" name="213bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="214" name="214bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="215" name="215bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="216" name="216bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="217" name="217bmp" color="18" fill="1" visible="no" active="no"/>
<layer number="218" name="218bmp" color="19" fill="1" visible="no" active="no"/>
<layer number="219" name="219bmp" color="20" fill="1" visible="no" active="no"/>
<layer number="220" name="220bmp" color="21" fill="1" visible="no" active="no"/>
<layer number="221" name="221bmp" color="22" fill="1" visible="no" active="no"/>
<layer number="222" name="222bmp" color="23" fill="1" visible="no" active="no"/>
<layer number="223" name="223bmp" color="24" fill="1" visible="no" active="no"/>
<layer number="224" name="224bmp" color="25" fill="1" visible="no" active="no"/>
<layer number="225" name="225bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="226" name="226bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="227" name="227bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="228" name="228bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="229" name="229bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="230" name="230bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="231" name="231bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="232" name="Eagle3D_PG2" color="7" fill="1" visible="no" active="no"/>
<layer number="233" name="Eagle3D_PG3" color="7" fill="1" visible="no" active="no"/>
<layer number="248" name="Housing" color="7" fill="1" visible="no" active="no"/>
<layer number="249" name="Edge" color="7" fill="1" visible="no" active="no"/>
<layer number="250" name="Descript" color="3" fill="1" visible="no" active="no"/>
<layer number="251" name="SMDround" color="12" fill="11" visible="no" active="no"/>
<layer number="254" name="cooling" color="7" fill="1" visible="no" active="no"/>
<layer number="255" name="routoute" color="7" fill="1" visible="no" active="no"/>
</layers>
<schematic xreflabel="%F%N/%S.%C%R" xrefpart="/%S.%C%R">
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X2">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="3.81" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="3.81" y1="-2.54" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<wire x1="2.54" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="2.54" y2="-1.27" width="0.127" layer="21"/>
<wire x1="2.54" y1="-1.27" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<text x="-1.27" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20" align="top-left">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.75" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.75" y1="3.15" x2="5.75" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.75" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4" y1="-1" x2="-4" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="-4" y1="-4.5" x2="-3.2" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="-3.2" y1="-4.5" x2="-3.2" y2="-2" width="0.2032" layer="21"/>
<wire x1="-3.2" y1="-2" x2="-2" y2="-2" width="0.2032" layer="21"/>
<wire x1="2" y1="-2" x2="3.2" y2="-2" width="0.2032" layer="21"/>
<wire x1="3.2" y1="-2" x2="3.2" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="3.2" y1="-4.5" x2="4" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="4" y1="-4.5" x2="4" y2="-1" width="0.2032" layer="21"/>
<wire x1="2" y1="3" x2="-2" y2="3" width="0.2032" layer="21"/>
<smd name="1" x="-1" y="-3.7" dx="1" dy="4.6" layer="1"/>
<smd name="2" x="1" y="-3.7" dx="1" dy="4.6" layer="1"/>
<smd name="NC1" x="-3.4" y="1.5" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<smd name="NC2" x="3.4" y="1.5" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<text x="-1.397" y="1.778" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="0.635" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_BIG">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.15"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="1.27" x2="-1.27" y2="-1.27" width="0.127" layer="21"/>
<wire x1="-1.27" y1="-1.27" x2="5.08" y2="-1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="-1.27" x2="5.08" y2="1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="1.27" x2="-1.27" y2="1.27" width="0.127" layer="21"/>
<pad name="P$1" x="0" y="0" drill="1.0668"/>
<pad name="P$2" x="3.81" y="0" drill="1.0668"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-SMD-VERT">
<description>&lt;h3&gt;JST-Vertical Male Header SMT &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.1" y1="2.97" x2="4.2" y2="2.97" width="0.2032" layer="51"/>
<wire x1="4.2" y1="2.97" x2="4.2" y2="-2.13" width="0.2032" layer="51"/>
<wire x1="4.2" y1="-2.13" x2="-4.1" y2="-2.13" width="0.2032" layer="51"/>
<wire x1="-4.1" y1="-2.13" x2="-4.1" y2="2.97" width="0.2032" layer="51"/>
<wire x1="-4.1" y1="3" x2="4.2" y2="3" width="0.2032" layer="21"/>
<wire x1="4.2" y1="3" x2="4.2" y2="2.3" width="0.2032" layer="21"/>
<wire x1="-4.1" y1="3" x2="-4.1" y2="2.3" width="0.2032" layer="21"/>
<wire x1="2" y1="-2.1" x2="4.2" y2="-2.1" width="0.2032" layer="21"/>
<wire x1="4.2" y1="-2.1" x2="4.2" y2="-1.7" width="0.2032" layer="21"/>
<wire x1="-2" y1="-2.1" x2="-4.1" y2="-2.1" width="0.2032" layer="21"/>
<wire x1="-4.1" y1="-2.1" x2="-4.1" y2="-1.8" width="0.2032" layer="21"/>
<smd name="P$1" x="-3.4" y="0.27" dx="3" dy="1.6" layer="1" rot="R90"/>
<smd name="P$2" x="3.4" y="0.27" dx="3" dy="1.6" layer="1" rot="R90"/>
<smd name="VCC" x="-1" y="-2" dx="1" dy="5.5" layer="1"/>
<smd name="GND" x="1" y="-2" dx="1" dy="5.5" layer="1"/>
<text x="-3.81" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-3.81" y="2.21" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
</package>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.1" y1="4.2" x2="8.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="8.1" y1="4.2" x2="8.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-2.3" x2="8.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-3.3" x2="-3.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-3.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-2.3" x2="-3.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-2.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-1.35" x2="-3.7" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-1.35" x2="-3.7" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-2.35" x2="-3.1" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="8.1" y1="4" x2="8.7" y2="4" width="0.2032" layer="51"/>
<wire x1="8.7" y1="4" x2="8.7" y2="3" width="0.2032" layer="51"/>
<wire x1="8.7" y1="3" x2="8.1" y2="3" width="0.2032" layer="51"/>
<circle x="2.5" y="3.7" radius="0.2828" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="1.3" diameter="2.032" shape="square"/>
<pad name="2" x="5" y="0" drill="1.3" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="-0.1778" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.7178" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X2_LOCK">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset from center by 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="3.81" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="3.81" y1="-2.54" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<wire x1="2.54" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="2.54" y2="-1.27" width="0.127" layer="21"/>
<wire x1="2.54" y1="-1.27" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="-0.127" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.667" y="0" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20" align="top-left">&gt;VALUE</text>
</package>
<package name="1X02_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.651" y1="0" x2="0.889" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.016" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.9906" x2="-0.9906" y2="1.27" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.9906" x2="-0.9906" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.556" y2="0" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.9906" x2="3.5306" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.9906" x2="3.5306" y2="1.27" width="0.2032" layer="21"/>
<pad name="1" x="-0.127" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.667" y="0" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="1.651" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH Locking&lt;/h3&gt;
Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.15" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-1.35" x2="-2.15" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.65" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.15" x2="5.65" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<circle x="0" y="0" radius="0.4318" width="0.0254" layer="51"/>
<circle x="3.5" y="0" radius="0.4318" width="0.0254" layer="51"/>
<pad name="1" x="-0.1778" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.6778" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.397" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-PTH">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.6"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="2.73" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
<wire x1="-2.95" y1="-1.6" x2="-2.95" y2="6" width="0.2032" layer="21"/>
<wire x1="-2.95" y1="6" x2="2.95" y2="6" width="0.2032" layer="21"/>
<wire x1="2.95" y1="6" x2="2.95" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-2.95" y1="-1.6" x2="-2.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="2.95" y1="-1.6" x2="2.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-2.3" y1="-1.6" x2="-2.3" y2="0" width="0.2032" layer="21"/>
<wire x1="2.3" y1="-1.6" x2="2.3" y2="0" width="0.2032" layer="21"/>
</package>
<package name="1X02_XTRA_BIG">
<description>&lt;h3&gt;Plated Through Hole - 0.1" holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.2"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-5.08" y1="2.54" x2="-5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-5.08" y1="-2.54" x2="5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="-2.54" x2="5.08" y2="2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="2.54" x2="-5.08" y2="2.54" width="0.127" layer="21"/>
<pad name="1" x="-2.54" y="0" drill="2.0574" diameter="3.556"/>
<pad name="2" x="2.54" y="0" drill="2.0574" diameter="3.556"/>
<text x="-5.08" y="2.667" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-5.08" y="-3.302" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_PP_HOLES_ONLY">
<description>&lt;h3&gt;Pogo Pins Connector - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="0" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.635" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<hole x="0" y="0" drill="1.4732"/>
<hole x="2.54" y="0" drill="1.4732"/>
<text x="-1.27" y="1.143" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-1.778" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-1.35" x2="-2.15" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-1.35" x2="-2.15" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.65" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.15" x2="5.65" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-PTH-NS">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole- No Silk&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; No silk outline of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2" y1="0" x2="-2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-2" y1="-1.8" x2="-3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-3" y1="-1.8" x2="-3" y2="6" width="0.2032" layer="51"/>
<wire x1="-3" y1="6" x2="3" y2="6" width="0.2032" layer="51"/>
<wire x1="3" y1="6" x2="3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="3" y1="-1.8" x2="2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="2" y1="-1.8" x2="2" y2="0" width="0.2032" layer="51"/>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.6"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="4" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
</package>
<package name="JST-2-PTH-KIT">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole - KIT&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad.
&lt;br&gt; This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2" y1="0" x2="-2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-2" y1="-1.8" x2="-3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-3" y1="-1.8" x2="-3" y2="6" width="0.2032" layer="51"/>
<wire x1="-3" y1="6" x2="3" y2="6" width="0.2032" layer="51"/>
<wire x1="3" y1="6" x2="3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="3" y1="-1.8" x2="2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="2" y1="-1.8" x2="2" y2="0" width="0.2032" layer="51"/>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.4478" stop="no"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.4478" stop="no"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="4" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
<polygon width="0.127" layer="30">
<vertex x="-0.9975" y="-0.6604" curve="-90.025935"/>
<vertex x="-1.6604" y="0" curve="-90.017354"/>
<vertex x="-1" y="0.6604" curve="-90"/>
<vertex x="-0.3396" y="0" curve="-90.078137"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-1" y="-0.2865" curve="-90.08005"/>
<vertex x="-1.2865" y="0" curve="-90.040011"/>
<vertex x="-1" y="0.2865" curve="-90"/>
<vertex x="-0.7135" y="0" curve="-90"/>
</polygon>
<polygon width="0.127" layer="30">
<vertex x="1.0025" y="-0.6604" curve="-90.025935"/>
<vertex x="0.3396" y="0" curve="-90.017354"/>
<vertex x="1" y="0.6604" curve="-90"/>
<vertex x="1.6604" y="0" curve="-90.078137"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="1" y="-0.2865" curve="-90.08005"/>
<vertex x="0.7135" y="0" curve="-90.040011"/>
<vertex x="1" y="0.2865" curve="-90"/>
<vertex x="1.2865" y="0" curve="-90"/>
</polygon>
</package>
<package name="SPRINGTERMINAL-2.54MM-2">
<description>&lt;h3&gt;Spring Terminal- PCB Mount 2 Pin PTH&lt;/h3&gt;
tDocu marks the spring arms
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/SpringTerminal.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.2" y1="7.88" x2="-4.2" y2="-2.8" width="0.254" layer="21"/>
<wire x1="-4.2" y1="-2.8" x2="-4.2" y2="-4.72" width="0.254" layer="51"/>
<wire x1="-4.2" y1="-4.72" x2="3.44" y2="-4.72" width="0.254" layer="51"/>
<wire x1="3.44" y1="-4.72" x2="3.44" y2="-2.8" width="0.254" layer="51"/>
<wire x1="3.44" y1="7.88" x2="-4.2" y2="7.88" width="0.254" layer="21"/>
<wire x1="0" y1="0" x2="0" y2="5.08" width="0.254" layer="1"/>
<wire x1="0" y1="0" x2="0" y2="5.08" width="0.254" layer="16"/>
<wire x1="2.54" y1="0" x2="2.54" y2="5.08" width="0.254" layer="16"/>
<wire x1="2.54" y1="0" x2="2.54" y2="5.08" width="0.254" layer="1"/>
<wire x1="-4.2" y1="-2.8" x2="3.44" y2="-2.8" width="0.254" layer="21"/>
<wire x1="3.44" y1="4" x2="3.44" y2="1" width="0.254" layer="21"/>
<wire x1="3.44" y1="7.88" x2="3.44" y2="6" width="0.254" layer="21"/>
<wire x1="3.44" y1="-0.9" x2="3.44" y2="-2.8" width="0.254" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1" diameter="1.9"/>
<pad name="P$2" x="0" y="5.08" drill="1.1" diameter="1.9"/>
<pad name="P$3" x="2.54" y="5.08" drill="1.1" diameter="1.9"/>
<pad name="2" x="2.54" y="0" drill="1.1" diameter="1.9"/>
</package>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="P2" x="0" y="0" drill="1.016" shape="square"/>
<pad name="P1" x="2.54" y="0" drill="1.016" shape="square"/>
<wire x1="-1.5" y1="3.25" x2="4" y2="3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="3.25" x2="4" y2="2.5" width="0.2032" layer="21"/>
<wire x1="4" y1="2.5" x2="4" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="-3.25" x2="-1.5" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="-3.25" x2="-1.5" y2="2.5" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="-1.5" y2="3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="4" y2="2.5" width="0.2032" layer="21"/>
<text x="-1.27" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-4.064" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_POKEHOME">
<description>2 pin poke-home connector

part number 2062-2P from STA</description>
<wire x1="-7" y1="-4" x2="-7" y2="2" width="0.2032" layer="21"/>
<wire x1="-7" y1="2" x2="-7" y2="4" width="0.2032" layer="21"/>
<wire x1="4.7" y1="4" x2="4.7" y2="-4" width="0.2032" layer="21"/>
<wire x1="4.7" y1="-4" x2="-7" y2="-4" width="0.2032" layer="21"/>
<smd name="P2" x="5.25" y="-2" dx="3.5" dy="2" layer="1"/>
<smd name="P1" x="5.25" y="2" dx="3.5" dy="2" layer="1"/>
<smd name="P4" x="-4" y="-2" dx="6" dy="2" layer="1"/>
<smd name="P3" x="-4" y="2" dx="6" dy="2" layer="1"/>
<wire x1="-7" y1="4" x2="4.7" y2="4" width="0.2032" layer="21"/>
<text x="0.635" y="-3.175" size="0.4064" layer="25">&gt;NAME</text>
<text x="0.635" y="-1.905" size="0.4064" layer="27">&gt;VALUE</text>
<text x="-7.239" y="-1.397" size="0.3048" layer="51" rot="R90">BOARD EDGE</text>
</package>
<package name="1X02_RA_PTH_FEMALE">
<wire x1="-2.79" y1="4.25" x2="-2.79" y2="-4.25" width="0.1778" layer="21"/>
<text x="-1.397" y="0.762" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.524" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<wire x1="2.79" y1="4.25" x2="2.79" y2="-4.25" width="0.1778" layer="21"/>
<wire x1="-2.79" y1="4.25" x2="2.79" y2="4.25" width="0.1778" layer="21"/>
<wire x1="-2.79" y1="-4.25" x2="2.79" y2="-4.25" width="0.1778" layer="21"/>
<pad name="2" x="-1.27" y="-5.85" drill="0.8"/>
<pad name="1" x="1.27" y="-5.85" drill="0.8"/>
</package>
</packages>
<symbols>
<symbol name="CONN_02">
<description>&lt;h3&gt;2 Pin Connection&lt;/h3&gt;</description>
<wire x1="3.81" y1="-2.54" x2="-2.54" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="1.27" y1="2.54" x2="2.54" y2="2.54" width="0.6096" layer="94"/>
<wire x1="1.27" y1="0" x2="2.54" y2="0" width="0.6096" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="-2.54" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="3.81" y1="-2.54" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<text x="-2.54" y="-4.826" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-2.54" y="5.588" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CONN_02" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;

 Molex polarized connector foot print use with: PRT-08233 with associated crimp pins and housings.&lt;br&gt;&lt;br&gt;

2.54_SCREWTERM for use with  PRT-10571.&lt;br&gt;&lt;br&gt;

3.5mm Screw Terminal footprints for  PRT-08084&lt;br&gt;&lt;br&gt;

5mm Screw Terminal footprints for use with PRT-08432</description>
<gates>
<gate name="G$1" symbol="CONN_02" x="-2.54" y="0"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918" constant="no"/>
</technology>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="PRT-08432" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09863" constant="no"/>
<attribute name="SKU" value="PRT-09914" constant="no"/>
</technology>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.54MM_SCREWTERM" package="1X02_2.54_SCREWTERM">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_POKEHOME" package="1X02_POKEHOME">
<connects>
<connect gate="G$1" pin="1" pad="P1 P3"/>
<connect gate="G$1" pin="2" pad="P2 P4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13512"/>
</technology>
</technologies>
</device>
<device name="PTH_RA_FEMALE" package="1X02_RA_PTH_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13700"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="diy-modules">
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.8.0 (2017-Jul-02)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;
&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://www.diymodules.org/img/diymodules-lbr-image.php?v=1.8.0" alt="DIYmodules.org"&gt;&lt;/a&gt;
&lt;/center&gt;</description>
<packages>
<package name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<wire x1="-21.59" y1="10.414" x2="21.59" y2="10.414" width="0.127" layer="21"/>
<wire x1="21.59" y1="10.414" x2="21.59" y2="-10.414" width="0.127" layer="21"/>
<wire x1="21.59" y1="-10.414" x2="-21.59" y2="-10.414" width="0.127" layer="21"/>
<wire x1="-21.59" y1="-10.414" x2="-21.59" y2="10.414" width="0.127" layer="21"/>
<pad name="IN+" x="-19.812" y="8.636" drill="1.5" diameter="2.5" shape="square"/>
<pad name="IN-" x="-19.812" y="-8.636" drill="1.5" diameter="2.5" shape="square"/>
<pad name="OUT-" x="19.812" y="-8.636" drill="1.5" diameter="2.5" shape="square"/>
<pad name="OUT+" x="19.812" y="8.636" drill="1.5" diameter="2.5" shape="square"/>
<hole x="-14.478" y="7.62" drill="3"/>
<hole x="15.24" y="-7.62" drill="3"/>
<text x="0" y="11.43" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-11.43" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<text x="-19.685" y="0" size="1.778" layer="21" rot="R90" align="center">IN</text>
<text x="19.685" y="0" size="1.778" layer="21" rot="R90" align="center">OUT</text>
<wire x1="19.685" y1="6.985" x2="19.685" y2="5.715" width="0.254" layer="21"/>
<wire x1="19.05" y1="6.35" x2="20.32" y2="6.35" width="0.254" layer="21"/>
<wire x1="-19.685" y1="-6.985" x2="-19.685" y2="-5.715" width="0.254" layer="21"/>
<wire x1="19.685" y1="-6.985" x2="19.685" y2="-5.715" width="0.254" layer="21"/>
<wire x1="-19.685" y1="6.985" x2="-19.685" y2="5.715" width="0.254" layer="21"/>
<wire x1="-20.32" y1="6.35" x2="-19.05" y2="6.35" width="0.254" layer="21"/>
</package>
<package name="BATTERY-CHARGER-LI-PROT">
<description>&lt;b&gt;Protected Lithium Battery 5V Charger&lt;/b&gt; with micro-USB connector</description>
<wire x1="-13.97" y1="8.636" x2="13.97" y2="8.636" width="0.127" layer="21"/>
<wire x1="13.97" y1="-8.636" x2="-13.97" y2="-8.636" width="0.127" layer="21"/>
<pad name="IN+" x="-12.065" y="6.985" drill="1.2" diameter="2.5" shape="square"/>
<pad name="IN-" x="-12.065" y="-6.985" drill="1.2" diameter="2.5" shape="square"/>
<pad name="B+" x="10.795" y="3.81" drill="1.2" diameter="2.5" shape="square"/>
<pad name="B-" x="10.795" y="-3.81" drill="1.2" diameter="2.5" shape="square"/>
<text x="-9.525" y="6.985" size="1.27" layer="21" align="center-left">IN+</text>
<text x="-9.525" y="-6.985" size="1.27" layer="21" align="center-left">IN-</text>
<text x="8.255" y="3.81" size="1.27" layer="21" align="center-right">B+</text>
<text x="8.255" y="-3.81" size="1.27" layer="21" align="center-right">B-</text>
<wire x1="-13.97" y1="8.636" x2="-13.97" y2="4.064" width="0.127" layer="21"/>
<wire x1="-13.97" y1="-8.636" x2="-13.97" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-14.605" y1="4.064" x2="-13.97" y2="4.064" width="0.127" layer="21"/>
<wire x1="-14.605" y1="-4.064" x2="-13.97" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-13.97" y1="-4.064" x2="-8.128" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-14.605" y1="4.064" x2="-14.605" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-8.128" y1="4.064" x2="-8.128" y2="-4.064" width="0.127" layer="21"/>
<text x="-11.43" y="0" size="1.778" layer="21" align="center">USB</text>
<text x="0" y="10.16" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-10.16" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<wire x1="13.97" y1="8.636" x2="13.97" y2="6.35" width="0.127" layer="21"/>
<wire x1="13.97" y1="6.35" x2="12.7" y2="6.35" width="0.127" layer="21"/>
<wire x1="12.7" y1="6.35" x2="12.7" y2="-6.35" width="0.127" layer="21"/>
<wire x1="12.7" y1="-6.35" x2="13.97" y2="-6.35" width="0.127" layer="21"/>
<wire x1="13.97" y1="-6.35" x2="13.97" y2="-8.636" width="0.127" layer="21"/>
<pad name="OUT+" x="10.795" y="6.985" drill="1.2" diameter="2.5" shape="square"/>
<pad name="OUT-" x="10.795" y="-6.985" drill="1.2" diameter="2.5" shape="square"/>
<wire x1="-13.97" y1="4.064" x2="-8.128" y2="4.064" width="0.127" layer="21"/>
<text x="8.255" y="6.985" size="1.27" layer="21" align="center-right">OUT+</text>
<text x="8.255" y="-6.985" size="1.27" layer="21" align="center-right">OUT-</text>
</package>
<package name="WIRELESS-LORA-RFM95W#THT">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt;&lt;br /&gt;
Footprint for THT assembly.</description>
<wire x1="-8" y1="8" x2="8" y2="8" width="0.127" layer="21"/>
<wire x1="8" y1="-8" x2="-8" y2="-8" width="0.127" layer="21"/>
<pad name="A1" x="-6.5" y="7" drill="0.8"/>
<text x="0" y="9.525" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-9.525" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<text x="-5" y="7" size="1.016" layer="21" align="center-left">GND</text>
<wire x1="-8" y1="8" x2="-8" y2="-8" width="0.127" layer="21"/>
<wire x1="8" y1="-8" x2="8" y2="8" width="0.127" layer="21"/>
<pad name="A2" x="-6.5" y="5" drill="0.8"/>
<pad name="A3" x="-6.5" y="3" drill="0.8"/>
<pad name="A4" x="-6.5" y="1" drill="0.8"/>
<pad name="A5" x="-6.5" y="-1" drill="0.8"/>
<pad name="A6" x="-6.5" y="-3" drill="0.8"/>
<pad name="A7" x="-6.5" y="-5" drill="0.8"/>
<pad name="A8" x="-6.5" y="-7" drill="0.8"/>
<text x="-5" y="5" size="1.016" layer="21" align="center-left">MISO</text>
<text x="-5" y="3" size="1.016" layer="21" align="center-left">MOSI</text>
<text x="-5" y="1" size="1.016" layer="21" align="center-left">SCK</text>
<text x="-5" y="-1" size="1.016" layer="21" align="center-left">NSS</text>
<text x="-5" y="-3" size="1.016" layer="21" align="center-left">RST</text>
<text x="-5" y="-5" size="1.016" layer="21" align="center-left">DIO5</text>
<text x="-5" y="-7" size="1.016" layer="21" align="center-left">GND</text>
<pad name="B1" x="6.5" y="7" drill="0.8"/>
<pad name="B2" x="6.5" y="5" drill="0.8"/>
<pad name="B3" x="6.5" y="3" drill="0.8"/>
<pad name="B4" x="6.5" y="1" drill="0.8"/>
<pad name="B5" x="6.5" y="-1" drill="0.8"/>
<pad name="B6" x="6.5" y="-3" drill="0.8"/>
<pad name="B7" x="6.5" y="-5" drill="0.8"/>
<pad name="B8" x="6.5" y="-7" drill="0.8"/>
<text x="5" y="7" size="1.016" layer="21" align="center-right">DIO2</text>
<text x="5" y="5" size="1.016" layer="21" align="center-right">DIO1</text>
<text x="5" y="3" size="1.016" layer="21" align="center-right">DIO0</text>
<text x="5" y="1" size="1.016" layer="21" align="center-right">3.3V</text>
<text x="5" y="-1" size="1.016" layer="21" align="center-right">DIO4</text>
<text x="5" y="-3" size="1.016" layer="21" align="center-right">DIO3</text>
<text x="5" y="-5" size="1.016" layer="21" align="center-right">GND</text>
<text x="5" y="-7" size="1.016" layer="21" align="center-right">ANT</text>
</package>
<package name="WIRELESS-LORA-RFM95W#SMD">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt;&lt;br /&gt;
Footprint for SMD assembly.</description>
<wire x1="-8" y1="8" x2="8" y2="8" width="0.127" layer="21"/>
<wire x1="8" y1="-8" x2="-8" y2="-8" width="0.127" layer="21"/>
<text x="0" y="9.525" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-9.525" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<text x="-5" y="7" size="1.016" layer="21" align="center-left">GND</text>
<text x="-5" y="5" size="1.016" layer="21" align="center-left">MISO</text>
<text x="-5" y="3" size="1.016" layer="21" align="center-left">MOSI</text>
<text x="-5" y="1" size="1.016" layer="21" align="center-left">SCK</text>
<text x="-5" y="-1" size="1.016" layer="21" align="center-left">NSS</text>
<text x="-5" y="-3" size="1.016" layer="21" align="center-left">RST</text>
<text x="-5" y="-5" size="1.016" layer="21" align="center-left">DIO5</text>
<text x="-5" y="-7" size="1.016" layer="21" align="center-left">GND</text>
<text x="5" y="7" size="1.016" layer="21" align="center-right">DIO2</text>
<text x="5" y="5" size="1.016" layer="21" align="center-right">DIO1</text>
<text x="5" y="3" size="1.016" layer="21" align="center-right">DIO0</text>
<text x="5" y="1" size="1.016" layer="21" align="center-right">3.3V</text>
<text x="5" y="-1" size="1.016" layer="21" align="center-right">DIO4</text>
<text x="5" y="-3" size="1.016" layer="21" align="center-right">DIO3</text>
<text x="5" y="-5" size="1.016" layer="21" align="center-right">GND</text>
<text x="5" y="-7" size="1.016" layer="21" align="center-right">ANT</text>
<smd name="A1" x="-7.5" y="7" dx="3.6" dy="1.2" layer="1"/>
<smd name="A2" x="-7.5" y="5" dx="3.6" dy="1.2" layer="1"/>
<smd name="B1" x="7.5" y="7" dx="3.6" dy="1.2" layer="1"/>
<smd name="A3" x="-7.5" y="3" dx="3.6" dy="1.2" layer="1"/>
<smd name="A4" x="-7.5" y="1" dx="3.6" dy="1.2" layer="1"/>
<smd name="A5" x="-7.5" y="-1" dx="3.6" dy="1.2" layer="1"/>
<smd name="A6" x="-7.5" y="-3" dx="3.6" dy="1.2" layer="1"/>
<smd name="A7" x="-7.5" y="-5" dx="3.6" dy="1.2" layer="1"/>
<smd name="A8" x="-7.5" y="-7" dx="3.6" dy="1.2" layer="1"/>
<smd name="B2" x="7.5" y="5" dx="3.6" dy="1.2" layer="1"/>
<smd name="B3" x="7.5" y="3" dx="3.6" dy="1.2" layer="1"/>
<smd name="B4" x="7.5" y="1" dx="3.6" dy="1.2" layer="1"/>
<smd name="B5" x="7.5" y="-1" dx="3.6" dy="1.2" layer="1"/>
<smd name="B6" x="7.5" y="-3" dx="3.6" dy="1.2" layer="1"/>
<smd name="B7" x="7.5" y="-5" dx="3.6" dy="1.2" layer="1"/>
<smd name="B8" x="7.5" y="-7" dx="3.6" dy="1.2" layer="1"/>
<wire x1="-8" y1="6.2" x2="-8" y2="5.8" width="0.127" layer="21"/>
<wire x1="-8" y1="4.2" x2="-8" y2="3.8" width="0.127" layer="21"/>
<wire x1="-8" y1="2.2" x2="-8" y2="1.8" width="0.127" layer="21"/>
<wire x1="-8" y1="0.2" x2="-8" y2="-0.2" width="0.127" layer="21"/>
<wire x1="-8" y1="-1.8" x2="-8" y2="-2.2" width="0.127" layer="21"/>
<wire x1="-8" y1="-3.8" x2="-8" y2="-4.2" width="0.127" layer="21"/>
<wire x1="-8" y1="-5.8" x2="-8" y2="-6.2" width="0.127" layer="21"/>
<wire x1="-8" y1="8" x2="-8" y2="7.8" width="0.127" layer="21"/>
<wire x1="-8" y1="-8" x2="-8" y2="-7.8" width="0.127" layer="21"/>
<wire x1="8" y1="6.2" x2="8" y2="5.8" width="0.127" layer="21"/>
<wire x1="8" y1="4.2" x2="8" y2="3.8" width="0.127" layer="21"/>
<wire x1="8" y1="2.2" x2="8" y2="1.8" width="0.127" layer="21"/>
<wire x1="8" y1="0.2" x2="8" y2="-0.2" width="0.127" layer="21"/>
<wire x1="8" y1="-1.8" x2="8" y2="-2.2" width="0.127" layer="21"/>
<wire x1="8" y1="-3.8" x2="8" y2="-4.2" width="0.127" layer="21"/>
<wire x1="8" y1="-5.8" x2="8" y2="-6.2" width="0.127" layer="21"/>
<wire x1="8" y1="8" x2="8" y2="7.8" width="0.127" layer="21"/>
<wire x1="8" y1="-8" x2="8" y2="-7.8" width="0.127" layer="21"/>
</package>
<package name="TEMP-HUM-SENSOR-HTU21D">
<description>&lt;b&gt;Digital Humidity &amp; Temperature Sensor&lt;/b&gt; based on &lt;b&gt;HTU21D&lt;/b&gt; device</description>
<wire x1="-5.715" y1="5.08" x2="-4.445" y2="5.08" width="0.127" layer="21"/>
<text x="0" y="6.35" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-6.35" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<pad name="1" x="-5.08" y="3.81" drill="1" shape="square"/>
<pad name="2" x="-5.08" y="1.27" drill="1"/>
<pad name="3" x="-5.08" y="-1.27" drill="1"/>
<pad name="4" x="-5.08" y="-3.81" drill="1"/>
<wire x1="-4.445" y1="5.08" x2="-3.81" y2="4.445" width="0.127" layer="21"/>
<wire x1="-3.81" y1="4.445" x2="-3.81" y2="3.175" width="0.127" layer="21"/>
<wire x1="-3.81" y1="3.175" x2="-4.445" y2="2.54" width="0.127" layer="21"/>
<wire x1="-4.445" y1="2.54" x2="-3.81" y2="1.905" width="0.127" layer="21"/>
<wire x1="-3.81" y1="1.905" x2="-3.81" y2="0.635" width="0.127" layer="21"/>
<wire x1="-3.81" y1="0.635" x2="-4.445" y2="0" width="0.127" layer="21"/>
<wire x1="-4.445" y1="0" x2="-3.81" y2="-0.635" width="0.127" layer="21"/>
<wire x1="-3.81" y1="-0.635" x2="-3.81" y2="-1.905" width="0.127" layer="21"/>
<wire x1="-3.81" y1="-1.905" x2="-4.445" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-4.445" y1="-2.54" x2="-3.81" y2="-3.175" width="0.127" layer="21"/>
<wire x1="-3.81" y1="-3.175" x2="-3.81" y2="-4.445" width="0.127" layer="21"/>
<wire x1="-3.81" y1="-4.445" x2="-4.445" y2="-5.08" width="0.127" layer="21"/>
<wire x1="-6.35" y1="4.445" x2="-5.715" y2="5.08" width="0.127" layer="21"/>
<wire x1="-6.35" y1="3.175" x2="-5.715" y2="2.54" width="0.127" layer="21"/>
<wire x1="-5.715" y1="2.54" x2="-6.35" y2="1.905" width="0.127" layer="21"/>
<wire x1="-6.35" y1="0.635" x2="-5.715" y2="0" width="0.127" layer="21"/>
<wire x1="-5.715" y1="0" x2="-6.35" y2="-0.635" width="0.127" layer="21"/>
<wire x1="-6.35" y1="-1.905" x2="-5.715" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-5.715" y1="-2.54" x2="-6.35" y2="-3.175" width="0.127" layer="21"/>
<wire x1="-6.35" y1="-4.445" x2="-5.715" y2="-5.08" width="0.127" layer="21"/>
<text x="-3.175" y="-1.27" size="1.27" layer="21" align="center-left">SCL</text>
<wire x1="-6.604" y1="5.334" x2="6.604" y2="5.334" width="0.127" layer="21"/>
<wire x1="6.604" y1="5.334" x2="6.604" y2="-5.334" width="0.127" layer="21"/>
<wire x1="6.604" y1="-5.334" x2="-6.604" y2="-5.334" width="0.127" layer="21"/>
<wire x1="-6.604" y1="-5.334" x2="-6.604" y2="5.334" width="0.127" layer="21"/>
<wire x1="-6.35" y1="4.445" x2="-6.35" y2="3.175" width="0.127" layer="21"/>
<wire x1="-6.35" y1="1.905" x2="-6.35" y2="0.635" width="0.127" layer="21"/>
<wire x1="-6.35" y1="-0.635" x2="-6.35" y2="-1.905" width="0.127" layer="21"/>
<wire x1="-6.35" y1="-3.175" x2="-6.35" y2="-4.445" width="0.127" layer="21"/>
<wire x1="-5.715" y1="-5.08" x2="-4.445" y2="-5.08" width="0.127" layer="21"/>
<text x="-3.175" y="1.27" size="1.27" layer="21" align="center-left">GND</text>
<text x="-3.175" y="3.81" size="1.27" layer="21" align="center-left">VIN</text>
<text x="-3.175" y="-3.81" size="1.27" layer="21" align="center-left">SDA</text>
<hole x="3.81" y="2.54" drill="3"/>
<wire x1="2.54" y1="-1.27" x2="5.08" y2="-1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="-1.27" x2="5.08" y2="-3.81" width="0.127" layer="21"/>
<wire x1="5.08" y1="-3.81" x2="2.54" y2="-3.81" width="0.127" layer="21"/>
<wire x1="2.54" y1="-3.81" x2="2.54" y2="-1.27" width="0.127" layer="21"/>
</package>
</packages>
<symbols>
<symbol name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<pin name="IN+" x="-17.78" y="5.08" visible="pin" length="middle"/>
<pin name="IN-" x="-17.78" y="-5.08" visible="pin" length="middle"/>
<pin name="OUT+" x="17.78" y="5.08" visible="pin" length="middle" rot="R180"/>
<pin name="OUT-" x="17.78" y="-5.08" visible="pin" length="middle" rot="R180"/>
<wire x1="-12.7" y1="10.16" x2="12.7" y2="10.16" width="0.254" layer="94"/>
<wire x1="12.7" y1="10.16" x2="12.7" y2="-10.16" width="0.254" layer="94"/>
<wire x1="12.7" y1="-10.16" x2="-12.7" y2="-10.16" width="0.254" layer="94"/>
<wire x1="-12.7" y1="-10.16" x2="-12.7" y2="10.16" width="0.254" layer="94"/>
<text x="-12.7" y="15.24" size="1.778" layer="95">&gt;NAME</text>
<text x="-12.7" y="12.7" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
<symbol name="BATTERY-CHARGER-LI-PROT">
<description>&lt;b&gt;Protected Lithium Battery 5V Charger&lt;/b&gt; with micro-USB connector</description>
<pin name="IN+" x="-17.78" y="7.62" visible="pin" length="middle"/>
<pin name="IN-" x="-17.78" y="-7.62" visible="pin" length="middle"/>
<pin name="B+" x="15.24" y="2.54" visible="pin" length="middle" rot="R180"/>
<pin name="B-" x="15.24" y="-2.54" visible="pin" length="middle" rot="R180"/>
<wire x1="-12.7" y1="10.16" x2="10.16" y2="10.16" width="0.254" layer="94"/>
<wire x1="10.16" y1="10.16" x2="10.16" y2="-10.16" width="0.254" layer="94"/>
<wire x1="10.16" y1="-10.16" x2="-12.7" y2="-10.16" width="0.254" layer="94"/>
<wire x1="-12.7" y1="-10.16" x2="-12.7" y2="-3.81" width="0.254" layer="94"/>
<wire x1="-12.7" y1="-3.81" x2="-12.7" y2="3.81" width="0.254" layer="94"/>
<wire x1="-12.7" y1="3.81" x2="-12.7" y2="10.16" width="0.254" layer="94"/>
<wire x1="-12.7" y1="3.81" x2="-3.81" y2="3.81" width="0.254" layer="94"/>
<wire x1="-3.81" y1="3.81" x2="-3.81" y2="-3.81" width="0.254" layer="94"/>
<wire x1="-3.81" y1="-3.81" x2="-12.7" y2="-3.81" width="0.254" layer="94"/>
<text x="-8.382" y="0" size="1.778" layer="94" align="center">USB</text>
<text x="-12.7" y="15.24" size="1.778" layer="95">&gt;NAME</text>
<text x="-12.7" y="12.7" size="1.778" layer="96">&gt;VALUE</text>
<pin name="OUT+" x="15.24" y="7.62" visible="pin" length="middle" rot="R180"/>
<pin name="OUT-" x="15.24" y="-7.62" visible="pin" length="middle" rot="R180"/>
</symbol>
<symbol name="WIRELESS-LORA-RFM95W">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt;</description>
<pin name="GND.1" x="-17.78" y="10.16" length="middle" direction="pwr"/>
<pin name="MISO" x="-17.78" y="7.62" length="middle"/>
<pin name="MOSI" x="-17.78" y="5.08" length="middle"/>
<pin name="SCK" x="-17.78" y="2.54" length="middle"/>
<pin name="NSS" x="-17.78" y="0" length="middle"/>
<pin name="RST" x="-17.78" y="-2.54" length="middle"/>
<pin name="DIO5" x="-17.78" y="-5.08" length="middle"/>
<pin name="GND.2" x="-17.78" y="-7.62" length="middle" direction="pwr"/>
<wire x1="12.7" y1="12.7" x2="12.7" y2="-10.16" width="0.254" layer="94"/>
<wire x1="12.7" y1="-10.16" x2="-12.7" y2="-10.16" width="0.254" layer="94"/>
<wire x1="-12.7" y1="-10.16" x2="-12.7" y2="12.7" width="0.254" layer="94"/>
<text x="-12.7" y="17.78" size="1.778" layer="95">&gt;NAME</text>
<text x="-12.7" y="15.24" size="1.778" layer="96">&gt;VALUE</text>
<pin name="ANT" x="17.78" y="-7.62" length="middle" direction="pas" rot="R180"/>
<pin name="GND.3" x="17.78" y="-5.08" length="middle" direction="pwr" rot="R180"/>
<pin name="DIO3" x="17.78" y="-2.54" length="middle" rot="R180"/>
<pin name="DIO4" x="17.78" y="0" length="middle" rot="R180"/>
<pin name="3.3V" x="17.78" y="2.54" length="middle" direction="pwr" rot="R180"/>
<pin name="DIO0" x="17.78" y="5.08" length="middle" rot="R180"/>
<pin name="DIO1" x="17.78" y="7.62" length="middle" rot="R180"/>
<pin name="DIO2" x="17.78" y="10.16" length="middle" rot="R180"/>
<wire x1="-12.7" y1="12.7" x2="12.7" y2="12.7" width="0.254" layer="94"/>
</symbol>
<symbol name="TEMP-HUM-SENSOR-HTU21D">
<description>&lt;b&gt;Digital Humidity &amp; Temperature Sensor&lt;/b&gt; based on &lt;b&gt;HTU21D&lt;/b&gt; device</description>
<pin name="VIN" x="-15.24" y="5.08" length="middle" direction="pwr"/>
<pin name="GND" x="-15.24" y="2.54" length="middle" direction="pwr"/>
<pin name="SCL" x="-15.24" y="0" length="middle"/>
<pin name="SDA" x="-15.24" y="-2.54" length="middle"/>
<wire x1="-10.16" y1="10.16" x2="7.62" y2="10.16" width="0.254" layer="94"/>
<wire x1="7.62" y1="-7.62" x2="-10.16" y2="-7.62" width="0.254" layer="94"/>
<wire x1="-10.16" y1="-7.62" x2="-10.16" y2="10.16" width="0.254" layer="94"/>
<text x="-10.16" y="15.24" size="1.778" layer="95">&gt;NAME</text>
<text x="-10.16" y="12.7" size="1.778" layer="95">&gt;VALUE</text>
<wire x1="7.62" y1="10.16" x2="7.62" y2="-7.62" width="0.254" layer="94"/>
<wire x1="5.08" y1="-5.08" x2="5.08" y2="0" width="0.254" layer="94"/>
<wire x1="5.08" y1="0" x2="0" y2="0" width="0.254" layer="94"/>
<wire x1="0" y1="0" x2="0" y2="-5.08" width="0.254" layer="94"/>
<wire x1="0" y1="-5.08" x2="5.08" y2="-5.08" width="0.254" layer="94"/>
<circle x="0.762" y="-2.54" radius="0.359209375" width="0.254" layer="94"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;LM2596&lt;/b&gt; datasheet available here:&lt;br /&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/lm2596.pdf"&gt;http://www.ti.com/lit/ds/symlink/lm2596.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/lm2596+power+regulator"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-DOWN-LM2596"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-DOWN-LM2596" x="0" y="0"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-DOWN-LM2596">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-CHARGER-LI-PROT">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt; with protection circuit
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://www.instructables.com/id/DIY-Lithium-ion-Battery-Charger/step4/TP4056-based-lithium-ion-battery-charger-module/"&gt;
http://www.instructables.com/id/DIY-Lithium-ion-Battery-Charger/step4/TP4056-based-lithium-ion-battery-charger-module/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/tp4056+charger+usb+protection"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-CHARGER-LI-PROT"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-CHARGER-LI-PROT" x="0" y="0"/>
</gates>
<devices>
<device name="" package="BATTERY-CHARGER-LI-PROT">
<connects>
<connect gate="G$1" pin="B+" pad="B+"/>
<connect gate="G$1" pin="B-" pad="B-"/>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-LORA-RFM95W">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt; based on &lt;b&gt;SX1276&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/RFM95W+transceiver"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-LORA-RFM95W"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-LORA-RFM95W" x="0" y="0"/>
</gates>
<devices>
<device name="#THT" package="WIRELESS-LORA-RFM95W#THT">
<connects>
<connect gate="G$1" pin="3.3V" pad="B4"/>
<connect gate="G$1" pin="ANT" pad="B8"/>
<connect gate="G$1" pin="DIO0" pad="B3"/>
<connect gate="G$1" pin="DIO1" pad="B2"/>
<connect gate="G$1" pin="DIO2" pad="B1"/>
<connect gate="G$1" pin="DIO3" pad="B6"/>
<connect gate="G$1" pin="DIO4" pad="B5"/>
<connect gate="G$1" pin="DIO5" pad="A7"/>
<connect gate="G$1" pin="GND.1" pad="A1"/>
<connect gate="G$1" pin="GND.2" pad="A8"/>
<connect gate="G$1" pin="GND.3" pad="B7"/>
<connect gate="G$1" pin="MISO" pad="A2"/>
<connect gate="G$1" pin="MOSI" pad="A3"/>
<connect gate="G$1" pin="NSS" pad="A5"/>
<connect gate="G$1" pin="RST" pad="A6"/>
<connect gate="G$1" pin="SCK" pad="A4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="#SMD" package="WIRELESS-LORA-RFM95W#SMD">
<connects>
<connect gate="G$1" pin="3.3V" pad="B4"/>
<connect gate="G$1" pin="ANT" pad="B8"/>
<connect gate="G$1" pin="DIO0" pad="B3"/>
<connect gate="G$1" pin="DIO1" pad="B2"/>
<connect gate="G$1" pin="DIO2" pad="B1"/>
<connect gate="G$1" pin="DIO3" pad="B6"/>
<connect gate="G$1" pin="DIO4" pad="B5"/>
<connect gate="G$1" pin="DIO5" pad="A7"/>
<connect gate="G$1" pin="GND.1" pad="A1"/>
<connect gate="G$1" pin="GND.2" pad="A8"/>
<connect gate="G$1" pin="GND.3" pad="B7"/>
<connect gate="G$1" pin="MISO" pad="A2"/>
<connect gate="G$1" pin="MOSI" pad="A3"/>
<connect gate="G$1" pin="NSS" pad="A5"/>
<connect gate="G$1" pin="RST" pad="A6"/>
<connect gate="G$1" pin="SCK" pad="A4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP-HUM-SENSOR-HTU21D">
<description>&lt;b&gt;Digital Humidity &amp; Temperature Sensor&lt;/b&gt; based on &lt;b&gt;HTU21D&lt;/b&gt; device
&lt;p&gt;More information about &lt;b&gt;HTU21D&lt;/b&gt; device is available here:&lt;br&gt;
&lt;a href="http://futureeverything.org/wp-content/uploads/2014/05/Humidity-Datasheet.pdf"&gt;http://futureeverything.org/wp-content/uploads/2014/05/Humidity-Datasheet.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;HTU21D&lt;/b&gt; Arudino Library is available here:&lt;br&gt;
&lt;a href="https://learn.sparkfun.com/tutorials/htu21d-humidity-sensor-hookup-guide/htu21d-library-and-functions"&gt;https://learn.sparkfun.com/tutorials/htu21d-humidity-sensor-hookup-guide/htu21d-library-and-functions&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/htu21d+board"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TEMP-HUM-SENSOR-HTU21D"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEMP-HUM-SENSOR-HTU21D" x="0" y="0"/>
</gates>
<devices>
<device name="" package="TEMP-HUM-SENSOR-HTU21D">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
<wire x1="-1.6" y1="0.7" x2="1.6" y2="0.7" width="0.0508" layer="39"/>
<wire x1="1.6" y1="0.7" x2="1.6" y2="-0.7" width="0.0508" layer="39"/>
<wire x1="1.6" y1="-0.7" x2="-1.6" y2="-0.7" width="0.0508" layer="39"/>
<wire x1="-1.6" y1="-0.7" x2="-1.6" y2="0.7" width="0.0508" layer="39"/>
<wire x1="-0.356" y1="0.432" x2="0.356" y2="0.432" width="0.1016" layer="51"/>
<wire x1="-0.356" y1="-0.419" x2="0.356" y2="-0.419" width="0.1016" layer="51"/>
<smd name="1" x="-0.85" y="0" dx="1.1" dy="1" layer="1"/>
<smd name="2" x="0.85" y="0" dx="1.1" dy="1" layer="1"/>
<text x="0" y="0.762" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-0.762" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
<rectangle x1="-0.8382" y1="-0.4699" x2="-0.3381" y2="0.4801" layer="51"/>
<rectangle x1="0.3302" y1="-0.4699" x2="0.8303" y2="0.4801" layer="51"/>
<rectangle x1="-0.1999" y1="-0.3" x2="0.1999" y2="0.3" layer="35"/>
</package>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
<wire x1="-2.54" y1="0.762" x2="2.54" y2="0.762" width="0.2032" layer="21"/>
<wire x1="2.54" y1="0.762" x2="2.54" y2="0" width="0.2032" layer="21"/>
<wire x1="2.54" y1="0" x2="2.54" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="2.54" y1="-0.762" x2="-2.54" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="-0.762" x2="-2.54" y2="0" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="0" x2="-2.54" y2="0.762" width="0.2032" layer="21"/>
<wire x1="2.54" y1="0" x2="2.794" y2="0" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="0" x2="-2.794" y2="0" width="0.2032" layer="21"/>
<pad name="P$1" x="-3.81" y="0" drill="0.9" diameter="1.8796"/>
<pad name="P$2" x="3.81" y="0" drill="0.9" diameter="1.8796"/>
<text x="0" y="1.016" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-1.016" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="AXIAL-0.1">
<description>&lt;h3&gt;AXIAL-0.1&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.1" pitch between holes.&lt;/p&gt;</description>
<wire x1="0" y1="-0.762" x2="0" y2="0" width="0.2032" layer="21"/>
<wire x1="0" y1="0" x2="0" y2="0.762" width="0.2032" layer="21"/>
<wire x1="0.254" y1="0" x2="0" y2="0" width="0.2032" layer="21"/>
<wire x1="0" y1="0" x2="-0.254" y2="0" width="0.2032" layer="21"/>
<pad name="P$1" x="-1.27" y="0" drill="0.9" diameter="1.8796"/>
<pad name="P$2" x="1.27" y="0" drill="0.9" diameter="1.8796"/>
<text x="0" y="1.143" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-1.143" size="0.6096" layer="21" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="AXIAL-0.1-KIT">
<description>&lt;h3&gt;AXIAL-0.1-KIT&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.1" pitch between holes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.1 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;</description>
<wire x1="0" y1="-0.762" x2="0" y2="0" width="0.2032" layer="21"/>
<wire x1="0" y1="0" x2="0" y2="0.762" width="0.2032" layer="21"/>
<wire x1="0.254" y1="0" x2="0" y2="0" width="0.2032" layer="21"/>
<wire x1="0" y1="0" x2="-0.254" y2="0" width="0.2032" layer="21"/>
<pad name="P$1" x="-1.27" y="0" drill="0.9" diameter="1.8796" stop="no"/>
<pad name="P$2" x="1.27" y="0" drill="0.9" diameter="1.8796" stop="no"/>
<text x="0" y="1.143" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-1.143" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
<circle x="-1.27" y="0" radius="0.4572" width="0" layer="29"/>
<circle x="-1.27" y="0" radius="1.016" width="0" layer="30"/>
<circle x="1.27" y="0" radius="1.016" width="0" layer="30"/>
<circle x="-1.27" y="0" radius="0.4572" width="0" layer="29"/>
<circle x="1.27" y="0" radius="0.4572" width="0" layer="29"/>
</package>
<package name="AXIAL-0.3-KIT">
<description>&lt;h3&gt;AXIAL-0.3-KIT&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.3 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;</description>
<wire x1="-2.54" y1="1.27" x2="2.54" y2="1.27" width="0.254" layer="21"/>
<wire x1="2.54" y1="1.27" x2="2.54" y2="0" width="0.254" layer="21"/>
<wire x1="2.54" y1="0" x2="2.54" y2="-1.27" width="0.254" layer="21"/>
<wire x1="2.54" y1="-1.27" x2="-2.54" y2="-1.27" width="0.254" layer="21"/>
<wire x1="-2.54" y1="-1.27" x2="-2.54" y2="0" width="0.254" layer="21"/>
<wire x1="-2.54" y1="0" x2="-2.54" y2="1.27" width="0.254" layer="21"/>
<wire x1="2.54" y1="0" x2="2.794" y2="0" width="0.254" layer="21"/>
<wire x1="-2.54" y1="0" x2="-2.794" y2="0" width="0.254" layer="21"/>
<pad name="P$1" x="-3.81" y="0" drill="1.016" diameter="2.032" stop="no"/>
<pad name="P$2" x="3.81" y="0" drill="1.016" diameter="2.032" stop="no"/>
<text x="0" y="1.524" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.524" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
<polygon width="0.127" layer="30">
<vertex x="3.8201" y="-0.9449" curve="-90"/>
<vertex x="2.8652" y="-0.0152" curve="-90.011749"/>
<vertex x="3.8176" y="0.9602" curve="-90"/>
<vertex x="4.7676" y="-0.0178" curve="-90.024193"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="3.8176" y="-0.4369" curve="-90.012891"/>
<vertex x="3.3731" y="-0.0127" curve="-90"/>
<vertex x="3.8176" y="0.4546" curve="-90"/>
<vertex x="4.2595" y="-0.0025" curve="-90.012967"/>
</polygon>
<polygon width="0.127" layer="30">
<vertex x="-3.8075" y="-0.9525" curve="-90"/>
<vertex x="-4.7624" y="-0.0228" curve="-90.011749"/>
<vertex x="-3.81" y="0.9526" curve="-90"/>
<vertex x="-2.86" y="-0.0254" curve="-90.024193"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-3.81" y="-0.4445" curve="-90.012891"/>
<vertex x="-4.2545" y="-0.0203" curve="-90"/>
<vertex x="-3.81" y="0.447" curve="-90"/>
<vertex x="-3.3681" y="-0.0101" curve="-90.012967"/>
</polygon>
</package>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
<wire x1="-0.2704" y1="0.2286" x2="0.2704" y2="0.2286" width="0.1524" layer="51"/>
<wire x1="0.2704" y1="-0.2286" x2="-0.2704" y2="-0.2286" width="0.1524" layer="51"/>
<wire x1="-1.2" y1="0.65" x2="1.2" y2="0.65" width="0.0508" layer="39"/>
<wire x1="1.2" y1="0.65" x2="1.2" y2="-0.65" width="0.0508" layer="39"/>
<wire x1="1.2" y1="-0.65" x2="-1.2" y2="-0.65" width="0.0508" layer="39"/>
<wire x1="-1.2" y1="-0.65" x2="-1.2" y2="0.65" width="0.0508" layer="39"/>
<smd name="1" x="-0.58" y="0" dx="0.85" dy="0.9" layer="1"/>
<smd name="2" x="0.58" y="0" dx="0.85" dy="0.9" layer="1"/>
<text x="0" y="0.762" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-0.762" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
<rectangle x1="-0.554" y1="-0.3048" x2="-0.254" y2="0.3048" layer="51"/>
<rectangle x1="0.2588" y1="-0.3048" x2="0.5588" y2="0.3048" layer="51"/>
<rectangle x1="-0.1999" y1="-0.3" x2="0.1999" y2="0.3" layer="35"/>
</package>
<package name="0402-TIGHT">
<smd name="1" x="-0.5" y="0" dx="0.6" dy="0.6" layer="1"/>
<smd name="2" x="0.5" y="0" dx="0.6" dy="0.6" layer="1"/>
<text x="0" y="0.562" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-0.562" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
<wire x1="-0.5" y1="-0.25" x2="-0.5" y2="0.25" width="0.002540625" layer="51"/>
<wire x1="-0.5" y1="0.25" x2="0.5" y2="0.25" width="0.002540625" layer="51"/>
<wire x1="0.5" y1="0.25" x2="0.5" y2="-0.25" width="0.002540625" layer="51"/>
<wire x1="0.5" y1="-0.25" x2="-0.5" y2="-0.25" width="0.002540625" layer="51"/>
<rectangle x1="-0.5" y1="-0.25" x2="-0.3" y2="0.25" layer="51"/>
<rectangle x1="0.3" y1="-0.25" x2="0.5" y2="0.25" layer="51" rot="R180"/>
<wire x1="0.9262" y1="0.4262" x2="-0.9262" y2="0.4262" width="0.05" layer="39"/>
<wire x1="-0.9262" y1="0.4262" x2="-0.9262" y2="-0.4262" width="0.05" layer="39"/>
<wire x1="-0.9262" y1="-0.4262" x2="0.9262" y2="-0.4262" width="0.05" layer="39"/>
<wire x1="0.9262" y1="-0.4262" x2="0.9262" y2="0.4262" width="0.05" layer="39"/>
</package>
</packages>
<symbols>
<symbol name="RESISTOR">
<wire x1="-2.54" y1="0" x2="-2.159" y2="1.016" width="0.1524" layer="94"/>
<wire x1="-2.159" y1="1.016" x2="-1.524" y2="-1.016" width="0.1524" layer="94"/>
<wire x1="-1.524" y1="-1.016" x2="-0.889" y2="1.016" width="0.1524" layer="94"/>
<wire x1="-0.889" y1="1.016" x2="-0.254" y2="-1.016" width="0.1524" layer="94"/>
<wire x1="-0.254" y1="-1.016" x2="0.381" y2="1.016" width="0.1524" layer="94"/>
<wire x1="0.381" y1="1.016" x2="1.016" y2="-1.016" width="0.1524" layer="94"/>
<wire x1="1.016" y1="-1.016" x2="1.651" y2="1.016" width="0.1524" layer="94"/>
<wire x1="1.651" y1="1.016" x2="2.286" y2="-1.016" width="0.1524" layer="94"/>
<wire x1="2.286" y1="-1.016" x2="2.54" y2="0" width="0.1524" layer="94"/>
<text x="0" y="1.524" size="1.778" layer="95" font="vector" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.524" size="1.778" layer="96" font="vector" align="top-center">&gt;VALUE</text>
<pin name="2" x="5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1" rot="R180"/>
<pin name="1" x="-5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="4.7KOHM" prefix="R">
<description>&lt;h3&gt;4.7kΩ resistor&lt;/h3&gt;
&lt;p&gt;A resistor is a passive two-terminal electrical component that implements electrical resistance as a circuit element. Resistors act to reduce current flow, and, at the same time, act to lower voltage levels within circuits. - Wikipedia&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR" x="0" y="0"/>
</gates>
<devices>
<device name="-0603-1/10W-1%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE" value="4.7k"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10KOHM" prefix="R">
<description>&lt;h3&gt;10kΩ resistor&lt;/h3&gt;
&lt;p&gt;A resistor is a passive two-terminal electrical component that implements electrical resistance as a circuit element. Resistors act to reduce current flow, and, at the same time, act to lower voltage levels within circuits. - Wikipedia&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR" x="0" y="0"/>
</gates>
<devices>
<device name="-HORIZ-1/4W-1%" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12183" constant="no"/>
<attribute name="VALUE" value="10k" constant="no"/>
</technology>
</technologies>
</device>
<device name="-VERT-1/4W-1%" package="AXIAL-0.1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-VERT_KIT-1/4W-1%" package="AXIAL-0.1-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12183" constant="no"/>
<attribute name="VALUE" value="10k" constant="no"/>
</technology>
</technologies>
</device>
<device name="-VERT-1/4W-5%" package="AXIAL-0.1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-09435"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-VERT_KIT-1/4W-5%" package="AXIAL-0.1-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-09435"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ-1/4W-5%" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-09435"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ_KIT-1/4W-5%" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-09435"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ_KIT-1/4W-1%" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-VERT-1/6W-5%" package="AXIAL-0.1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-VERT_KIT-1/6W-5%" package="AXIAL-0.1-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ-1/6W-5%" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ_KIT-1/6W-5%" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-0603-1/10W-1%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-0402-1/16W-1%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-14241"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="-0402T-1/16W-1%" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-14241" constant="no"/>
<attribute name="VALUE" value="10k" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-PowerSymbols">
<description>&lt;h3&gt;SparkFun Power Symbols&lt;/h3&gt;
This library contains power, ground, and voltage-supply symbols.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
</packages>
<symbols>
<symbol name="VCC">
<description>&lt;h3&gt;VCC Voltage Supply&lt;/h3&gt;</description>
<wire x1="0.762" y1="1.27" x2="0" y2="2.54" width="0.254" layer="94"/>
<wire x1="0" y1="2.54" x2="-0.762" y2="1.27" width="0.254" layer="94"/>
<pin name="VCC" x="0" y="0" visible="off" length="short" direction="sup" rot="R90"/>
<text x="0" y="2.794" size="1.778" layer="96" align="bottom-center">&gt;VALUE</text>
</symbol>
<symbol name="DGND">
<description>&lt;h3&gt;Digital Ground Supply&lt;/h3&gt;</description>
<wire x1="-1.905" y1="0" x2="1.905" y2="0" width="0.254" layer="94"/>
<pin name="GND" x="0" y="2.54" visible="off" length="short" direction="sup" rot="R270"/>
<text x="0" y="-0.254" size="1.778" layer="96" align="top-center">&gt;VALUE</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="VCC" prefix="SUPPLY">
<description>&lt;h3&gt;VCC Voltage Supply&lt;/h3&gt;
&lt;p&gt;Positive voltage supply (traditionally for a BJT device, C=collector).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VCC" x="0" y="0"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;h3&gt;Ground Supply Symbol&lt;/h3&gt;
&lt;p&gt;Generic signal ground supply symbol.&lt;/p&gt;</description>
<gates>
<gate name="1" symbol="DGND" x="0" y="0"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="BK-18650-PC2">
<packages>
<package name="MPD_BK-18650-PC2">
<wire x1="-36.94" y1="-0.03" x2="-36.94" y2="0.08" width="0" layer="46"/>
<wire x1="-36.94" y1="1.2" x2="-35.56" y2="1.2" width="0" layer="46"/>
<wire x1="-35.56" y1="1.2" x2="-35.56" y2="-1.2" width="0" layer="46"/>
<wire x1="-35.56" y1="-1.2" x2="-36.94" y2="-1.2" width="0" layer="46"/>
<wire x1="-36.94" y1="-1.2" x2="-36.94" y2="1.2" width="0" layer="46"/>
<wire x1="35.56" y1="0.03" x2="35.56" y2="0.14" width="0" layer="46"/>
<wire x1="35.56" y1="1.2" x2="36.94" y2="1.2" width="0" layer="46"/>
<wire x1="36.94" y1="1.2" x2="36.94" y2="-1.2" width="0" layer="46"/>
<wire x1="36.94" y1="-1.2" x2="35.56" y2="-1.2" width="0" layer="46"/>
<wire x1="35.56" y1="-1.2" x2="35.56" y2="1.2" width="0" layer="46"/>
<wire x1="-38.48" y1="-10.49" x2="-38.48" y2="10.49" width="0.127" layer="51"/>
<wire x1="-38.48" y1="10.49" x2="38.48" y2="10.49" width="0.127" layer="51"/>
<wire x1="38.48" y1="10.49" x2="38.48" y2="-10.49" width="0.127" layer="51"/>
<wire x1="38.48" y1="-10.49" x2="-38.48" y2="-10.49" width="0.127" layer="51"/>
<wire x1="-38.48" y1="10.49" x2="38.48" y2="10.49" width="0.127" layer="21"/>
<wire x1="38.48" y1="10.49" x2="38.48" y2="-10.49" width="0.127" layer="21"/>
<wire x1="38.48" y1="-10.49" x2="-38.48" y2="-10.49" width="0.127" layer="21"/>
<wire x1="-38.48" y1="-10.49" x2="-38.48" y2="10.49" width="0.127" layer="21"/>
<wire x1="-38.73" y1="-10.74" x2="-38.73" y2="10.74" width="0.05" layer="39"/>
<wire x1="-38.73" y1="10.74" x2="38.73" y2="10.74" width="0.05" layer="39"/>
<wire x1="38.73" y1="10.74" x2="38.73" y2="-10.74" width="0.05" layer="39"/>
<wire x1="38.73" y1="-10.74" x2="-38.73" y2="-10.74" width="0.05" layer="39"/>
<text x="-38.4734" y="11.6222" size="1.7814" layer="25">&gt;NAME</text>
<text x="-38.5653" y="-12.7215" size="1.781009375" layer="27">&gt;VALUE</text>
<text x="-40.4673" y="-0.9015" size="1.780959375" layer="21">+</text>
<text x="39.4562" y="-0.300428125" size="1.780540625" layer="21">-</text>
<hole x="27.805" y="0" drill="3.2"/>
<hole x="-27.805" y="0" drill="3.2"/>
<pad name="P" x="-36.25" y="0" drill="1.38" shape="long" rot="R90"/>
<pad name="M" x="36.25" y="0" drill="1.38" shape="long" rot="R90"/>
</package>
</packages>
<symbols>
<symbol name="BK-18650-PC2">
<wire x1="-5.08" y1="-5.08" x2="-5.08" y2="5.08" width="0.254" layer="94"/>
<wire x1="-5.08" y1="5.08" x2="5.08" y2="5.08" width="0.254" layer="94"/>
<wire x1="5.08" y1="5.08" x2="5.08" y2="-5.08" width="0.254" layer="94"/>
<wire x1="5.08" y1="-5.08" x2="-5.08" y2="-5.08" width="0.254" layer="94"/>
<text x="-5.08493125" y="5.72055" size="1.67803125" layer="95">&gt;NAME</text>
<text x="-5.082240625" y="-7.62336875" size="1.677140625" layer="96">&gt;VALUE</text>
<pin name="+" x="-10.16" y="2.54" length="middle" direction="pas"/>
<pin name="-" x="-10.16" y="-2.54" length="middle" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BK-18650-PC2" prefix="X">
<description>HOLDER BATT 1/LI-ION PROTECTED</description>
<gates>
<gate name="G$1" symbol="BK-18650-PC2" x="0" y="0"/>
</gates>
<devices>
<device name="" package="MPD_BK-18650-PC2">
<connects>
<connect gate="G$1" pin="+" pad="P"/>
<connect gate="G$1" pin="-" pad="M"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Holder Batt 1/Li-Ion Protected "/>
<attribute name="MF" value="MPD _Memory"/>
<attribute name="MP" value="BK-18650-PC2"/>
<attribute name="PACKAGE" value="DFN-14 MPD _Memory Protection Devices_"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="switch_dip">
<packages>
<package name="418117270901">
<description>WS-BS 2.54 mm compact THT Dip Switch with raised actuator, 1 Pole</description>
<wire x1="-1.77" y1="4.8" x2="1.77" y2="4.8" width="0.127" layer="21"/>
<wire x1="1.77" y1="4.8" x2="1.77" y2="-4.8" width="0.127" layer="21"/>
<wire x1="1.77" y1="-4.8" x2="-1.77" y2="-4.8" width="0.127" layer="21"/>
<wire x1="-1.77" y1="-4.8" x2="-1.77" y2="4.8" width="0.127" layer="21"/>
<text x="-0.535" y="-2.545" size="1.27" layer="51">1</text>
<text x="0.11" y="5.67" size="0.8128" layer="25" align="bottom-center">&gt;NAME</text>
<text x="-2.19" y="-6.235" size="0.8128" layer="27">&gt;VALUE</text>
<polygon width="0.127" layer="39">
<vertex x="-2.02" y="5.05"/>
<vertex x="2.02" y="5.05"/>
<vertex x="2.02" y="-5.05"/>
<vertex x="-2.02" y="-5.05"/>
</polygon>
<circle x="-1" y="-4.5" radius="0.05" width="0.2" layer="21"/>
<pad name="1" x="0" y="-3.81" drill="0.8"/>
<pad name="A1" x="0" y="3.81" drill="0.8"/>
</package>
</packages>
<symbols>
<symbol name="1POLE">
<description>This symbol is 1pole</description>
<wire x1="-1.905" y1="7.62" x2="-1.905" y2="-7.62" width="0.2" layer="94"/>
<wire x1="-1.905" y1="7.62" x2="0" y2="7.62" width="0.2" layer="94"/>
<wire x1="0" y1="7.62" x2="1.905" y2="7.62" width="0.2" layer="94"/>
<wire x1="1.905" y1="-7.62" x2="1.905" y2="7.62" width="0.2" layer="94"/>
<wire x1="1.905" y1="-7.62" x2="0" y2="-7.62" width="0.2" layer="94"/>
<text x="-2.54" y="-5.08" size="1.778" layer="95" rot="R90">&gt;NAME</text>
<text x="4.445" y="-5.08" size="1.778" layer="96" rot="R90">&gt;VALUE</text>
<wire x1="0" y1="-7.62" x2="-1.905" y2="-7.62" width="0.2" layer="94"/>
<wire x1="0" y1="-7.62" x2="0" y2="-2.54" width="0.254" layer="94"/>
<wire x1="0" y1="7.62" x2="0" y2="2.54" width="0.254" layer="94"/>
<circle x="0" y="2.032" radius="0.508" width="0.254" layer="94"/>
<circle x="0" y="-2.032" radius="0.508" width="0.254" layer="94"/>
<wire x1="0.51" y1="-2.05" x2="1.09" y2="2.03" width="0.254" layer="94"/>
<pin name="1" x="0" y="-12.7" visible="pad" length="middle" direction="pas" rot="R90"/>
<pin name="A1" x="0" y="12.7" visible="pad" length="middle" direction="pas" rot="R270"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="418117270901" prefix="S">
<description>&lt;B&gt;2.54 mm compact THT with raised actuator WS-DITV, 1 Pole&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WS_BS_4181172709xx_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WS_BS_4181172709xx_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR"&gt;http://katalog.we-online.de/en/em/DITV_2_54_COMPACT_THT_WITH_RAISED_ACTUATOR&lt;/a&gt;&lt;p&gt;



2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE" x="0" y="0"/>
</gates>
<devices>
<device name="" package="418117270901">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Switch Slide Dip Spst 25ma 24v "/>
<attribute name="MF" value="Wurth Electronics"/>
<attribute name="MP" value="418117270901"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-RGB-THRU">
<description>&lt;h3&gt;LED - RGB PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Area:5 x 5.8 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Datasheet Referenced: &lt;a href="https://www.sparkfun.com/datasheets/Components/YSL-R596CR3G4B5C-C10.pdf"&gt;YSL-R596CR3G4B5C&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-RGB-CA&lt;/li&gt;
&lt;li&gt;LED-RGB-CC&lt;/li&gt;</description>
<wire x1="2.5" y1="-1" x2="2.5" y2="1" width="0.127" layer="51"/>
<wire x1="2.5" y1="-1" x2="2.5" y2="1" width="0.127" layer="51" curve="-316.397181"/>
<pad name="2" x="0.635" y="0" drill="0.762" diameter="0.889" shape="long" rot="R90"/>
<pad name="1" x="1.905" y="0" drill="0.762" diameter="0.889" shape="long" rot="R90"/>
<pad name="3" x="-0.635" y="0" drill="0.762" diameter="0.889" shape="long" rot="R90"/>
<pad name="4" x="-1.905" y="0" drill="0.762" diameter="0.889" shape="long" rot="R90"/>
<wire x1="2.5" y1="-1" x2="2.5" y2="1" width="0.127" layer="22"/>
<text x="0" y="2.8575" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.8575" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
<wire x1="2.5" y1="-1" x2="2.5" y2="1" width="0.127" layer="21"/>
<wire x1="2.5" y1="-1" x2="2.5" y2="1" width="0.127" layer="21" curve="-316.397181"/>
</package>
<package name="LED_PIRANHA_5MM">
<description>&lt;h3&gt;LED 5mm PTH - Piranha&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.5mm, 5.06 mm&lt;/li&gt;
&lt;li&gt;Area:5mm x 5mm &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/YSRGB7A5BSW25.pdf"&gt;YSRGB7A5BSW25&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED Pirahana&lt;/li&gt;</description>
<wire x1="-3.81" y1="-3.81" x2="3.69" y2="-3.81" width="0.127" layer="21"/>
<wire x1="3.69" y1="-3.81" x2="3.69" y2="3.69" width="0.127" layer="21"/>
<wire x1="3.69" y1="3.69" x2="-2.81" y2="3.69" width="0.127" layer="21"/>
<wire x1="-2.81" y1="3.69" x2="-3.81" y2="2.69" width="0.127" layer="21"/>
<wire x1="-3.81" y1="2.69" x2="-3.81" y2="-3.81" width="0.127" layer="21"/>
<pad name="-" x="-2.684" y="-2.684" drill="0.9"/>
<pad name="R" x="2.579" y="-2.696" drill="0.9"/>
<pad name="B" x="-2.688" y="2.574" drill="0.9"/>
<pad name="G" x="2.575" y="2.562" drill="0.9"/>
<text x="-1.65" y="2.323" size="0.6096" layer="25" font="vector" ratio="20">B</text>
<text x="0.962" y="2.298" size="0.6096" layer="25" font="vector" ratio="20">G</text>
<text x="1.037" y="-3.131" size="0.6096" layer="25" font="vector" ratio="20">R</text>
<text x="-1.524" y="-3.031" size="0.6096" layer="25" font="vector" ratio="20">-</text>
<text x="0" y="4.064" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-4.064" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
<circle x="-3.81" y="3.4925" radius="0.254" width="0" layer="21"/>
</package>
</packages>
<symbols>
<symbol name="LED-RGB-CC">
<description>&lt;h3&gt;RGB LED - Common Cathode&lt;/h3&gt;
&lt;p&gt;4 pin Common Cathode RGB LED&lt;/p&gt;</description>
<wire x1="10.16" y1="5.08" x2="10.16" y2="-5.08" width="0.254" layer="94"/>
<wire x1="10.16" y1="-5.08" x2="-7.62" y2="-5.08" width="0.254" layer="94"/>
<wire x1="-7.62" y1="-5.08" x2="-7.62" y2="5.08" width="0.254" layer="94"/>
<wire x1="-7.62" y1="5.08" x2="10.16" y2="5.08" width="0.254" layer="94"/>
<wire x1="1.27" y1="1.27" x2="1.27" y2="0" width="0.254" layer="94"/>
<wire x1="1.27" y1="0" x2="1.27" y2="-1.27" width="0.254" layer="94"/>
<wire x1="1.27" y1="-1.27" x2="2.54" y2="0" width="0.254" layer="94"/>
<wire x1="2.54" y1="0" x2="1.27" y2="1.27" width="0.254" layer="94"/>
<wire x1="2.54" y1="1.27" x2="2.54" y2="0" width="0.254" layer="94"/>
<wire x1="2.54" y1="0" x2="2.54" y2="-1.27" width="0.254" layer="94"/>
<wire x1="2.54" y1="0" x2="3.81" y2="0" width="0.254" layer="94"/>
<wire x1="1.27" y1="0" x2="0" y2="0" width="0.254" layer="94"/>
<text x="-7.62" y="5.3975" size="1.778" layer="95" font="vector">&gt;NAME</text>
<text x="-7.62" y="-5.3975" size="1.778" layer="95" font="vector" align="top-left">&gt;VALUE</text>
<pin name="GRN" x="-10.16" y="-2.54" visible="pin" length="short"/>
<pin name="BLU" x="-10.16" y="0" visible="pin" length="short"/>
<pin name="C" x="12.7" y="0" visible="pin" length="short" rot="R180"/>
<pin name="RED" x="-10.16" y="2.54" visible="pin" length="short"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED-RGB-CC" prefix="D" uservalue="yes">
<description>&lt;h3&gt;LED-RGB Common Cathode&lt;/h3&gt;

&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt; LED RGB-THRU&lt;/li&gt;
&lt;li&gt; LED_PIRANHA_5MM&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;


&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/9264]”&gt;RGB Diffused Common Cathode- Diffuse&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/105]”&gt;RGB Diffused Common Cathode - Clear&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/11679]”&gt;LED-RGB 5mm Square (Piranha)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-RGB-CC" x="-2.54" y="0"/>
</gates>
<devices>
<device name="DIFFUSE" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09434"/>
<attribute name="VALUE" value="DIFFUSE" constant="no"/>
</technology>
</technologies>
</device>
<device name="CLEAR" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08418"/>
<attribute name="VALUE" value="CLEAR" constant="no"/>
</technology>
</technologies>
</device>
<device name="PIRANHA" package="LED_PIRANHA_5MM">
<connects>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="C" pad="-"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="COM-11679" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pic16f6xx_14pin">
<packages>
<package name="DIL14">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
<wire x1="-11.43" y1="-0.635" x2="-11.43" y2="-2.54" width="0.1524" layer="21"/>
<wire x1="-11.43" y1="-0.635" x2="-11.43" y2="0.635" width="0.1524" layer="21" curve="180"/>
<wire x1="6.35" y1="-2.54" x2="-11.43" y2="-2.54" width="0.1524" layer="21"/>
<wire x1="6.35" y1="-2.54" x2="6.35" y2="2.54" width="0.1524" layer="21"/>
<wire x1="-11.43" y1="2.54" x2="6.35" y2="2.54" width="0.1524" layer="21"/>
<wire x1="-11.43" y1="2.54" x2="-11.43" y2="0.635" width="0.1524" layer="21"/>
<pad name="1" x="-10.16" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="2" x="-7.62" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="3" x="-5.08" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="4" x="-2.54" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="5" x="0" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="6" x="2.54" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="7" x="5.08" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="8" x="5.08" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="9" x="2.54" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="10" x="0" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="11" x="-2.54" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="12" x="-5.08" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="13" x="-7.62" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="14" x="-10.16" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<text x="-11.8618" y="-2.54" size="1.778" layer="25" ratio="10" rot="R90">&gt;NAME</text>
<text x="-10.16" y="-0.889" size="1.778" layer="27" ratio="10">&gt;VALUE</text>
</package>
<package name="SO-14W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
<wire x1="-5.6642" y1="-3.6957" x2="3.3274" y2="-3.6957" width="0.1524" layer="21"/>
<wire x1="3.3274" y1="-3.6957" x2="3.3274" y2="3.6703" width="0.1524" layer="21"/>
<wire x1="3.3274" y1="3.6703" x2="-5.6642" y2="3.6703" width="0.1524" layer="21"/>
<wire x1="-5.6642" y1="3.6703" x2="-5.6642" y2="-3.6957" width="0.1524" layer="21"/>
<circle x="-4.6736" y="-2.7813" radius="0.5334" width="0.1524" layer="21"/>
<smd name="1" x="-5.08" y="-4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="2" x="-3.81" y="-4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="3" x="-2.54" y="-4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="4" x="-1.27" y="-4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="5" x="0" y="-4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="6" x="1.27" y="-4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="7" x="2.54" y="-4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="8" x="2.5273" y="4.8006" dx="0.762" dy="1.143" layer="1"/>
<smd name="9" x="1.2573" y="4.8006" dx="0.762" dy="1.143" layer="1"/>
<smd name="10" x="0" y="4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="11" x="-1.27" y="4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="12" x="-2.54" y="4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="13" x="-3.81" y="4.7879" dx="0.762" dy="1.143" layer="1"/>
<smd name="14" x="-5.08" y="4.7879" dx="0.762" dy="1.143" layer="1"/>
<text x="-6.0579" y="-3.81" size="1.778" layer="25" ratio="10" rot="R90">&gt;NAME</text>
<text x="5.3721" y="-3.81" size="1.778" layer="27" ratio="10" rot="R90">&gt;VALUE</text>
<rectangle x1="2.3368" y1="3.7211" x2="2.7432" y2="5.0673" layer="51"/>
<rectangle x1="1.0668" y1="3.7211" x2="1.4732" y2="5.0673" layer="51"/>
<rectangle x1="-0.2032" y1="3.7211" x2="0.2032" y2="5.0673" layer="51"/>
<rectangle x1="-1.4732" y1="3.7211" x2="-1.0668" y2="5.0673" layer="51"/>
<rectangle x1="-2.7432" y1="3.7211" x2="-2.3368" y2="5.0673" layer="51"/>
<rectangle x1="-4.0132" y1="3.7211" x2="-3.6068" y2="5.0673" layer="51"/>
<rectangle x1="-5.2832" y1="3.7211" x2="-4.8768" y2="5.0673" layer="51"/>
<rectangle x1="-5.2832" y1="-5.0927" x2="-4.8768" y2="-3.7465" layer="51"/>
<rectangle x1="-4.0132" y1="-5.0927" x2="-3.6068" y2="-3.7465" layer="51"/>
<rectangle x1="-2.7432" y1="-5.0927" x2="-2.3368" y2="-3.7465" layer="51"/>
<rectangle x1="-1.4732" y1="-5.0927" x2="-1.0668" y2="-3.7465" layer="51"/>
<rectangle x1="-0.2032" y1="-5.0927" x2="0.2032" y2="-3.7465" layer="51"/>
<rectangle x1="1.0668" y1="-5.0927" x2="1.4732" y2="-3.7465" layer="51"/>
<rectangle x1="2.3368" y1="-5.0927" x2="2.7432" y2="-3.7465" layer="51"/>
</package>
</packages>
<symbols>
<symbol name="PIC16F6*">
<wire x1="17.78" y1="-17.78" x2="-10.16" y2="-17.78" width="0.4064" layer="94"/>
<wire x1="-10.16" y1="-17.78" x2="-10.16" y2="17.78" width="0.4064" layer="94"/>
<wire x1="-10.16" y1="17.78" x2="17.78" y2="17.78" width="0.4064" layer="94"/>
<wire x1="17.78" y1="17.78" x2="17.78" y2="-17.78" width="0.4064" layer="94"/>
<text x="-10.16" y="19.05" size="1.778" layer="95">&gt;NAME</text>
<text x="-10.16" y="-20.32" size="1.778" layer="96">&gt;VALUE</text>
<pin name="MCLR/RA3" x="-12.7" y="-5.08" length="short" direction="in"/>
<pin name="OSC1/RA5" x="-12.7" y="0" length="short" direction="in"/>
<pin name="RA0/AN0" x="20.32" y="-12.7" length="short" rot="R180"/>
<pin name="RA1/AN1" x="20.32" y="-10.16" length="short" rot="R180"/>
<pin name="RA2/AN2" x="20.32" y="-7.62" length="short" rot="R180"/>
<pin name="RC0/AN4" x="20.32" y="2.54" length="short" rot="R180"/>
<pin name="RC1/AN5" x="20.32" y="5.08" length="short" rot="R180"/>
<pin name="RC2/AN6" x="20.32" y="7.62" length="short" rot="R180"/>
<pin name="RC3/AN7" x="20.32" y="10.16" length="short" rot="R180"/>
<pin name="RC4" x="20.32" y="12.7" length="short" rot="R180"/>
<pin name="RC5" x="20.32" y="15.24" length="short" rot="R180"/>
<pin name="OSC2/RA4" x="-12.7" y="-2.54" length="short" direction="out"/>
<pin name="VSS" x="-12.7" y="-15.24" length="short" direction="pwr"/>
<pin name="VDD" x="-12.7" y="15.24" length="short" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PIC16F8*" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;&lt;p&gt;
&lt;B&gt;14-Pin&lt;/b&gt;, 8-Bit PIC16F8X Family - CMOS Flash &lt;p&gt;
Pin Compatible :&lt;p&gt;
16F630, 16F676, 16F684, 16F688 &lt;p&gt;

&lt;p&gt;&lt;BR&gt;Keywords: PIC16F630, PIC16F676, PIC16F684, PIC16F688</description>
<gates>
<gate name="G$1" symbol="PIC16F6*" x="-2.54" y="0"/>
</gates>
<devices>
<device name="DIL" package="DIL14">
<connects>
<connect gate="G$1" pin="MCLR/RA3" pad="4"/>
<connect gate="G$1" pin="OSC1/RA5" pad="2"/>
<connect gate="G$1" pin="OSC2/RA4" pad="3"/>
<connect gate="G$1" pin="RA0/AN0" pad="13"/>
<connect gate="G$1" pin="RA1/AN1" pad="12"/>
<connect gate="G$1" pin="RA2/AN2" pad="11"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SO-14W">
<connects>
<connect gate="G$1" pin="MCLR/RA3" pad="4"/>
<connect gate="G$1" pin="OSC1/RA5" pad="2"/>
<connect gate="G$1" pin="OSC2/RA4" pad="3"/>
<connect gate="G$1" pin="RA0/AN0" pad="13"/>
<connect gate="G$1" pin="RA1/AN1" pad="12"/>
<connect gate="G$1" pin="RA2/AN2" pad="11"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
<description>&lt;h3&gt;TO-92 3-Pin PTH AMMO package&lt;/h3&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Dimensions:  3.68 x 4.83 x 4.83 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;DS18B20&lt;/li&gt;
&lt;/ul&gt;</description>
<wire x1="-2.0946" y1="-1.651" x2="-0.7863" y2="2.5485" width="0.2032" layer="21" curve="-111.098957" cap="flat"/>
<wire x1="0.7863" y1="2.5484" x2="2.0945" y2="-1.651" width="0.2032" layer="21" curve="-111.09954" cap="flat"/>
<wire x1="-2.0945" y1="-1.651" x2="2.0945" y2="-1.651" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="2.54" x2="0.635" y2="2.54" width="0.2032" layer="21" curve="-25.057615"/>
<wire x1="0.635" y1="2.54" x2="1.905" y2="1.905" width="0.2032" layer="21" curve="-28.072487"/>
<wire x1="-1.905" y1="1.905" x2="0.635" y2="2.54" width="0.2032" layer="21" curve="-53.130102"/>
<pad name="3" x="2.54" y="0" drill="0.8128" diameter="1.8796"/>
<pad name="2" x="0" y="0" drill="0.8128" diameter="1.8796"/>
<pad name="1" x="-2.54" y="0" drill="0.8128" diameter="1.8796"/>
<text x="0" y="-1.778" size="0.6096" layer="25" font="vector" ratio="20" rot="R180" align="bottom-center">&gt;NAME</text>
<text x="0" y="2.794" size="0.6096" layer="27" font="vector" ratio="20" rot="R180" align="top-center">&gt;VALUE</text>
</package>
<package name="BRM-2508">
<description>&lt;h3&gt;BRM-2A18 Infrared Receiver - Horizontal Facing&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Area: 6.0 x 5.6 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 m,&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;BRM-2A18&lt;/li&gt;
&lt;li&gt;BRM-2508&lt;/li&gt;
&lt;/ul&gt;</description>
<pad name="1" x="-2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<rectangle x1="-2.794" y1="-0.254" x2="-2.286" y2="0.254" layer="51"/>
<wire x1="-3" y1="-2.4" x2="-2.2" y2="-2.4" width="0.127" layer="51"/>
<wire x1="-2.2" y1="-2.4" x2="2.2" y2="-2.4" width="0.127" layer="51"/>
<wire x1="2.2" y1="-2.4" x2="3" y2="-2.4" width="0.127" layer="51"/>
<wire x1="-3" y1="1.5" x2="3" y2="1.5" width="0.127" layer="51"/>
<wire x1="-3" y1="1.5" x2="-3" y2="-2.4" width="0.127" layer="51"/>
<wire x1="3" y1="1.5" x2="3" y2="-2.4" width="0.127" layer="51"/>
<wire x1="2.2" y1="-2.4" x2="-2.2" y2="-2.4" width="0.127" layer="51" curve="-151.38954"/>
<circle x="-2.5" y="-1.7" radius="0.2236" width="0.127" layer="51"/>
<wire x1="-3" y1="1.627" x2="3" y2="1.627" width="0.2032" layer="21"/>
<wire x1="3" y1="1.627" x2="3" y2="1.1" width="0.2032" layer="21"/>
<wire x1="-1.39" y1="-1.1" x2="-3.69" y2="-1.1" width="0.2032" layer="21"/>
<wire x1="-1.39" y1="1.1" x2="-3.69" y2="1.1" width="0.2032" layer="21"/>
<wire x1="-3.69" y1="1.1" x2="-3.69" y2="-1.1" width="0.2032" layer="21"/>
<wire x1="-1.39" y1="1.1" x2="-1.39" y2="-1.1" width="0.2032" layer="21"/>
<text x="0" y="1.778" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.54" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
</package>
<package name="BRM-2508_VERT">
<description>&lt;h3&gt;BRM-2A18 Infrared Receive - Vertical Facingr&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Area: 6.0 x 5.6 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 m,&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;BRM-2A18&lt;/li&gt;
&lt;li&gt;BRM-2508&lt;/li&gt;
&lt;/ul&gt;</description>
<pad name="1" x="-2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<rectangle x1="-2.794" y1="-0.254" x2="-2.286" y2="0.254" layer="51"/>
<wire x1="-3" y1="8.18" x2="3" y2="8.18" width="0.127" layer="51"/>
<wire x1="-3" y1="1.23" x2="3" y2="1.23" width="0.127" layer="51"/>
<circle x="-2.54" y="0.7" radius="0.2236" width="0.127" layer="51"/>
<wire x1="-3" y1="8.2" x2="3" y2="8.2" width="0.2032" layer="21"/>
<wire x1="-1.39" y1="-1.1" x2="-3.69" y2="-1.1" width="0.2032" layer="21"/>
<wire x1="-1.39" y1="1.1" x2="-3.69" y2="1.1" width="0.2032" layer="21"/>
<wire x1="-3.69" y1="1.1" x2="-3.69" y2="-1.1" width="0.2032" layer="21"/>
<wire x1="-1.39" y1="1.1" x2="-1.39" y2="-1.1" width="0.2032" layer="21"/>
<circle x="0" y="5.48" radius="2.5" width="0.127" layer="51"/>
<wire x1="-3" y1="8.18" x2="-3" y2="1.23" width="0.127" layer="51"/>
<wire x1="3" y1="8.18" x2="3" y2="1.23" width="0.127" layer="51"/>
<wire x1="0" y1="1.2" x2="0" y2="0" width="0.127" layer="51"/>
<wire x1="-2.5" y1="0" x2="-2" y2="0" width="0.127" layer="51"/>
<wire x1="-2" y1="0" x2="-2" y2="1.2" width="0.127" layer="51"/>
<wire x1="2.5" y1="0" x2="2" y2="0" width="0.127" layer="51"/>
<wire x1="2" y1="0" x2="2" y2="1.2" width="0.127" layer="51"/>
<wire x1="-3" y1="1.2" x2="3" y2="1.2" width="0.2032" layer="21"/>
<wire x1="-3" y1="8.18" x2="-3" y2="1.23" width="0.2032" layer="21"/>
<wire x1="3" y1="8.18" x2="3" y2="1.23" width="0.2032" layer="21"/>
<wire x1="2.34923125" y1="4.62495" x2="2.34923125" y2="6.33505" width="0.2032" layer="21" curve="39.999989"/>
<wire x1="0.85505" y1="7.82923125" x2="-0.85505" y2="7.82923125" width="0.2032" layer="21" curve="39.999989"/>
<wire x1="-2.34923125" y1="6.33505" x2="-2.34923125" y2="4.62495" width="0.2032" layer="21" curve="39.999989"/>
<wire x1="-0.85505" y1="3.13076875" x2="0.85505" y2="3.13076875" width="0.2032" layer="21" curve="39.999989"/>
<text x="0" y="8.382" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
</package>
</packages>
<symbols>
<symbol name="DS18B20">
<description>&lt;h3&gt;Dallas/Maxim DS18B20 1-Wire Temperature Sensor&lt;/h3&gt;
&lt;p&gt;The DS18B20 reports degrees C with 9 to 12-bit precision, -55C to 125C (+/-0.5C). Each sensor has a unique 64-Bit Serial number etched into it - allows for a huge number of sensors to be used on one data bus.&lt;/p&gt;</description>
<wire x1="-7.62" y1="7.62" x2="-7.62" y2="-7.62" width="0.254" layer="94"/>
<wire x1="-7.62" y1="-7.62" x2="5.08" y2="-7.62" width="0.254" layer="94"/>
<wire x1="5.08" y1="-7.62" x2="5.08" y2="7.62" width="0.254" layer="94"/>
<wire x1="5.08" y1="7.62" x2="-7.62" y2="7.62" width="0.254" layer="94"/>
<pin name="DQ" x="-10.16" y="0" length="short"/>
<pin name="VDD" x="-10.16" y="5.08" length="short" direction="pwr"/>
<pin name="GND" x="-10.16" y="-5.08" length="short" direction="pwr"/>
<text x="-7.62" y="7.874" size="1.778" layer="95" font="vector">&gt;Name</text>
<text x="-7.62" y="-7.874" size="1.778" layer="96" font="vector" align="top-left">&gt;Value</text>
</symbol>
<symbol name="BRM-2508">
<description>&lt;h3&gt;BRM-2508 IR Receiver Module&lt;/h3&gt;
&lt;p&gt; 2.7V/5.5V IR Receiver with Low Power Consumption, High-immunity Against Ambient Light.&lt;/p&gt;</description>
<wire x1="5.08" y1="5.08" x2="-5.08" y2="5.08" width="0.254" layer="94"/>
<wire x1="-5.08" y1="5.08" x2="-5.08" y2="-5.08" width="0.254" layer="94"/>
<wire x1="-5.08" y1="-5.08" x2="5.08" y2="-5.08" width="0.254" layer="94"/>
<wire x1="5.08" y1="-5.08" x2="5.08" y2="5.08" width="0.254" layer="94"/>
<pin name="VCC" x="7.62" y="-2.54" length="short" rot="R180"/>
<pin name="GND" x="7.62" y="0" length="short" rot="R180"/>
<pin name="OUT" x="7.62" y="2.54" length="short" rot="R180"/>
<text x="-5.08" y="5.334" size="1.778" layer="95" font="vector">&gt;Name</text>
<text x="-5.08" y="-5.334" size="1.778" layer="96" font="vector" align="top-left">&gt;Value</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="DS18B20" prefix="U">
<description>&lt;h3&gt;Dallas/Maxim DS18B20 1-Wire Temperature Sensor&lt;/h3&gt;
&lt;p&gt;The DS18B20 reports degrees C with 9 to 12-bit precision, -55C to 125C (+/-0.5C). Each sensor has a unique 64-Bit Serial number etched into it - allows for a huge number of sensors to be used on one data bus.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/245"&gt;One Wire Digital Temperature Sensor - DS18B20&lt;/a&gt; (SEN-00245)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="DS18B20" x="0" y="0"/>
</gates>
<devices>
<device name="" package="TO-92-AMMO">
<connects>
<connect gate="G$1" pin="DQ" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="STORE_ID" value="SEN-00245" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BRM-2508" prefix="D">
<description>&lt;h3&gt;BRM-2508 IR Receiver Module&lt;/h3&gt;
&lt;p&gt; 2.7V/5.5V IR Receiver with Low Power Consumption, High-immunity Against Ambient Light.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BRM-2508" x="0" y="0"/>
</gates>
<devices>
<device name="RA" package="BRM-2508">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12059"/>
</technology>
</technologies>
</device>
<device name="VERT" package="BRM-2508_VERT">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12059"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<classes>
<class number="0" name="default" width="0" drill="0">
<clearance class="0" value="0.205"/>
</class>
</classes>
<parts>
<part name="U$1" library="diy-modules" deviceset="DC-DC-STEP-DOWN-LM2596" device=""/>
<part name="U$2" library="diy-modules" deviceset="BATTERY-CHARGER-LI-PROT" device=""/>
<part name="SOLAR_PANEL" library="SparkFun-Connectors" deviceset="CONN_02" device="LOCK_LONGPADS"/>
<part name="GND1" library="SparkFun-PowerSymbols" deviceset="GND" device=""/>
<part name="GND3" library="SparkFun-PowerSymbols" deviceset="GND" device=""/>
<part name="SX1276-RF" library="diy-modules" deviceset="WIRELESS-LORA-RFM95W" device="#THT"/>
<part name="SUPPLY3" library="SparkFun-PowerSymbols" deviceset="VCC" device=""/>
<part name="BATTERY" library="BK-18650-PC2" deviceset="BK-18650-PC2" device=""/>
<part name="S1" library="switch_dip" deviceset="418117270901" device=""/>
<part name="S2" library="switch_dip" deviceset="418117270901" device=""/>
<part name="PIC16F18426" library="pic16f6xx_14pin" deviceset="PIC16F8*" device="DIL"/>
<part name="DS18B20" library="SparkFun-Sensors" deviceset="DS18B20" device=""/>
<part name="CAPACITIVE_SENSOR" library="SparkFun-Sensors" deviceset="BRM-2508" device="RA"/>
<part name="MAX44009" library="diy-modules" deviceset="TEMP-HUM-SENSOR-HTU21D" device=""/>
<part name="SHT30" library="diy-modules" deviceset="TEMP-HUM-SENSOR-HTU21D" device=""/>
<part name="SUPPLY1" library="SparkFun-PowerSymbols" deviceset="VCC" device=""/>
<part name="R1" library="SparkFun-Resistors" deviceset="4.7KOHM" device="-0603-1/10W-1%" value="4.7k"/>
<part name="RGB-LED" library="SparkFun-LED" deviceset="LED-RGB-CC" device="DIFFUSE" value="DIFFUSE"/>
<part name="GND2" library="SparkFun-PowerSymbols" deviceset="GND" device=""/>
<part name="R2" library="SparkFun-Resistors" deviceset="10KOHM" device="-HORIZ-1/4W-1%" value="10k"/>
<part name="R3" library="SparkFun-Resistors" deviceset="10KOHM" device="-HORIZ-1/4W-1%" value="10k"/>
<part name="SUPPLY2" library="SparkFun-PowerSymbols" deviceset="VCC" device=""/>
<part name="GND4" library="SparkFun-PowerSymbols" deviceset="GND" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text x="-20.32" y="-27.94" size="2.54" layer="91">POWER SUPPLY MODULE</text>
<text x="-33.02" y="71.12" size="2.54" layer="91">MCU / TRANSMITTER / STATUS LED</text>
<text x="-20.32" y="22.86" size="2.54" layer="91">SENSING MODULE</text>
</plain>
<instances>
<instance part="U$1" gate="G$1" x="-7.62" y="-48.26" smashed="yes">
<attribute name="VALUE" x="-22.86" y="-35.56" size="1.778" layer="96"/>
</instance>
<instance part="U$2" gate="G$1" x="-45.72" y="-48.26" smashed="yes">
<attribute name="VALUE" x="-63.5" y="-35.56" size="1.778" layer="96"/>
</instance>
<instance part="SOLAR_PANEL" gate="G$1" x="-76.2" y="-48.26" smashed="yes">
<attribute name="VALUE" x="-78.74" y="-53.086" size="1.778" layer="96" font="vector"/>
<attribute name="NAME" x="-81.28" y="-42.672" size="1.778" layer="95" font="vector"/>
</instance>
<instance part="GND1" gate="1" x="-63.5" y="-17.78" smashed="yes">
<attribute name="VALUE" x="-63.5" y="-18.034" size="1.778" layer="96" align="top-center"/>
</instance>
<instance part="GND3" gate="1" x="-15.24" y="38.1" smashed="yes">
<attribute name="VALUE" x="-15.24" y="37.846" size="1.778" layer="96" align="top-center"/>
</instance>
<instance part="SX1276-RF" gate="G$1" x="7.62" y="53.34" smashed="yes" rot="MR180">
<attribute name="NAME" x="2.54" y="66.04" size="1.778" layer="95" rot="MR180"/>
</instance>
<instance part="SUPPLY3" gate="G$1" x="33.02" y="60.96" smashed="yes">
<attribute name="VALUE" x="33.02" y="63.754" size="1.778" layer="96" align="bottom-center"/>
</instance>
<instance part="BATTERY" gate="G$1" x="63.5" y="-33.02" smashed="yes">
<attribute name="NAME" x="58.41506875" y="-27.29945" size="1.67803125" layer="95"/>
</instance>
<instance part="S1" gate="G$1" x="43.18" y="-43.18" smashed="yes">
<attribute name="NAME" x="40.64" y="-48.26" size="1.778" layer="95" rot="R90"/>
<attribute name="VALUE" x="47.625" y="-48.26" size="1.778" layer="96" rot="R90"/>
</instance>
<instance part="S2" gate="G$1" x="27.94" y="-43.18" smashed="yes" rot="R180">
<attribute name="NAME" x="30.48" y="-38.1" size="1.778" layer="95" rot="R270"/>
<attribute name="VALUE" x="23.495" y="-35.56" size="1.778" layer="96" rot="R270"/>
</instance>
<instance part="PIC16F18426" gate="G$1" x="-58.42" y="50.8" smashed="yes">
<attribute name="NAME" x="-60.96" y="69.85" size="1.778" layer="95"/>
</instance>
<instance part="DS18B20" gate="G$1" x="30.48" y="7.62" smashed="yes">
<attribute name="NAME" x="22.86" y="18.034" size="1.778" layer="95" font="vector"/>
<attribute name="VALUE" x="22.86" y="-0.254" size="1.778" layer="96" font="vector" align="top-left"/>
</instance>
<instance part="CAPACITIVE_SENSOR" gate="G$1" x="63.5" y="10.16" smashed="yes" rot="R180">
<attribute name="NAME" x="73.66" y="20.066" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="MAX44009" gate="G$1" x="-10.16" y="5.08" smashed="yes">
<attribute name="NAME" x="-17.78" y="17.78" size="1.778" layer="95"/>
</instance>
<instance part="SHT30" gate="G$1" x="-45.72" y="5.08" smashed="yes">
<attribute name="NAME" x="-50.8" y="17.78" size="1.778" layer="95"/>
</instance>
<instance part="SUPPLY1" gate="G$1" x="-66.04" y="17.78" smashed="yes">
<attribute name="VALUE" x="-66.04" y="20.574" size="1.778" layer="96" align="bottom-center"/>
</instance>
<instance part="R1" gate="G$1" x="7.62" y="7.62" smashed="yes">
<attribute name="NAME" x="7.62" y="9.144" size="1.778" layer="95" font="vector" align="bottom-center"/>
<attribute name="VALUE" x="7.62" y="6.096" size="1.778" layer="96" font="vector" align="top-center"/>
</instance>
<instance part="RGB-LED" gate="G$1" x="55.88" y="53.34" smashed="yes">
<attribute name="NAME" x="53.34" y="58.7375" size="1.778" layer="95" font="vector"/>
</instance>
<instance part="GND2" gate="1" x="71.12" y="48.26" smashed="yes">
<attribute name="VALUE" x="71.12" y="48.006" size="1.778" layer="96" align="top-center"/>
</instance>
<instance part="R2" gate="G$1" x="50.8" y="-7.62" smashed="yes">
<attribute name="NAME" x="50.8" y="-6.096" size="1.778" layer="95" font="vector" align="bottom-center"/>
<attribute name="VALUE" x="50.8" y="-9.144" size="1.778" layer="96" font="vector" align="top-center"/>
</instance>
<instance part="R3" gate="G$1" x="66.04" y="-7.62" smashed="yes">
<attribute name="NAME" x="66.04" y="-6.096" size="1.778" layer="95" font="vector" align="bottom-center"/>
<attribute name="VALUE" x="66.04" y="-9.144" size="1.778" layer="96" font="vector" align="top-center"/>
</instance>
<instance part="SUPPLY2" gate="G$1" x="45.72" y="-2.54" smashed="yes">
<attribute name="VALUE" x="45.72" y="0.254" size="1.778" layer="96" align="bottom-center"/>
</instance>
<instance part="GND4" gate="1" x="71.12" y="-15.24" smashed="yes">
<attribute name="VALUE" x="71.12" y="-15.494" size="1.778" layer="96" align="top-center"/>
</instance>
</instances>
<busses>
</busses>
<nets>
<net name="VCC" class="0">
<segment>
<pinref part="SX1276-RF" gate="G$1" pin="3.3V"/>
<wire x1="25.4" y1="50.8" x2="33.02" y2="50.8" width="0.1524" layer="91"/>
<wire x1="33.02" y1="50.8" x2="33.02" y2="60.96" width="0.1524" layer="91"/>
<pinref part="SUPPLY3" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="S2" gate="G$1" pin="1"/>
<wire x1="27.94" y1="-30.48" x2="27.94" y2="-27.94" width="0.1524" layer="91"/>
<wire x1="27.94" y1="-27.94" x2="30.48" y2="-27.94" width="0.1524" layer="91"/>
<label x="30.48" y="-27.94" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="VDD"/>
<wire x1="-71.12" y1="66.04" x2="-73.66" y2="66.04" width="0.1524" layer="91"/>
<label x="-73.66" y="66.04" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="SHT30" gate="G$1" pin="VIN"/>
<wire x1="-60.96" y1="10.16" x2="-66.04" y2="10.16" width="0.1524" layer="91"/>
<pinref part="SUPPLY1" gate="G$1" pin="VCC"/>
<wire x1="-66.04" y1="10.16" x2="-66.04" y2="17.78" width="0.1524" layer="91"/>
<wire x1="-66.04" y1="10.16" x2="-66.04" y2="-5.08" width="0.1524" layer="91"/>
<junction x="-66.04" y="10.16"/>
<wire x1="-66.04" y1="-5.08" x2="-35.56" y2="-5.08" width="0.1524" layer="91"/>
<pinref part="MAX44009" gate="G$1" pin="VIN"/>
<wire x1="-35.56" y1="-5.08" x2="-35.56" y2="10.16" width="0.1524" layer="91"/>
<wire x1="-35.56" y1="10.16" x2="-25.4" y2="10.16" width="0.1524" layer="91"/>
<wire x1="-35.56" y1="-5.08" x2="0" y2="-5.08" width="0.1524" layer="91"/>
<junction x="-35.56" y="-5.08"/>
<pinref part="R1" gate="G$1" pin="1"/>
<wire x1="0" y1="7.62" x2="2.54" y2="7.62" width="0.1524" layer="91"/>
<wire x1="0" y1="-5.08" x2="0" y2="7.62" width="0.1524" layer="91"/>
<wire x1="0" y1="-5.08" x2="38.1" y2="-5.08" width="0.1524" layer="91"/>
<junction x="0" y="-5.08"/>
<pinref part="CAPACITIVE_SENSOR" gate="G$1" pin="VCC"/>
<wire x1="38.1" y1="12.7" x2="55.88" y2="12.7" width="0.1524" layer="91"/>
<wire x1="38.1" y1="12.7" x2="38.1" y2="-5.08" width="0.1524" layer="91"/>
<pinref part="DS18B20" gate="G$1" pin="VDD"/>
<wire x1="20.32" y1="12.7" x2="0" y2="12.7" width="0.1524" layer="91"/>
<wire x1="0" y1="12.7" x2="0" y2="7.62" width="0.1524" layer="91"/>
<junction x="0" y="7.62"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<wire x1="45.72" y1="-7.62" x2="45.72" y2="-2.54" width="0.1524" layer="91"/>
<pinref part="SUPPLY2" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="GND" class="0">
<segment>
<wire x1="-15.24" y1="40.64" x2="-15.24" y2="43.18" width="0.1524" layer="91"/>
<wire x1="-15.24" y1="43.18" x2="-15.24" y2="60.96" width="0.1524" layer="91"/>
<wire x1="-15.24" y1="60.96" x2="-10.16" y2="60.96" width="0.1524" layer="91"/>
<pinref part="GND3" gate="1" pin="GND"/>
<wire x1="-10.16" y1="43.18" x2="-15.24" y2="43.18" width="0.1524" layer="91"/>
<junction x="-15.24" y="43.18"/>
<pinref part="SX1276-RF" gate="G$1" pin="GND.1"/>
<pinref part="SX1276-RF" gate="G$1" pin="GND.2"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="OUT-"/>
<wire x1="10.16" y1="-53.34" x2="12.7" y2="-53.34" width="0.1524" layer="91"/>
<label x="12.7" y="-53.34" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="VSS"/>
<wire x1="-71.12" y1="35.56" x2="-73.66" y2="35.56" width="0.1524" layer="91"/>
<label x="-73.66" y="35.56" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="SHT30" gate="G$1" pin="GND"/>
<wire x1="-60.96" y1="7.62" x2="-63.5" y2="7.62" width="0.1524" layer="91"/>
<wire x1="-63.5" y1="7.62" x2="-63.5" y2="-7.62" width="0.1524" layer="91"/>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="MAX44009" gate="G$1" pin="GND"/>
<wire x1="-63.5" y1="-7.62" x2="-63.5" y2="-15.24" width="0.1524" layer="91"/>
<wire x1="-25.4" y1="7.62" x2="-33.02" y2="7.62" width="0.1524" layer="91"/>
<wire x1="-33.02" y1="7.62" x2="-33.02" y2="-7.62" width="0.1524" layer="91"/>
<wire x1="-33.02" y1="-7.62" x2="-63.5" y2="-7.62" width="0.1524" layer="91"/>
<junction x="-63.5" y="-7.62"/>
<wire x1="-33.02" y1="-7.62" x2="17.78" y2="-7.62" width="0.1524" layer="91"/>
<junction x="-33.02" y="-7.62"/>
<wire x1="17.78" y1="-7.62" x2="40.64" y2="-7.62" width="0.1524" layer="91"/>
<wire x1="40.64" y1="-7.62" x2="40.64" y2="10.16" width="0.1524" layer="91"/>
<pinref part="CAPACITIVE_SENSOR" gate="G$1" pin="GND"/>
<wire x1="40.64" y1="10.16" x2="55.88" y2="10.16" width="0.1524" layer="91"/>
<pinref part="DS18B20" gate="G$1" pin="GND"/>
<wire x1="20.32" y1="2.54" x2="17.78" y2="2.54" width="0.1524" layer="91"/>
<wire x1="17.78" y1="2.54" x2="17.78" y2="-7.62" width="0.1524" layer="91"/>
<junction x="17.78" y="-7.62"/>
</segment>
<segment>
<pinref part="RGB-LED" gate="G$1" pin="C"/>
<wire x1="68.58" y1="53.34" x2="71.12" y2="53.34" width="0.1524" layer="91"/>
<wire x1="71.12" y1="53.34" x2="71.12" y2="50.8" width="0.1524" layer="91"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
</net>
<net name="N$2" class="0">
<segment>
<pinref part="SOLAR_PANEL" gate="G$1" pin="1"/>
<wire x1="-68.58" y1="-48.26" x2="-66.04" y2="-48.26" width="0.1524" layer="91"/>
<wire x1="-66.04" y1="-48.26" x2="-66.04" y2="-55.88" width="0.1524" layer="91"/>
<pinref part="U$2" gate="G$1" pin="IN-"/>
<wire x1="-66.04" y1="-55.88" x2="-63.5" y2="-55.88" width="0.1524" layer="91"/>
</segment>
</net>
<net name="N$8" class="0">
<segment>
<wire x1="-83.82" y1="-22.86" x2="76.2" y2="-22.86" width="0.1524" layer="91" style="longdash"/>
<wire x1="76.2" y1="-22.86" x2="76.2" y2="-66.04" width="0.1524" layer="91" style="longdash"/>
<wire x1="76.2" y1="-66.04" x2="-83.82" y2="-66.04" width="0.1524" layer="91" style="longdash"/>
<wire x1="-83.82" y1="-66.04" x2="-83.82" y2="-22.86" width="0.1524" layer="91" style="longdash"/>
</segment>
</net>
<net name="N$9" class="0">
<segment>
<wire x1="-66.04" y1="-40.64" x2="-66.04" y2="-45.72" width="0.1524" layer="91"/>
<pinref part="SOLAR_PANEL" gate="G$1" pin="2"/>
<wire x1="-66.04" y1="-45.72" x2="-68.58" y2="-45.72" width="0.1524" layer="91"/>
<pinref part="U$2" gate="G$1" pin="IN+"/>
<wire x1="-63.5" y1="-40.64" x2="-66.04" y2="-40.64" width="0.1524" layer="91"/>
</segment>
</net>
<net name="N$1" class="0">
<segment>
<pinref part="U$1" gate="G$1" pin="IN+"/>
<wire x1="-25.4" y1="-43.18" x2="-25.4" y2="-40.64" width="0.1524" layer="91"/>
<pinref part="U$2" gate="G$1" pin="OUT+"/>
<wire x1="-25.4" y1="-40.64" x2="-30.48" y2="-40.64" width="0.1524" layer="91"/>
</segment>
</net>
<net name="N$6" class="0">
<segment>
<pinref part="U$2" gate="G$1" pin="OUT-"/>
<wire x1="-30.48" y1="-55.88" x2="-25.4" y2="-55.88" width="0.1524" layer="91"/>
<pinref part="U$1" gate="G$1" pin="IN-"/>
<wire x1="-25.4" y1="-55.88" x2="-25.4" y2="-53.34" width="0.1524" layer="91"/>
</segment>
</net>
<net name="RA4" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="OSC2/RA4"/>
<wire x1="-71.12" y1="48.26" x2="-73.66" y2="48.26" width="0.1524" layer="91"/>
<label x="-73.66" y="48.26" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="SX1276-RF" gate="G$1" pin="RST"/>
<wire x1="-10.16" y1="55.88" x2="-17.78" y2="55.88" width="0.1524" layer="91"/>
<label x="-17.78" y="55.88" size="1.016" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RA3" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="MCLR/RA3"/>
<wire x1="-71.12" y1="45.72" x2="-73.66" y2="45.72" width="0.1524" layer="91"/>
<label x="-73.66" y="45.72" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="SX1276-RF" gate="G$1" pin="MISO"/>
<wire x1="-10.16" y1="45.72" x2="-17.78" y2="45.72" width="0.1524" layer="91"/>
<label x="-17.78" y="45.72" size="1.016" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RC5" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RC5"/>
<wire x1="-38.1" y1="66.04" x2="-35.56" y2="66.04" width="0.1524" layer="91"/>
<label x="-35.56" y="66.04" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="SX1276-RF" gate="G$1" pin="MOSI"/>
<wire x1="-10.16" y1="48.26" x2="-17.78" y2="48.26" width="0.1524" layer="91"/>
<label x="-17.78" y="48.26" size="1.016" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="SX1276-RF" gate="G$1" pin="NSS"/>
<wire x1="-10.16" y1="53.34" x2="-17.78" y2="53.34" width="0.1524" layer="91"/>
<label x="-17.78" y="53.34" size="1.016" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RC4" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RC4"/>
<wire x1="-38.1" y1="63.5" x2="-35.56" y2="63.5" width="0.1524" layer="91"/>
<label x="-35.56" y="63.5" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="SX1276-RF" gate="G$1" pin="SCK"/>
<wire x1="-10.16" y1="50.8" x2="-17.78" y2="50.8" width="0.1524" layer="91"/>
<label x="-17.78" y="50.8" size="1.016" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RC3" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RC3/AN7"/>
<wire x1="-38.1" y1="60.96" x2="-35.56" y2="60.96" width="0.1524" layer="91"/>
<label x="-35.56" y="60.96" size="1.27" layer="95" xref="yes"/>
</segment>
</net>
<net name="RA0" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RA0/AN0"/>
<wire x1="-38.1" y1="38.1" x2="-35.56" y2="38.1" width="0.1524" layer="91"/>
<label x="-35.56" y="38.1" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="SHT30" gate="G$1" pin="SDA"/>
<wire x1="-60.96" y1="2.54" x2="-71.12" y2="2.54" width="0.1524" layer="91"/>
<pinref part="MAX44009" gate="G$1" pin="SDA"/>
<wire x1="-25.4" y1="2.54" x2="-27.94" y2="2.54" width="0.1524" layer="91"/>
<wire x1="-27.94" y1="2.54" x2="-27.94" y2="-12.7" width="0.1524" layer="91"/>
<wire x1="-27.94" y1="-12.7" x2="-71.12" y2="-12.7" width="0.1524" layer="91"/>
<wire x1="-71.12" y1="-12.7" x2="-71.12" y2="2.54" width="0.1524" layer="91"/>
<wire x1="-71.12" y1="2.54" x2="-73.66" y2="2.54" width="0.1524" layer="91"/>
<junction x="-71.12" y="2.54"/>
<label x="-73.66" y="2.54" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RA1" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RA1/AN1"/>
<wire x1="-38.1" y1="40.64" x2="-35.56" y2="40.64" width="0.1524" layer="91"/>
<label x="-35.56" y="40.64" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="SHT30" gate="G$1" pin="SCL"/>
<wire x1="-60.96" y1="5.08" x2="-68.58" y2="5.08" width="0.1524" layer="91"/>
<wire x1="-68.58" y1="5.08" x2="-68.58" y2="-10.16" width="0.1524" layer="91"/>
<junction x="-68.58" y="5.08"/>
<wire x1="-68.58" y1="-10.16" x2="-30.48" y2="-10.16" width="0.1524" layer="91"/>
<wire x1="-30.48" y1="-10.16" x2="-30.48" y2="5.08" width="0.1524" layer="91"/>
<pinref part="MAX44009" gate="G$1" pin="SCL"/>
<wire x1="-30.48" y1="5.08" x2="-25.4" y2="5.08" width="0.1524" layer="91"/>
<wire x1="-68.58" y1="5.08" x2="-73.66" y2="5.08" width="0.1524" layer="91"/>
<label x="-73.66" y="5.08" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RA2" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RA2/AN2"/>
<wire x1="-38.1" y1="43.18" x2="-35.56" y2="43.18" width="0.1524" layer="91"/>
<label x="-35.56" y="43.18" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="DS18B20" gate="G$1" pin="DQ"/>
<wire x1="20.32" y1="7.62" x2="15.24" y2="7.62" width="0.1524" layer="91"/>
<pinref part="R1" gate="G$1" pin="2"/>
<wire x1="15.24" y1="7.62" x2="12.7" y2="7.62" width="0.1524" layer="91"/>
<wire x1="15.24" y1="7.62" x2="15.24" y2="0" width="0.1524" layer="91"/>
<junction x="15.24" y="7.62"/>
<wire x1="15.24" y1="0" x2="12.7" y2="0" width="0.1524" layer="91"/>
<label x="12.7" y="0" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RC0" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RC0/AN4"/>
<wire x1="-38.1" y1="53.34" x2="-35.56" y2="53.34" width="0.1524" layer="91"/>
<label x="-35.56" y="53.34" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="CAPACITIVE_SENSOR" gate="G$1" pin="OUT"/>
<wire x1="55.88" y1="7.62" x2="50.8" y2="7.62" width="0.1524" layer="91"/>
<label x="50.8" y="7.62" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RC1" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RC1/AN5"/>
<wire x1="-38.1" y1="55.88" x2="-35.56" y2="55.88" width="0.1524" layer="91"/>
<label x="-35.56" y="55.88" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="RGB-LED" gate="G$1" pin="BLU"/>
<wire x1="45.72" y1="53.34" x2="43.18" y2="53.34" width="0.1524" layer="91"/>
<label x="43.18" y="53.34" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RC2" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="RC2/AN6"/>
<wire x1="-38.1" y1="58.42" x2="-35.56" y2="58.42" width="0.1524" layer="91"/>
<label x="-35.56" y="58.42" size="1.27" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="RGB-LED" gate="G$1" pin="RED"/>
<wire x1="45.72" y1="55.88" x2="43.18" y2="55.88" width="0.1524" layer="91"/>
<label x="43.18" y="55.88" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="RA5" class="0">
<segment>
<pinref part="PIC16F18426" gate="G$1" pin="OSC1/RA5"/>
<wire x1="-71.12" y1="50.8" x2="-73.66" y2="50.8" width="0.1524" layer="91"/>
<label x="-73.66" y="50.8" size="1.27" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="R3" gate="G$1" pin="1"/>
<wire x1="55.88" y1="-7.62" x2="58.42" y2="-7.62" width="0.1524" layer="91"/>
<wire x1="58.42" y1="-7.62" x2="60.96" y2="-7.62" width="0.1524" layer="91"/>
<wire x1="58.42" y1="-7.62" x2="58.42" y2="0" width="0.1524" layer="91"/>
<junction x="58.42" y="-7.62"/>
<wire x1="58.42" y1="0" x2="60.96" y2="0" width="0.1524" layer="91"/>
<label x="60.96" y="0" size="1.778" layer="95" xref="yes"/>
</segment>
</net>
<net name="SS" class="0">
<segment>
<pinref part="U$1" gate="G$1" pin="OUT+"/>
<label x="12.7" y="-43.18" size="1.778" layer="95" xref="yes"/>
<wire x1="12.7" y1="-43.18" x2="10.16" y2="-43.18" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="S2" gate="G$1" pin="A1"/>
<wire x1="27.94" y1="-55.88" x2="27.94" y2="-58.42" width="0.1524" layer="91"/>
<label x="27.94" y="-58.42" size="1.778" layer="95" rot="R270" xref="yes"/>
</segment>
</net>
<net name="B-" class="0">
<segment>
<pinref part="U$2" gate="G$1" pin="B-"/>
<wire x1="-30.48" y1="-50.8" x2="-27.94" y2="-50.8" width="0.1524" layer="91"/>
<label x="-27.94" y="-50.8" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="BATTERY" gate="G$1" pin="-"/>
<wire x1="53.34" y1="-35.56" x2="50.8" y2="-35.56" width="0.1524" layer="91"/>
<wire x1="50.8" y1="-35.56" x2="50.8" y2="-38.1" width="0.1524" layer="91"/>
<label x="50.8" y="-38.1" size="1.778" layer="95" rot="R270" xref="yes"/>
</segment>
</net>
<net name="SB" class="0">
<segment>
<pinref part="U$2" gate="G$1" pin="B+"/>
<wire x1="-30.48" y1="-45.72" x2="-27.94" y2="-45.72" width="0.1524" layer="91"/>
<label x="-27.94" y="-45.72" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="S1" gate="G$1" pin="1"/>
<wire x1="43.18" y1="-55.88" x2="43.18" y2="-58.42" width="0.1524" layer="91"/>
<label x="43.18" y="-58.42" size="1.778" layer="95" rot="R270" xref="yes"/>
</segment>
</net>
<net name="N$3" class="0">
<segment>
<pinref part="BATTERY" gate="G$1" pin="+"/>
<pinref part="S1" gate="G$1" pin="A1"/>
<wire x1="53.34" y1="-30.48" x2="43.18" y2="-30.48" width="0.1524" layer="91"/>
</segment>
</net>
<net name="N$5" class="0">
<segment>
<wire x1="-83.82" y1="27.94" x2="76.2" y2="27.94" width="0.1524" layer="91" style="longdash"/>
<wire x1="76.2" y1="27.94" x2="76.2" y2="-20.32" width="0.1524" layer="91" style="longdash"/>
<wire x1="76.2" y1="-20.32" x2="-83.82" y2="-20.32" width="0.1524" layer="91" style="longdash"/>
<wire x1="-83.82" y1="-20.32" x2="-83.82" y2="27.94" width="0.1524" layer="91" style="longdash"/>
</segment>
</net>
<net name="N$7" class="0">
<segment>
<wire x1="-83.82" y1="30.48" x2="76.2" y2="30.48" width="0.1524" layer="91" style="longdash"/>
<wire x1="76.2" y1="30.48" x2="76.2" y2="76.2" width="0.1524" layer="91" style="longdash"/>
<wire x1="76.2" y1="76.2" x2="-83.82" y2="76.2" width="0.1524" layer="91" style="longdash"/>
<wire x1="-83.82" y1="76.2" x2="-83.82" y2="30.48" width="0.1524" layer="91" style="longdash"/>
</segment>
</net>
<net name="N$11" class="0">
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
<wire x1="71.12" y1="-7.62" x2="71.12" y2="-12.7" width="0.1524" layer="91"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
