<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="50" unitdist="mil" unit="mil" style="lines" multiple="1" display="no" altdistance="5" altunitdist="mil" altunit="mil"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="2" name="Route2" color="16" fill="1" visible="no" active="no"/>
<layer number="3" name="Route3" color="17" fill="1" visible="no" active="no"/>
<layer number="4" name="Route4" color="18" fill="1" visible="no" active="no"/>
<layer number="5" name="Route5" color="19" fill="1" visible="no" active="no"/>
<layer number="6" name="Route6" color="25" fill="1" visible="no" active="no"/>
<layer number="7" name="Route7" color="26" fill="1" visible="no" active="no"/>
<layer number="8" name="Route8" color="27" fill="1" visible="no" active="no"/>
<layer number="9" name="Route9" color="28" fill="1" visible="no" active="no"/>
<layer number="10" name="Route10" color="29" fill="1" visible="no" active="no"/>
<layer number="11" name="Route11" color="30" fill="1" visible="no" active="no"/>
<layer number="12" name="Route12" color="20" fill="1" visible="no" active="no"/>
<layer number="13" name="Route13" color="21" fill="1" visible="no" active="no"/>
<layer number="14" name="Route14" color="22" fill="1" visible="no" active="no"/>
<layer number="15" name="Route15" color="23" fill="1" visible="no" active="no"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="24" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="50" name="dxf" color="7" fill="1" visible="no" active="no"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="no" active="no"/>
<layer number="57" name="tCAD" color="7" fill="1" visible="no" active="no"/>
<layer number="59" name="tCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="60" name="bCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="88" name="SimResults" color="9" fill="1" visible="no" active="no"/>
<layer number="89" name="SimProbes" color="9" fill="1" visible="no" active="no"/>
<layer number="90" name="Modules" color="5" fill="1" visible="no" active="no"/>
<layer number="91" name="Nets" color="2" fill="1" visible="no" active="no"/>
<layer number="92" name="Busses" color="1" fill="1" visible="no" active="no"/>
<layer number="93" name="Pins" color="2" fill="1" visible="no" active="no"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="no" active="no"/>
<layer number="95" name="Names" color="7" fill="1" visible="no" active="no"/>
<layer number="96" name="Values" color="7" fill="1" visible="no" active="no"/>
<layer number="97" name="Info" color="7" fill="1" visible="no" active="no"/>
<layer number="98" name="Guide" color="6" fill="1" visible="no" active="no"/>
<layer number="99" name="SpiceOrder" color="7" fill="1" visible="no" active="no"/>
<layer number="100" name="Muster" color="7" fill="1" visible="no" active="no"/>
<layer number="101" name="Patch_Top" color="12" fill="4" visible="no" active="no"/>
<layer number="102" name="Vscore" color="7" fill="1" visible="no" active="no"/>
<layer number="103" name="tMap" color="7" fill="1" visible="no" active="no"/>
<layer number="104" name="Name" color="16" fill="1" visible="no" active="no"/>
<layer number="105" name="tPlate" color="7" fill="1" visible="no" active="no"/>
<layer number="106" name="bPlate" color="7" fill="1" visible="no" active="no"/>
<layer number="107" name="Crop" color="7" fill="1" visible="no" active="no"/>
<layer number="108" name="tplace-old" color="10" fill="1" visible="no" active="no"/>
<layer number="109" name="ref-old" color="11" fill="1" visible="no" active="no"/>
<layer number="110" name="fp0" color="7" fill="1" visible="no" active="no"/>
<layer number="111" name="LPC17xx" color="7" fill="1" visible="no" active="no"/>
<layer number="112" name="tSilk" color="7" fill="1" visible="no" active="no"/>
<layer number="113" name="IDFDebug" color="4" fill="1" visible="no" active="no"/>
<layer number="114" name="Badge_Outline" color="7" fill="1" visible="no" active="no"/>
<layer number="115" name="ReferenceISLANDS" color="7" fill="1" visible="no" active="no"/>
<layer number="116" name="Patch_BOT" color="9" fill="4" visible="no" active="no"/>
<layer number="117" name="PM_Ref" color="7" fill="1" visible="yes" active="yes"/>
<layer number="118" name="Rect_Pads" color="7" fill="1" visible="no" active="no"/>
<layer number="119" name="PF_Ref" color="7" fill="1" visible="yes" active="yes"/>
<layer number="120" name="WFL_Ref" color="7" fill="1" visible="yes" active="yes"/>
<layer number="121" name="_tsilk" color="7" fill="1" visible="no" active="no"/>
<layer number="122" name="_bsilk" color="7" fill="1" visible="no" active="no"/>
<layer number="123" name="tTestmark" color="7" fill="1" visible="no" active="no"/>
<layer number="124" name="bTestmark" color="7" fill="1" visible="no" active="no"/>
<layer number="125" name="_tNames" color="7" fill="1" visible="no" active="no"/>
<layer number="126" name="_bNames" color="7" fill="1" visible="no" active="no"/>
<layer number="127" name="_tValues" color="7" fill="1" visible="no" active="no"/>
<layer number="128" name="_bValues" color="7" fill="1" visible="no" active="no"/>
<layer number="129" name="Mask" color="7" fill="1" visible="no" active="no"/>
<layer number="131" name="tAdjust" color="7" fill="1" visible="no" active="no"/>
<layer number="132" name="bAdjust" color="7" fill="1" visible="no" active="no"/>
<layer number="144" name="Drill_legend" color="7" fill="1" visible="no" active="no"/>
<layer number="150" name="Notes" color="7" fill="1" visible="no" active="no"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="no" active="no"/>
<layer number="152" name="_bDocu" color="7" fill="1" visible="no" active="no"/>
<layer number="153" name="FabDoc1" color="7" fill="1" visible="no" active="no"/>
<layer number="154" name="FabDoc2" color="7" fill="1" visible="no" active="no"/>
<layer number="155" name="FabDoc3" color="7" fill="1" visible="no" active="no"/>
<layer number="199" name="Contour" color="7" fill="1" visible="no" active="no"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="no" active="no"/>
<layer number="201" name="201bmp" color="2" fill="10" visible="no" active="no"/>
<layer number="202" name="202bmp" color="3" fill="10" visible="no" active="no"/>
<layer number="203" name="203bmp" color="4" fill="10" visible="no" active="no"/>
<layer number="204" name="204bmp" color="5" fill="10" visible="no" active="no"/>
<layer number="205" name="205bmp" color="6" fill="10" visible="no" active="no"/>
<layer number="206" name="206bmp" color="7" fill="10" visible="no" active="no"/>
<layer number="207" name="207bmp" color="8" fill="10" visible="no" active="no"/>
<layer number="208" name="208bmp" color="9" fill="10" visible="no" active="no"/>
<layer number="209" name="209bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="210" name="210bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="211" name="211bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="212" name="212bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="213" name="213bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="214" name="214bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="215" name="215bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="216" name="216bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="217" name="217bmp" color="18" fill="1" visible="no" active="no"/>
<layer number="218" name="218bmp" color="19" fill="1" visible="no" active="no"/>
<layer number="219" name="219bmp" color="20" fill="1" visible="no" active="no"/>
<layer number="220" name="220bmp" color="21" fill="1" visible="no" active="no"/>
<layer number="221" name="221bmp" color="22" fill="1" visible="no" active="no"/>
<layer number="222" name="222bmp" color="23" fill="1" visible="no" active="no"/>
<layer number="223" name="223bmp" color="24" fill="1" visible="no" active="no"/>
<layer number="224" name="224bmp" color="25" fill="1" visible="no" active="no"/>
<layer number="225" name="225bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="226" name="226bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="227" name="227bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="228" name="228bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="229" name="229bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="230" name="230bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="231" name="231bmp" color="7" fill="1" visible="no" active="no"/>
<layer number="232" name="Eagle3D_PG2" color="7" fill="1" visible="no" active="no"/>
<layer number="233" name="Eagle3D_PG3" color="7" fill="1" visible="no" active="no"/>
<layer number="248" name="Housing" color="7" fill="1" visible="no" active="no"/>
<layer number="249" name="Edge" color="7" fill="1" visible="no" active="no"/>
<layer number="250" name="Descript" color="3" fill="1" visible="no" active="no"/>
<layer number="251" name="SMDround" color="12" fill="11" visible="no" active="no"/>
<layer number="254" name="cooling" color="7" fill="1" visible="no" active="no"/>
<layer number="255" name="routoute" color="7" fill="1" visible="no" active="no"/>
</layers>
<board>
<plain>
<wire x1="-185.42" y1="-57.15" x2="-121.94" y2="-57.15" width="0" layer="20"/>
<wire x1="-121.94" y1="-57.15" x2="-121.94" y2="55.55" width="0" layer="20"/>
<wire x1="-121.94" y1="55.55" x2="-185.42" y2="55.55" width="0" layer="20"/>
<wire x1="-185.42" y1="55.55" x2="-185.42" y2="-57.15" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="11.43" y1="0.635" x2="11.43" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="0.635" x2="6.35" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.651" y1="0" x2="0.889" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.016" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.9906" x2="-0.9906" y2="1.27" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.9906" x2="-0.9906" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.556" y2="0" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.9906" x2="3.5306" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.9906" x2="3.5306" y2="1.27" width="0.2032" layer="21"/>
<pad name="1" x="-0.127" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.667" y="0" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="1.651" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
</packages>
</library>
<library name="diy-modules">
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.8.0 (2017-Jul-02)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;
&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://www.diymodules.org/img/diymodules-lbr-image.php?v=1.8.0" alt="DIYmodules.org"&gt;&lt;/a&gt;
&lt;/center&gt;</description>
<packages>
<package name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<wire x1="-21.59" y1="10.414" x2="21.59" y2="10.414" width="0.127" layer="21"/>
<wire x1="21.59" y1="10.414" x2="21.59" y2="-10.414" width="0.127" layer="21"/>
<wire x1="21.59" y1="-10.414" x2="-21.59" y2="-10.414" width="0.127" layer="21"/>
<wire x1="-21.59" y1="-10.414" x2="-21.59" y2="10.414" width="0.127" layer="21"/>
<pad name="IN+" x="-19.812" y="8.636" drill="1.5" diameter="2.5" shape="square"/>
<pad name="IN-" x="-19.812" y="-8.636" drill="1.5" diameter="2.5" shape="square"/>
<pad name="OUT-" x="19.812" y="-8.636" drill="1.5" diameter="2.5" shape="square"/>
<pad name="OUT+" x="19.812" y="8.636" drill="1.5" diameter="2.5" shape="square"/>
<hole x="-14.478" y="7.62" drill="3"/>
<hole x="15.24" y="-7.62" drill="3"/>
<text x="0" y="11.43" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-11.43" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<text x="-19.685" y="0" size="1.778" layer="21" rot="R90" align="center">IN</text>
<text x="19.685" y="0" size="1.778" layer="21" rot="R90" align="center">OUT</text>
<wire x1="19.685" y1="6.985" x2="19.685" y2="5.715" width="0.254" layer="21"/>
<wire x1="19.05" y1="6.35" x2="20.32" y2="6.35" width="0.254" layer="21"/>
<wire x1="-19.685" y1="-6.985" x2="-19.685" y2="-5.715" width="0.254" layer="21"/>
<wire x1="19.685" y1="-6.985" x2="19.685" y2="-5.715" width="0.254" layer="21"/>
<wire x1="-19.685" y1="6.985" x2="-19.685" y2="5.715" width="0.254" layer="21"/>
<wire x1="-20.32" y1="6.35" x2="-19.05" y2="6.35" width="0.254" layer="21"/>
</package>
<package name="BATTERY-CHARGER-LI-PROT">
<description>&lt;b&gt;Protected Lithium Battery 5V Charger&lt;/b&gt; with micro-USB connector</description>
<wire x1="-13.97" y1="8.636" x2="13.97" y2="8.636" width="0.127" layer="21"/>
<wire x1="13.97" y1="-8.636" x2="-13.97" y2="-8.636" width="0.127" layer="21"/>
<pad name="IN+" x="-12.065" y="6.985" drill="1.2" diameter="2.5" shape="square"/>
<pad name="IN-" x="-12.065" y="-6.985" drill="1.2" diameter="2.5" shape="square"/>
<pad name="B+" x="10.795" y="3.81" drill="1.2" diameter="2.5" shape="square"/>
<pad name="B-" x="10.795" y="-3.81" drill="1.2" diameter="2.5" shape="square"/>
<text x="-9.525" y="6.985" size="1.27" layer="21" align="center-left">IN+</text>
<text x="-9.525" y="-6.985" size="1.27" layer="21" align="center-left">IN-</text>
<text x="8.255" y="3.81" size="1.27" layer="21" align="center-right">B+</text>
<text x="8.255" y="-3.81" size="1.27" layer="21" align="center-right">B-</text>
<wire x1="-13.97" y1="8.636" x2="-13.97" y2="4.064" width="0.127" layer="21"/>
<wire x1="-13.97" y1="-8.636" x2="-13.97" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-14.605" y1="4.064" x2="-13.97" y2="4.064" width="0.127" layer="21"/>
<wire x1="-14.605" y1="-4.064" x2="-13.97" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-13.97" y1="-4.064" x2="-8.128" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-14.605" y1="4.064" x2="-14.605" y2="-4.064" width="0.127" layer="21"/>
<wire x1="-8.128" y1="4.064" x2="-8.128" y2="-4.064" width="0.127" layer="21"/>
<text x="-11.43" y="0" size="1.778" layer="21" align="center">USB</text>
<text x="0" y="10.16" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-10.16" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<wire x1="13.97" y1="8.636" x2="13.97" y2="6.35" width="0.127" layer="21"/>
<wire x1="13.97" y1="6.35" x2="12.7" y2="6.35" width="0.127" layer="21"/>
<wire x1="12.7" y1="6.35" x2="12.7" y2="-6.35" width="0.127" layer="21"/>
<wire x1="12.7" y1="-6.35" x2="13.97" y2="-6.35" width="0.127" layer="21"/>
<wire x1="13.97" y1="-6.35" x2="13.97" y2="-8.636" width="0.127" layer="21"/>
<pad name="OUT+" x="10.795" y="6.985" drill="1.2" diameter="2.5" shape="square"/>
<pad name="OUT-" x="10.795" y="-6.985" drill="1.2" diameter="2.5" shape="square"/>
<wire x1="-13.97" y1="4.064" x2="-8.128" y2="4.064" width="0.127" layer="21"/>
<text x="8.255" y="6.985" size="1.27" layer="21" align="center-right">OUT+</text>
<text x="8.255" y="-6.985" size="1.27" layer="21" align="center-right">OUT-</text>
</package>
<package name="WIRELESS-LORA-RFM95W#THT">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt;&lt;br /&gt;
Footprint for THT assembly.</description>
<wire x1="-8" y1="8" x2="8" y2="8" width="0.127" layer="21"/>
<wire x1="8" y1="-8" x2="-8" y2="-8" width="0.127" layer="21"/>
<pad name="A1" x="-6.5" y="7" drill="0.8"/>
<text x="0" y="9.525" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-9.525" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
<text x="-5" y="7" size="1.016" layer="21" align="center-left">GND</text>
<wire x1="-8" y1="8" x2="-8" y2="-8" width="0.127" layer="21"/>
<wire x1="8" y1="-8" x2="8" y2="8" width="0.127" layer="21"/>
<pad name="A2" x="-6.5" y="5" drill="0.8"/>
<pad name="A3" x="-6.5" y="3" drill="0.8"/>
<pad name="A4" x="-6.5" y="1" drill="0.8"/>
<pad name="A5" x="-6.5" y="-1" drill="0.8"/>
<pad name="A6" x="-6.5" y="-3" drill="0.8"/>
<pad name="A7" x="-6.5" y="-5" drill="0.8"/>
<pad name="A8" x="-6.5" y="-7" drill="0.8"/>
<text x="-5" y="5" size="1.016" layer="21" align="center-left">MISO</text>
<text x="-5" y="3" size="1.016" layer="21" align="center-left">MOSI</text>
<text x="-5" y="1" size="1.016" layer="21" align="center-left">SCK</text>
<text x="-5" y="-1" size="1.016" layer="21" align="center-left">NSS</text>
<text x="-5" y="-3" size="1.016" layer="21" align="center-left">RST</text>
<text x="-5" y="-5" size="1.016" layer="21" align="center-left">DIO5</text>
<text x="-5" y="-7" size="1.016" layer="21" align="center-left">GND</text>
<pad name="B1" x="6.5" y="7" drill="0.8"/>
<pad name="B2" x="6.5" y="5" drill="0.8"/>
<pad name="B3" x="6.5" y="3" drill="0.8"/>
<pad name="B4" x="6.5" y="1" drill="0.8"/>
<pad name="B5" x="6.5" y="-1" drill="0.8"/>
<pad name="B6" x="6.5" y="-3" drill="0.8"/>
<pad name="B7" x="6.5" y="-5" drill="0.8"/>
<pad name="B8" x="6.5" y="-7" drill="0.8"/>
<text x="5" y="7" size="1.016" layer="21" align="center-right">DIO2</text>
<text x="5" y="5" size="1.016" layer="21" align="center-right">DIO1</text>
<text x="5" y="3" size="1.016" layer="21" align="center-right">DIO0</text>
<text x="5" y="1" size="1.016" layer="21" align="center-right">3.3V</text>
<text x="5" y="-1" size="1.016" layer="21" align="center-right">DIO4</text>
<text x="5" y="-3" size="1.016" layer="21" align="center-right">DIO3</text>
<text x="5" y="-5" size="1.016" layer="21" align="center-right">GND</text>
<text x="5" y="-7" size="1.016" layer="21" align="center-right">ANT</text>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
<wire x1="-2.54" y1="0.762" x2="2.54" y2="0.762" width="0.2032" layer="21"/>
<wire x1="2.54" y1="0.762" x2="2.54" y2="0" width="0.2032" layer="21"/>
<wire x1="2.54" y1="0" x2="2.54" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="2.54" y1="-0.762" x2="-2.54" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="-0.762" x2="-2.54" y2="0" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="0" x2="-2.54" y2="0.762" width="0.2032" layer="21"/>
<wire x1="2.54" y1="0" x2="2.794" y2="0" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="0" x2="-2.794" y2="0" width="0.2032" layer="21"/>
<pad name="P$1" x="-3.81" y="0" drill="0.9" diameter="1.8796"/>
<pad name="P$2" x="3.81" y="0" drill="0.9" diameter="1.8796"/>
<text x="0" y="1.016" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-1.016" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
</packages>
</library>
<library name="BK-18650-PC2">
<packages>
<package name="MPD_BK-18650-PC2">
<wire x1="-36.94" y1="-0.03" x2="-36.94" y2="0.08" width="0" layer="46"/>
<wire x1="-36.94" y1="1.2" x2="-35.56" y2="1.2" width="0" layer="46"/>
<wire x1="-35.56" y1="1.2" x2="-35.56" y2="-1.2" width="0" layer="46"/>
<wire x1="-35.56" y1="-1.2" x2="-36.94" y2="-1.2" width="0" layer="46"/>
<wire x1="-36.94" y1="-1.2" x2="-36.94" y2="1.2" width="0" layer="46"/>
<wire x1="35.56" y1="0.03" x2="35.56" y2="0.14" width="0" layer="46"/>
<wire x1="35.56" y1="1.2" x2="36.94" y2="1.2" width="0" layer="46"/>
<wire x1="36.94" y1="1.2" x2="36.94" y2="-1.2" width="0" layer="46"/>
<wire x1="36.94" y1="-1.2" x2="35.56" y2="-1.2" width="0" layer="46"/>
<wire x1="35.56" y1="-1.2" x2="35.56" y2="1.2" width="0" layer="46"/>
<wire x1="-38.48" y1="-10.49" x2="-38.48" y2="10.49" width="0.127" layer="51"/>
<wire x1="-38.48" y1="10.49" x2="38.48" y2="10.49" width="0.127" layer="51"/>
<wire x1="38.48" y1="10.49" x2="38.48" y2="-10.49" width="0.127" layer="51"/>
<wire x1="38.48" y1="-10.49" x2="-38.48" y2="-10.49" width="0.127" layer="51"/>
<wire x1="-38.48" y1="10.49" x2="38.48" y2="10.49" width="0.127" layer="21"/>
<wire x1="38.48" y1="10.49" x2="38.48" y2="-10.49" width="0.127" layer="21"/>
<wire x1="38.48" y1="-10.49" x2="-38.48" y2="-10.49" width="0.127" layer="21"/>
<wire x1="-38.48" y1="-10.49" x2="-38.48" y2="10.49" width="0.127" layer="21"/>
<wire x1="-38.73" y1="-10.74" x2="-38.73" y2="10.74" width="0.05" layer="39"/>
<wire x1="-38.73" y1="10.74" x2="38.73" y2="10.74" width="0.05" layer="39"/>
<wire x1="38.73" y1="10.74" x2="38.73" y2="-10.74" width="0.05" layer="39"/>
<wire x1="38.73" y1="-10.74" x2="-38.73" y2="-10.74" width="0.05" layer="39"/>
<text x="-38.4734" y="11.6222" size="1.7814" layer="25">&gt;NAME</text>
<text x="-38.5653" y="-12.7215" size="1.781009375" layer="27">&gt;VALUE</text>
<text x="-40.4673" y="-0.9015" size="1.780959375" layer="21">+</text>
<text x="39.4562" y="-0.300428125" size="1.780540625" layer="21">-</text>
<hole x="27.805" y="0" drill="3.2"/>
<hole x="-27.805" y="0" drill="3.2"/>
<pad name="P" x="-36.25" y="0" drill="1.38" shape="long" rot="R90"/>
<pad name="M" x="36.25" y="0" drill="1.38" shape="long" rot="R90"/>
</package>
</packages>
</library>
<library name="switch_dip">
<packages>
<package name="418117270901">
<description>WS-BS 2.54 mm compact THT Dip Switch with raised actuator, 1 Pole</description>
<wire x1="-1.77" y1="4.8" x2="1.77" y2="4.8" width="0.127" layer="21"/>
<wire x1="1.77" y1="4.8" x2="1.77" y2="-4.8" width="0.127" layer="21"/>
<wire x1="1.77" y1="-4.8" x2="-1.77" y2="-4.8" width="0.127" layer="21"/>
<wire x1="-1.77" y1="-4.8" x2="-1.77" y2="4.8" width="0.127" layer="21"/>
<text x="-0.535" y="-2.545" size="1.27" layer="51">1</text>
<text x="0.11" y="5.67" size="0.8128" layer="25" align="bottom-center">&gt;NAME</text>
<text x="-2.19" y="-6.235" size="0.8128" layer="27">&gt;VALUE</text>
<polygon width="0.127" layer="39">
<vertex x="-2.02" y="5.05"/>
<vertex x="2.02" y="5.05"/>
<vertex x="2.02" y="-5.05"/>
<vertex x="-2.02" y="-5.05"/>
</polygon>
<circle x="-1" y="-4.5" radius="0.05" width="0.2" layer="21"/>
<pad name="1" x="0" y="-3.81" drill="0.8"/>
<pad name="A1" x="0" y="3.81" drill="0.8"/>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="WS2812B-PTH-KIT">
<wire x1="-3.175" y1="2.8575" x2="-3.175" y2="1.4605" width="0.254" layer="21"/>
<wire x1="-3.175" y1="1.4605" x2="-3.175" y2="-2.159" width="0.254" layer="21"/>
<wire x1="-3.175" y1="2.8575" x2="-3.175" y2="-2.159" width="0.254" layer="21" curve="-288.461981"/>
<wire x1="-3.175" y1="1.4605" x2="-3.1115" y2="-0.8255" width="0.254" layer="21" curve="-323.123915"/>
<wire x1="0.635" y1="-0.5715" x2="1.143" y2="-0.5715" width="0.127" layer="21"/>
<pad name="1" x="2.413" y="0.0794" drill="0.762" diameter="1.27" shape="offset" rot="R270" stop="no"/>
<pad name="2" x="0.889" y="0.6509" drill="0.762" diameter="1.27" shape="offset" rot="R90" stop="no"/>
<pad name="3" x="-0.635" y="0.0794" drill="0.762" diameter="1.27" shape="offset" rot="R270" stop="no"/>
<pad name="4" x="-2.159" y="0.6509" drill="0.762" diameter="1.27" shape="offset" rot="R90" stop="no"/>
<text x="-0.9398" y="0.9398" size="0.8128" layer="21">+</text>
<polygon width="0.2032" layer="30">
<vertex x="-2.7686" y="0.6604"/>
<vertex x="-2.7686" y="1.9558" curve="-90"/>
<vertex x="-2.2098" y="2.5146"/>
<vertex x="-2.159" y="2.5146" curve="-90"/>
<vertex x="-1.5494" y="1.905"/>
<vertex x="-1.5494" y="0.6604" curve="-90"/>
<vertex x="-2.159" y="0.0508" curve="-90"/>
</polygon>
<polygon width="0.2032" layer="30">
<vertex x="-1.2446" y="-1.1938"/>
<vertex x="-1.2446" y="0.1016" curve="-90"/>
<vertex x="-0.6858" y="0.6604"/>
<vertex x="-0.635" y="0.6604" curve="-90"/>
<vertex x="-0.0254" y="0.0508"/>
<vertex x="-0.0254" y="-1.1938" curve="-90"/>
<vertex x="-0.635" y="-1.8034" curve="-90"/>
</polygon>
<polygon width="0.2032" layer="30">
<vertex x="0.2794" y="0.6604"/>
<vertex x="0.2794" y="1.9558" curve="-90"/>
<vertex x="0.8382" y="2.5146"/>
<vertex x="0.889" y="2.5146" curve="-90"/>
<vertex x="1.4986" y="1.905"/>
<vertex x="1.4986" y="0.6604" curve="-90"/>
<vertex x="0.889" y="0.0508" curve="-90"/>
</polygon>
<polygon width="0.2032" layer="30">
<vertex x="1.8034" y="-1.1684"/>
<vertex x="1.8034" y="0.127" curve="-90"/>
<vertex x="2.3622" y="0.6858"/>
<vertex x="2.413" y="0.6858" curve="-90"/>
<vertex x="3.0226" y="0.0762"/>
<vertex x="3.0226" y="-1.1684" curve="-90"/>
<vertex x="2.413" y="-1.778" curve="-90"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-2.159" y="0.1905" curve="-90.012891"/>
<vertex x="-2.6035" y="0.6147" curve="-90"/>
<vertex x="-2.159" y="1.082" curve="-90"/>
<vertex x="-1.7171" y="0.6249" curve="-90.012967"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="0.889" y="0.1905" curve="-90.012891"/>
<vertex x="0.4445" y="0.6147" curve="-90"/>
<vertex x="0.889" y="1.082" curve="-90"/>
<vertex x="1.3309" y="0.6249" curve="-90.012967"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-0.635" y="-0.381" curve="-90.012891"/>
<vertex x="-1.0795" y="0.0432" curve="-90"/>
<vertex x="-0.635" y="0.5105" curve="-90"/>
<vertex x="-0.1931" y="0.0534" curve="-90.012967"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="2.413" y="-0.381" curve="-90.012891"/>
<vertex x="1.9685" y="0.0432" curve="-90"/>
<vertex x="2.413" y="0.5105" curve="-90"/>
<vertex x="2.8549" y="0.0534" curve="-90.012967"/>
</polygon>
<text x="0" y="5.334" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;NAME</text>
<text x="0" y="-4.445" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;VALUE</text>
</package>
</packages>
</library>
<library name="pic16f6xx_14pin">
<packages>
<package name="DIL14">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
<wire x1="-11.43" y1="-0.635" x2="-11.43" y2="-2.54" width="0.1524" layer="21"/>
<wire x1="-11.43" y1="-0.635" x2="-11.43" y2="0.635" width="0.1524" layer="21" curve="180"/>
<wire x1="6.35" y1="-2.54" x2="-11.43" y2="-2.54" width="0.1524" layer="21"/>
<wire x1="6.35" y1="-2.54" x2="6.35" y2="2.54" width="0.1524" layer="21"/>
<wire x1="-11.43" y1="2.54" x2="6.35" y2="2.54" width="0.1524" layer="21"/>
<wire x1="-11.43" y1="2.54" x2="-11.43" y2="0.635" width="0.1524" layer="21"/>
<pad name="1" x="-10.16" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="2" x="-7.62" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="3" x="-5.08" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="4" x="-2.54" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="5" x="0" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="6" x="2.54" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="7" x="5.08" y="-3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="8" x="5.08" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="9" x="2.54" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="10" x="0" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="11" x="-2.54" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="12" x="-5.08" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="13" x="-7.62" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<pad name="14" x="-10.16" y="3.81" drill="0.8128" shape="long" rot="R90"/>
<text x="-11.8618" y="-2.54" size="1.778" layer="25" ratio="10" rot="R90">&gt;NAME</text>
<text x="-10.16" y="-0.889" size="1.778" layer="27" ratio="10">&gt;VALUE</text>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<classes>
<class number="0" name="default" width="0" drill="0">
<clearance class="0" value="0.205"/>
</class>
</classes>
<designrules name="default">
<description language="de">&lt;b&gt;EAGLE Design Rules&lt;/b&gt;
&lt;p&gt;
Die Standard-Design-Rules sind so gewählt, dass sie für 
die meisten Anwendungen passen. Sollte ihre Platine 
besondere Anforderungen haben, treffen Sie die erforderlichen
Einstellungen hier und speichern die Design Rules unter 
einem neuen Namen ab.</description>
<description language="en">&lt;b&gt;EAGLE Design Rules&lt;/b&gt;
&lt;p&gt;
The default Design Rules have been set to cover
a wide range of applications. Your particular design
may have different requirements, so please make the
necessary adjustments and save your customized
design rules under a new name.</description>
<param name="layerSetup" value="(1*16)"/>
<param name="mtCopper" value="0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm"/>
<param name="mtIsolate" value="1.5mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm"/>
<param name="mdWireWire" value="6mil"/>
<param name="mdWirePad" value="6mil"/>
<param name="mdWireVia" value="6mil"/>
<param name="mdPadPad" value="6mil"/>
<param name="mdPadVia" value="6mil"/>
<param name="mdViaVia" value="6mil"/>
<param name="mdSmdPad" value="6mil"/>
<param name="mdSmdVia" value="6mil"/>
<param name="mdSmdSmd" value="6mil"/>
<param name="mdViaViaSameLayer" value="6mil"/>
<param name="mnLayersViaInSmd" value="2"/>
<param name="mdCopperDimension" value="40mil"/>
<param name="mdDrill" value="6mil"/>
<param name="mdSmdStop" value="0mil"/>
<param name="msWidth" value="6mil"/>
<param name="msDrill" value="0.35mm"/>
<param name="msMicroVia" value="9.99mm"/>
<param name="msBlindViaRatio" value="0.5"/>
<param name="rvPadTop" value="0.25"/>
<param name="rvPadInner" value="0.25"/>
<param name="rvPadBottom" value="0.25"/>
<param name="rvViaOuter" value="0.25"/>
<param name="rvViaInner" value="0.25"/>
<param name="rvMicroViaOuter" value="0.25"/>
<param name="rvMicroViaInner" value="0.25"/>
<param name="rlMinPadTop" value="10mil"/>
<param name="rlMaxPadTop" value="20mil"/>
<param name="rlMinPadInner" value="10mil"/>
<param name="rlMaxPadInner" value="20mil"/>
<param name="rlMinPadBottom" value="10mil"/>
<param name="rlMaxPadBottom" value="20mil"/>
<param name="rlMinViaOuter" value="8mil"/>
<param name="rlMaxViaOuter" value="20mil"/>
<param name="rlMinViaInner" value="8mil"/>
<param name="rlMaxViaInner" value="20mil"/>
<param name="rlMinMicroViaOuter" value="4mil"/>
<param name="rlMaxMicroViaOuter" value="20mil"/>
<param name="rlMinMicroViaInner" value="4mil"/>
<param name="rlMaxMicroViaInner" value="20mil"/>
<param name="psTop" value="-1"/>
<param name="psBottom" value="-1"/>
<param name="psFirst" value="-1"/>
<param name="psElongationLong" value="100"/>
<param name="psElongationOffset" value="100"/>
<param name="mvStopFrame" value="1"/>
<param name="mvCreamFrame" value="0"/>
<param name="mlMinStopFrame" value="4mil"/>
<param name="mlMaxStopFrame" value="4mil"/>
<param name="mlMinCreamFrame" value="0mil"/>
<param name="mlMaxCreamFrame" value="0mil"/>
<param name="mlViaStopLimit" value="0mil"/>
<param name="srRoundness" value="0"/>
<param name="srMinRoundness" value="0mil"/>
<param name="srMaxRoundness" value="0mil"/>
<param name="slThermalIsolate" value="10mil"/>
<param name="slThermalsForVias" value="0"/>
<param name="dpMaxLengthDifference" value="10mm"/>
<param name="dpGapFactor" value="2.5"/>
<param name="checkAngle" value="0"/>
<param name="checkFont" value="1"/>
<param name="checkRestrict" value="1"/>
<param name="checkStop" value="0"/>
<param name="checkValues" value="0"/>
<param name="checkNames" value="1"/>
<param name="checkWireStubs" value="1"/>
<param name="checkPolygonWidth" value="0"/>
<param name="useDiameter" value="13"/>
<param name="maxErrors" value="50"/>
</designrules>
<autorouter>
<pass name="Default">
<param name="RoutingGrid" value="50mil"/>
<param name="AutoGrid" value="1"/>
<param name="Efforts" value="0"/>
<param name="TopRouterVariant" value="1"/>
<param name="tpViaShape" value="round"/>
<param name="PrefDir.1" value="a"/>
<param name="PrefDir.2" value="0"/>
<param name="PrefDir.3" value="0"/>
<param name="PrefDir.4" value="0"/>
<param name="PrefDir.5" value="0"/>
<param name="PrefDir.6" value="0"/>
<param name="PrefDir.7" value="0"/>
<param name="PrefDir.8" value="0"/>
<param name="PrefDir.9" value="0"/>
<param name="PrefDir.10" value="0"/>
<param name="PrefDir.11" value="0"/>
<param name="PrefDir.12" value="0"/>
<param name="PrefDir.13" value="0"/>
<param name="PrefDir.14" value="0"/>
<param name="PrefDir.15" value="0"/>
<param name="PrefDir.16" value="a"/>
<param name="cfVia" value="8"/>
<param name="cfNonPref" value="5"/>
<param name="cfChangeDir" value="2"/>
<param name="cfOrthStep" value="2"/>
<param name="cfDiagStep" value="3"/>
<param name="cfExtdStep" value="0"/>
<param name="cfBonusStep" value="1"/>
<param name="cfMalusStep" value="1"/>
<param name="cfPadImpact" value="4"/>
<param name="cfSmdImpact" value="4"/>
<param name="cfBusImpact" value="0"/>
<param name="cfHugging" value="3"/>
<param name="cfAvoid" value="4"/>
<param name="cfPolygon" value="10"/>
<param name="cfBase.1" value="0"/>
<param name="cfBase.2" value="1"/>
<param name="cfBase.3" value="1"/>
<param name="cfBase.4" value="1"/>
<param name="cfBase.5" value="1"/>
<param name="cfBase.6" value="1"/>
<param name="cfBase.7" value="1"/>
<param name="cfBase.8" value="1"/>
<param name="cfBase.9" value="1"/>
<param name="cfBase.10" value="1"/>
<param name="cfBase.11" value="1"/>
<param name="cfBase.12" value="1"/>
<param name="cfBase.13" value="1"/>
<param name="cfBase.14" value="1"/>
<param name="cfBase.15" value="1"/>
<param name="cfBase.16" value="0"/>
<param name="mnVias" value="20"/>
<param name="mnSegments" value="9999"/>
<param name="mnExtdSteps" value="9999"/>
<param name="mnRipupLevel" value="10"/>
<param name="mnRipupSteps" value="100"/>
<param name="mnRipupTotal" value="100"/>
</pass>
<pass name="Follow-me" refer="Default" active="yes">
</pass>
<pass name="Busses" refer="Default" active="yes">
<param name="cfNonPref" value="4"/>
<param name="cfBusImpact" value="4"/>
<param name="cfHugging" value="0"/>
<param name="mnVias" value="0"/>
</pass>
<pass name="Route" refer="Default" active="yes">
</pass>
<pass name="Optimize1" refer="Default" active="yes">
<param name="cfVia" value="99"/>
<param name="cfExtdStep" value="10"/>
<param name="cfHugging" value="1"/>
<param name="mnExtdSteps" value="1"/>
<param name="mnRipupLevel" value="0"/>
</pass>
<pass name="Optimize2" refer="Optimize1" active="yes">
<param name="cfNonPref" value="0"/>
<param name="cfChangeDir" value="6"/>
<param name="cfExtdStep" value="0"/>
<param name="cfBonusStep" value="2"/>
<param name="cfMalusStep" value="2"/>
<param name="cfPadImpact" value="2"/>
<param name="cfSmdImpact" value="2"/>
<param name="cfHugging" value="0"/>
</pass>
<pass name="Optimize3" refer="Optimize2" active="yes">
<param name="cfChangeDir" value="8"/>
<param name="cfPadImpact" value="0"/>
<param name="cfSmdImpact" value="0"/>
</pass>
<pass name="Optimize4" refer="Optimize3" active="yes">
<param name="cfChangeDir" value="25"/>
</pass>
</autorouter>
<elements>
<element name="BH1750" library="SparkFun-Connectors" package="1X05_LONGPADS" value="" x="-162.56" y="25.4" smashed="yes" rot="R90">
<attribute name="NAME" x="-164.592" y="24.13" size="0.6096" layer="25" font="vector" ratio="20" rot="R90"/>
<attribute name="VALUE" x="-159.893" y="24.13" size="0.6096" layer="27" font="vector" ratio="20" rot="R90"/>
</element>
<element name="ASDASD" library="SparkFun-Connectors" package="1X05_LONGPADS" value="" x="-167.64" y="25.4" smashed="yes" rot="R90">
<attribute name="NAME" x="-169.672" y="29.21" size="0.6096" layer="25" font="vector" ratio="20" rot="R90"/>
<attribute name="VALUE" x="-164.973" y="24.13" size="0.6096" layer="27" font="vector" ratio="20" rot="R90"/>
</element>
<element name="CAPACITIVE_SENSOR" library="SparkFun-Connectors" package="1X03_LONGPADS" value="" x="-177.8" y="27.94" smashed="yes" rot="R90">
<attribute name="NAME" x="-179.07" y="26.67" size="0.6096" layer="25" font="vector" ratio="20" rot="R90"/>
<attribute name="VALUE" x="-175.133" y="26.67" size="0.6096" layer="27" font="vector" ratio="20" rot="R90"/>
</element>
<element name="DS18B20" library="SparkFun-Connectors" package="1X03_LONGPADS" value="" x="-172.72" y="27.94" smashed="yes" rot="R90">
<attribute name="NAME" x="-174.752" y="26.67" size="0.6096" layer="25" font="vector" ratio="20" rot="R90"/>
<attribute name="VALUE" x="-170.053" y="26.67" size="0.6096" layer="27" font="vector" ratio="20" rot="R90"/>
</element>
<element name="U$1" library="diy-modules" package="DC-DC-STEP-DOWN-LM2596" value="DC-DC-STEP-DOWN-LM2596" x="-142.24" y="-1.27" smashed="yes" rot="R90">
<attribute name="NAME" x="-153.67" y="-1.27" size="1.27" layer="25" rot="R90" align="bottom-center"/>
<attribute name="VALUE" x="-130.81" y="-1.27" size="1.27" layer="27" rot="R90" align="top-center"/>
</element>
<element name="U$2" library="diy-modules" package="BATTERY-CHARGER-LI-PROT" value="BATTERY-CHARGER-LI-PROT" x="-142.24" y="-41.91" smashed="yes" rot="R90">
<attribute name="NAME" x="-152.4" y="-41.91" size="1.27" layer="25" rot="R90" align="bottom-center"/>
<attribute name="VALUE" x="-132.08" y="-41.91" size="1.27" layer="27" rot="R90" align="top-center"/>
</element>
<element name="SOLAR_PANEL" library="SparkFun-Connectors" package="1X02_LOCK_LONGPADS" value="" x="-125.73" y="-41.91" smashed="yes" rot="R90">
<attribute name="NAME" x="-127.381" y="-43.18" size="0.6096" layer="25" font="vector" ratio="20" rot="R90"/>
<attribute name="VALUE" x="-123.444" y="-43.18" size="0.6096" layer="27" font="vector" ratio="20" rot="R90"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="1k" x="-176.53" y="35.56" smashed="yes" rot="R180">
<attribute name="NAME" x="-176.53" y="34.544" size="0.6096" layer="25" font="vector" ratio="20" rot="R180" align="bottom-center"/>
<attribute name="PROD_ID" value="RES-12182" x="-176.53" y="35.56" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="SX1276-RF" library="diy-modules" package="WIRELESS-LORA-RFM95W#THT" value="WIRELESS-LORA-RFM95W#THT" x="-138.43" y="44.45" smashed="yes" rot="MR180">
<attribute name="NAME" x="-138.43" y="36.195" size="1.27" layer="26" rot="MR180" align="bottom-center"/>
</element>
<element name="BATTERY" library="BK-18650-PC2" package="MPD_BK-18650-PC2" value="BK-18650-PC2" x="-168.91" y="-17.78" smashed="yes" rot="R90">
<attribute name="AVAILABILITY" value="Unavailable" x="-168.91" y="-17.78" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="DESCRIPTION" value=" Holder Batt 1/Li-Ion Protected " x="-168.91" y="-17.78" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MF" value="MPD _Memory" x="-168.91" y="-17.78" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="MP" value="BK-18650-PC2" x="-168.91" y="-17.78" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="NAME" x="-180.5322" y="-56.2534" size="1.7814" layer="25" rot="R90"/>
<attribute name="PACKAGE" value="DFN-14 MPD _Memory Protection Devices_" x="-168.91" y="-17.78" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="PRICE" value="None" x="-168.91" y="-17.78" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="VALUE" x="-154.9185" y="-56.3453" size="1.781009375" layer="27" rot="R90"/>
</element>
<element name="S1" library="switch_dip" package="418117270901" value="418117270901" x="-182.88" y="-49.53" smashed="yes" rot="R180">
<attribute name="AVAILABILITY" value="Unavailable" x="-182.88" y="-49.53" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="DESCRIPTION" value=" Switch Slide Dip Spst 25ma 24v " x="-182.88" y="-49.53" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MF" value="Wurth Electronics" x="-182.88" y="-49.53" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MP" value="418117270901" x="-182.88" y="-49.53" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="NAME" x="-182.99" y="-55.2" size="0.8128" layer="25" rot="R180" align="bottom-center"/>
<attribute name="PACKAGE" value="None" x="-182.88" y="-49.53" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="PRICE" value="None" x="-182.88" y="-49.53" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="VALUE" x="-180.69" y="-43.295" size="0.8128" layer="27" rot="R180"/>
</element>
<element name="S2" library="switch_dip" package="418117270901" value="418117270901" x="-127" y="29.21" smashed="yes" rot="R180">
<attribute name="AVAILABILITY" value="Unavailable" x="-127" y="29.21" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="DESCRIPTION" value=" Switch Slide Dip Spst 25ma 24v " x="-127" y="29.21" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MF" value="Wurth Electronics" x="-127" y="29.21" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MP" value="418117270901" x="-127" y="29.21" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="NAME" x="-127.11" y="23.54" size="0.8128" layer="25" rot="R180" align="bottom-center"/>
<attribute name="PACKAGE" value="None" x="-127" y="29.21" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="PRICE" value="None" x="-127" y="29.21" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="VALUE" x="-124.81" y="35.445" size="0.8128" layer="27" rot="R180"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="1M" x="-142.24" y="33.02" smashed="yes">
<attribute name="PROD_ID" value="RES-09329" x="-142.24" y="33.02" size="1.778" layer="27" display="off"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="1M" x="-142.24" y="30.48" smashed="yes">
<attribute name="PROD_ID" value="RES-09329" x="-142.24" y="30.48" size="1.778" layer="27" display="off"/>
</element>
<element name="PIC16F18426" library="pic16f6xx_14pin" package="DIL14" value="PIC16F8DIL" x="-153.67" y="40.64" smashed="yes" rot="R90">
<attribute name="NAME" x="-151.13" y="24.9682" size="1.778" layer="25" ratio="10" rot="R180"/>
<attribute name="VALUE" x="-152.781" y="31.75" size="1.778" layer="27" ratio="10" rot="R90"/>
</element>
<element name="U$3" library="SparkFun-LED" package="WS2812B-PTH-KIT" value="WS2812B-PTH" x="-172.72" y="49.53" smashed="yes" rot="R270">
<attribute name="NAME" x="-167.386" y="49.53" size="0.6096" layer="25" font="vector" ratio="20" rot="R270" align="bottom-center"/>
<attribute name="VALUE" x="-177.165" y="49.53" size="0.6096" layer="27" font="vector" ratio="20" rot="R270" align="top-center"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="SX1276-RF" pad="B4"/>
<contactref element="S2" pad="1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="PIC16F18426" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="BH1750" pad="3"/>
<contactref element="DS18B20" pad="2"/>
<contactref element="CAPACITIVE_SENSOR" pad="2"/>
<contactref element="ASDASD" pad="3"/>
<wire x1="-180.34" y1="35.56" x2="-181.61" y2="34.29" width="1.27" layer="1"/>
<wire x1="-177.8" y1="30.48" x2="-172.72" y2="30.48" width="1.27" layer="1"/>
<wire x1="-172.72" y1="30.48" x2="-167.64" y2="30.48" width="1.27" layer="1"/>
<wire x1="-167.64" y1="30.48" x2="-162.56" y2="30.48" width="1.27" layer="1"/>
<wire x1="-180.34" y1="22.86" x2="-181.61" y2="24.13" width="1.27" layer="1"/>
<wire x1="-181.61" y1="24.13" x2="-181.61" y2="30.48" width="1.27" layer="1"/>
<wire x1="-181.61" y1="30.48" x2="-181.61" y2="34.29" width="1.27" layer="1"/>
<wire x1="-177.8" y1="30.48" x2="-181.61" y2="30.48" width="1.27" layer="1"/>
<wire x1="-127" y1="41.91" x2="-127" y2="33.02" width="1.27" layer="1"/>
<wire x1="-127" y1="41.91" x2="-128.54" y2="43.45" width="1.27" layer="1"/>
<wire x1="-128.54" y1="43.45" x2="-131.93" y2="43.45" width="1.27" layer="1"/>
<wire x1="-127" y1="33.02" x2="-127" y2="29.21" width="1.27" layer="1"/>
<wire x1="-127" y1="29.21" x2="-129.54" y2="26.67" width="1.27" layer="1"/>
<wire x1="-129.54" y1="26.67" x2="-129.54" y2="13.97" width="1.27" layer="1"/>
<wire x1="-129.54" y1="13.97" x2="-133.35" y2="10.16" width="1.27" layer="1"/>
<wire x1="-133.35" y1="10.16" x2="-139.7" y2="10.16" width="1.27" layer="1"/>
<wire x1="-147.32" y1="17.78" x2="-139.7" y2="10.16" width="1.27" layer="1"/>
<wire x1="-131.93" y1="43.45" x2="-135.62" y2="43.45" width="1.27" layer="1"/>
<wire x1="-138.43" y1="40.64" x2="-138.43" y2="33.02" width="1.27" layer="1"/>
<wire x1="-135.62" y1="43.45" x2="-138.43" y2="40.64" width="1.27" layer="1"/>
<wire x1="-149.86" y1="30.48" x2="-151.13" y2="30.48" width="1.27" layer="1"/>
<wire x1="-151.13" y1="30.48" x2="-158.75" y2="22.86" width="1.27" layer="1"/>
<wire x1="-158.75" y1="22.86" x2="-180.34" y2="22.86" width="1.27" layer="1"/>
<wire x1="-149.86" y1="30.48" x2="-147.32" y2="27.94" width="1.27" layer="1"/>
<wire x1="-147.32" y1="27.94" x2="-147.32" y2="17.78" width="1.27" layer="1"/>
</signal>
<signal name="GND">
<contactref element="ASDASD" pad="2"/>
<contactref element="BH1750" pad="2"/>
<contactref element="SX1276-RF" pad="A1"/>
<contactref element="SX1276-RF" pad="A8"/>
<contactref element="U$1" pad="OUT-"/>
<contactref element="R3" pad="P$2"/>
<contactref element="PIC16F18426" pad="14"/>
<wire x1="-162.56" y1="27.94" x2="-167.64" y2="27.94" width="1.27" layer="1"/>
<contactref element="BH1750" pad="1"/>
<contactref element="DS18B20" pad="1"/>
<contactref element="CAPACITIVE_SENSOR" pad="1"/>
<contactref element="ASDASD" pad="1"/>
<wire x1="-167.64" y1="27.94" x2="-172.72" y2="27.94" width="1.27" layer="1"/>
<wire x1="-172.72" y1="27.94" x2="-177.8" y2="27.94" width="1.27" layer="1"/>
<wire x1="-162.56" y1="25.4" x2="-167.64" y2="25.4" width="1.27" layer="1"/>
<wire x1="-167.64" y1="25.4" x2="-167.64" y2="27.94" width="1.27" layer="1"/>
<wire x1="-144.93" y1="51.45" x2="-144.16" y2="51.45" width="1.27" layer="1"/>
<wire x1="-142.24" y1="49.53" x2="-142.24" y2="36.83" width="1.27" layer="1"/>
<wire x1="-144.16" y1="51.45" x2="-142.24" y2="49.53" width="1.27" layer="1"/>
<wire x1="-156.21" y1="30.48" x2="-154.94" y2="31.75" width="1.27" layer="1"/>
<wire x1="-156.21" y1="30.48" x2="-157.48" y2="30.48" width="1.27" layer="1"/>
<wire x1="-162.56" y1="27.94" x2="-158.75" y2="27.94" width="1.27" layer="1"/>
<wire x1="-158.75" y1="27.94" x2="-157.48" y2="29.21" width="1.27" layer="1"/>
<wire x1="-157.48" y1="29.21" x2="-157.48" y2="30.48" width="1.27" layer="1"/>
<wire x1="-144.93" y1="37.45" x2="-144.31" y2="36.83" width="1.27" layer="1"/>
<wire x1="-144.31" y1="36.83" x2="-142.24" y2="36.83" width="1.27" layer="1"/>
<contactref element="U$3" pad="2"/>
<wire x1="-164.719" y1="48.641" x2="-172.0691" y2="48.641" width="1.27" layer="1"/>
<wire x1="-144.93" y1="51.45" x2="-154.94" y2="51.45" width="1.27" layer="1"/>
<wire x1="-154.94" y1="51.45" x2="-161.91" y2="51.45" width="1.27" layer="1"/>
<wire x1="-161.91" y1="51.45" x2="-164.719" y2="48.641" width="1.27" layer="1"/>
<wire x1="-154.94" y1="31.75" x2="-154.94" y2="51.45" width="1.27" layer="1"/>
<wire x1="-142.24" y1="36.83" x2="-142.24" y2="31.75" width="1.27" layer="1"/>
<wire x1="-142.24" y1="31.75" x2="-140.97" y2="30.48" width="1.27" layer="1"/>
<wire x1="-140.97" y1="30.48" x2="-138.43" y2="30.48" width="1.27" layer="1"/>
<wire x1="-138.43" y1="30.48" x2="-133.604" y2="25.654" width="1.27" layer="1"/>
<wire x1="-133.604" y1="25.654" x2="-133.604" y2="18.542" width="1.27" layer="1"/>
</signal>
<signal name="N$2">
<contactref element="SOLAR_PANEL" pad="1"/>
<contactref element="U$2" pad="IN-"/>
<wire x1="-135.255" y1="-53.975" x2="-135.255" y2="-47.625" width="1.27" layer="1"/>
<wire x1="-135.255" y1="-47.625" x2="-129.54" y2="-41.91" width="1.27" layer="1"/>
<wire x1="-129.54" y1="-41.91" x2="-125.857" y2="-41.91" width="1.27" layer="1"/>
<wire x1="-125.857" y1="-41.91" x2="-125.73" y2="-42.037" width="1.27" layer="1"/>
</signal>
<signal name="N$9">
<contactref element="SOLAR_PANEL" pad="2"/>
<contactref element="U$2" pad="IN+"/>
<wire x1="-149.225" y1="-53.975" x2="-134.493" y2="-39.243" width="1.27" layer="1"/>
<wire x1="-134.493" y1="-39.243" x2="-125.73" y2="-39.243" width="1.27" layer="1"/>
</signal>
<signal name="+5V">
</signal>
<signal name="N$1">
<contactref element="U$1" pad="IN+"/>
<contactref element="U$2" pad="OUT+"/>
<wire x1="-149.225" y1="-31.115" x2="-150.876" y2="-29.464" width="1.27" layer="1"/>
<wire x1="-150.876" y1="-29.464" x2="-150.876" y2="-21.082" width="1.27" layer="1"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="OUT-"/>
<contactref element="U$1" pad="IN-"/>
<wire x1="-133.604" y1="-21.082" x2="-133.604" y2="-29.464" width="1.27" layer="1"/>
<wire x1="-133.604" y1="-29.464" x2="-135.255" y2="-31.115" width="1.27" layer="1"/>
</signal>
<signal name="RA4">
<contactref element="PIC16F18426" pad="3"/>
<contactref element="SX1276-RF" pad="A6"/>
<wire x1="-145.5488375" y1="47.956" x2="-145.8528375" y2="48.26" width="1.27" layer="1"/>
<wire x1="-145.5488375" y1="47.956" x2="-145.436" y2="47.956" width="1.27" layer="1"/>
<wire x1="-145.436" y1="47.956" x2="-144.93" y2="47.45" width="1.27" layer="1"/>
<wire x1="-145.8528375" y1="48.26" x2="-151.13" y2="48.26" width="1.27" layer="1"/>
<wire x1="-151.13" y1="48.26" x2="-152.4" y2="46.99" width="1.27" layer="1"/>
<wire x1="-152.4" y1="46.99" x2="-152.4" y2="36.83" width="1.27" layer="1"/>
<wire x1="-152.4" y1="36.83" x2="-151.13" y2="35.56" width="1.27" layer="1"/>
<wire x1="-151.13" y1="35.56" x2="-149.86" y2="35.56" width="1.27" layer="1"/>
</signal>
<signal name="RA3">
<contactref element="PIC16F18426" pad="4"/>
<contactref element="SX1276-RF" pad="A2"/>
<wire x1="-149.86" y1="38.1" x2="-147.32" y2="38.1" width="1.27" layer="1"/>
<wire x1="-145.97" y1="39.45" x2="-144.93" y2="39.45" width="1.27" layer="1"/>
<wire x1="-147.32" y1="38.1" x2="-145.97" y2="39.45" width="1.27" layer="1"/>
</signal>
<signal name="RC5">
<contactref element="PIC16F18426" pad="5"/>
<contactref element="SX1276-RF" pad="A3"/>
<wire x1="-149.86" y1="40.64" x2="-149.05" y2="41.45" width="1.27" layer="1"/>
<wire x1="-149.05" y1="41.45" x2="-144.93" y2="41.45" width="1.27" layer="1"/>
</signal>
<signal name="RC4">
<contactref element="PIC16F18426" pad="6"/>
<contactref element="SX1276-RF" pad="A4"/>
<wire x1="-144.93" y1="43.45" x2="-149.59" y2="43.45" width="1.27" layer="1"/>
<wire x1="-149.59" y1="43.45" x2="-149.86" y2="43.18" width="1.27" layer="1"/>
</signal>
<signal name="RC3">
<contactref element="PIC16F18426" pad="7"/>
<contactref element="SX1276-RF" pad="A5"/>
<wire x1="-144.93" y1="45.45" x2="-145.2" y2="45.72" width="1.27" layer="1"/>
<wire x1="-145.2" y1="45.72" x2="-149.86" y2="45.72" width="1.27" layer="1"/>
</signal>
<signal name="RA0">
<contactref element="PIC16F18426" pad="13"/>
<contactref element="ASDASD" pad="4"/>
<contactref element="BH1750" pad="4"/>
<wire x1="-157.48" y1="33.02" x2="-162.56" y2="33.02" width="1.27" layer="1"/>
<wire x1="-162.56" y1="33.02" x2="-167.64" y2="33.02" width="1.27" layer="1"/>
</signal>
<signal name="RA1">
<contactref element="PIC16F18426" pad="12"/>
<contactref element="BH1750" pad="5"/>
<contactref element="ASDASD" pad="5"/>
<wire x1="-167.64" y1="35.56" x2="-162.56" y2="35.56" width="1.27" layer="1"/>
<wire x1="-162.56" y1="35.56" x2="-157.48" y2="35.56" width="1.27" layer="1"/>
</signal>
<signal name="RA2">
<contactref element="PIC16F18426" pad="11"/>
<contactref element="DS18B20" pad="3"/>
<contactref element="R1" pad="P$1"/>
<wire x1="-170.18" y1="38.1" x2="-157.48" y2="38.1" width="1.27" layer="1"/>
<wire x1="-172.72" y1="33.02" x2="-172.72" y2="35.56" width="1.27" layer="1"/>
<wire x1="-172.72" y1="35.56" x2="-170.18" y2="38.1" width="1.27" layer="1"/>
</signal>
<signal name="RC0">
<contactref element="PIC16F18426" pad="10"/>
<contactref element="CAPACITIVE_SENSOR" pad="3"/>
<wire x1="-177.8" y1="33.02" x2="-177.8" y2="38.1" width="1.27" layer="1"/>
<wire x1="-177.8" y1="38.1" x2="-175.26" y2="40.64" width="1.27" layer="1"/>
<wire x1="-175.26" y1="40.64" x2="-157.48" y2="40.64" width="1.27" layer="1"/>
</signal>
<signal name="RC1">
<contactref element="PIC16F18426" pad="9"/>
<contactref element="U$3" pad="4"/>
<wire x1="-172.0691" y1="51.689" x2="-175.641" y2="51.689" width="1.27" layer="1"/>
<wire x1="-177.8" y1="49.53" x2="-177.8" y2="44.45" width="1.27" layer="1"/>
<wire x1="-177.8" y1="44.45" x2="-176.53" y2="43.18" width="1.27" layer="1"/>
<wire x1="-176.53" y1="43.18" x2="-157.48" y2="43.18" width="1.27" layer="1"/>
<wire x1="-175.641" y1="51.689" x2="-177.8" y2="49.53" width="1.27" layer="1"/>
</signal>
<signal name="RC2">
<contactref element="PIC16F18426" pad="8"/>
<wire x1="-157.48" y1="45.72" x2="-171.2436" y2="45.72" width="1.27" layer="1"/>
<contactref element="U$3" pad="1"/>
<wire x1="-171.2436" y1="45.72" x2="-172.6406" y2="47.117" width="1.27" layer="1"/>
</signal>
<signal name="RA5">
<contactref element="PIC16F18426" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<wire x1="-146.05" y1="33.02" x2="-146.05" y2="30.48" width="1.016" layer="1"/>
<wire x1="-146.05" y1="33.02" x2="-149.86" y2="33.02" width="1.016" layer="1"/>
</signal>
<signal name="GND.3">
<contactref element="SX1276-RF" pad="B7"/>
</signal>
<signal name="SS">
<contactref element="U$1" pad="OUT+"/>
<contactref element="S2" pad="A1"/>
<wire x1="-127" y1="25.4" x2="-127" y2="11.43" width="1.27" layer="1"/>
<wire x1="-127" y1="11.43" x2="-130.81" y2="7.62" width="1.27" layer="1"/>
<wire x1="-130.81" y1="7.62" x2="-140.97" y2="7.62" width="1.27" layer="1"/>
<wire x1="-150.876" y1="17.526" x2="-150.876" y2="18.542" width="1.27" layer="1"/>
<wire x1="-140.97" y1="7.62" x2="-150.876" y2="17.526" width="1.27" layer="1"/>
</signal>
<signal name="B-">
<contactref element="U$2" pad="B-"/>
<contactref element="BATTERY" pad="M"/>
<wire x1="-138.43" y1="-31.115" x2="-138.43" y2="-12.01" width="1.27" layer="1"/>
<wire x1="-138.43" y1="-12.01" x2="-168.91" y2="18.47" width="1.27" layer="1"/>
</signal>
<signal name="SB">
<contactref element="U$2" pad="B+"/>
<contactref element="S1" pad="1"/>
<wire x1="-182.88" y1="-45.72" x2="-173.99" y2="-36.83" width="1.27" layer="1"/>
<wire x1="-173.99" y1="-36.83" x2="-148.59" y2="-36.83" width="1.27" layer="1"/>
<wire x1="-148.59" y1="-36.83" x2="-146.05" y2="-34.29" width="1.27" layer="1"/>
<wire x1="-146.05" y1="-34.29" x2="-146.05" y2="-31.115" width="1.27" layer="1"/>
</signal>
<signal name="N$3">
<contactref element="BATTERY" pad="P"/>
<contactref element="S1" pad="A1"/>
<wire x1="-168.91" y1="-54.03" x2="-182.19" y2="-54.03" width="1.27" layer="1"/>
<wire x1="-182.19" y1="-54.03" x2="-182.88" y2="-53.34" width="1.27" layer="1"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$4">
<polygon width="1.27" layer="1" isolate="1.27">
<vertex x="-185.42" y="55.88"/>
<vertex x="-185.42" y="-55.88"/>
<vertex x="-185.42" y="-57.15"/>
<vertex x="-121.92" y="-57.15"/>
<vertex x="-121.92" y="55.88"/>
</polygon>
</signal>
</signals>
<mfgpreviewcolors>
<mfgpreviewcolor name="soldermaskcolor" color="0xC8008000"/>
<mfgpreviewcolor name="silkscreencolor" color="0xFFFEFEFE"/>
<mfgpreviewcolor name="backgroundcolor" color="0xFF282828"/>
<mfgpreviewcolor name="coppercolor" color="0xFFFFBF00"/>
<mfgpreviewcolor name="substratecolor" color="0xFF786E46"/>
</mfgpreviewcolors>
</board>
</drawing>
</eagle>
