
[![ESP32 IoT GPT](https://files.oaiusercontent.com/file-MjQmD88EVw3aNF2I7HQ0Hkyj?se=2123-10-16T20%3A52%3A11Z&sp=r&sv=2021-08-06&sr=b&rscc=max-age%3D31536000%2C%20immutable&rscd=attachment%3B%20filename%3DyB0xE3NR_400x400.jpg&sig=NtSrKklJfRcWyluuZttEl97XIrVwb1AvaPSfMZfY2tU%3D)](https://chat.openai.com/g/g-mZV5yksrt-esp32-iot-gpt)

# ESP32 IoT GPT [ChatGPT Plus](https://chat.openai.com/g/g-mZV5yksrt-esp32-iot-gpt) / [Search ChatGPT Free](https://gptcall.net/index.html#/?search=ESP32%20IoT%20GPT)

Discover the versatile capabilities of the ESP32 IoT GPT App. This App is the go-to board for IoT innovations, allowing you to easily create IoT applications using its Wi-Fi and BLE functionalities. With the ESP32 IoT GPT App, you can start coding simple ESP32 projects at the Arduino Framework, make HTTP clients, and create GPIO and MQTT client examples. Whether you're a beginner or an experienced developer, this App provides a seamless and intuitive experience for exploring the potential of the ESP32 board. Get ready to unleash your creativity and bring your IoT ideas to life!

## Example prompts

1. **Prompt 1:** "Let's simple start code with ESP32 at Arduino Framework."

2. **Prompt 2:** "Let's make simple HTTP Client With ESP32."

3. **Prompt 3:** "Let's make GPIO and HTTP Client Example ESP32."

4. **Prompt 4:** "Let's make GPIO and MQTT Client Example ESP32."


## Features and commands

1. **Simple start code with ESP32 at Arduino Framework:** This command provides code snippets and instructions on how to get started with programming the ESP32 board using the Arduino Framework.

2. **Make simple HTTP Client With ESP32:** This command guides you through the process of creating an HTTP client application with the ESP32 board. It provides code examples and instructions on how to establish a connection, send HTTP requests, and handle responses.

3. **Make GPIO and HTTP Client Example ESP32:** This command helps you create an example project that involves using the ESP32 board's GPIO (General Purpose Input/Output) pins and integrating an HTTP client functionality. It provides code snippets and instructions on how to control GPIO pins and make HTTP requests simultaneously.

4. **Make GPIO and MQTT Client Example ESP32:** This command assists you in developing an example project that combines the usage of the ESP32 board's GPIO pins with an MQTT client functionality. It provides code examples and instructions on how to control GPIO pins and communicate with an MQTT broker using the ESP32 board.

Note: Please refer to the App documentation for detailed instructions and code snippets for each command.


