| LibDriver W25QXX 1.0.0 W25QXX full function driver

### - c -

- CHIP_NAME : driver_w25qxx.c

### - d -

- DRIVER_VERSION : driver_w25qxx.c
- DRIVER_W25QXX_LINK_DEBUG_PRINT : driver_w25qxx.h
- DRIVER_W25QXX_LINK_DELAY_MS : driver_w25qxx.h
- DRIVER_W25QXX_LINK_DELAY_US : driver_w25qxx.h
- DRIVER_W25QXX_LINK_INIT : driver_w25qxx.h
- DRIVER_W25QXX_LINK_SPI_QSPI_DEINIT : driver_w25qxx.h
- DRIVER_W25QXX_LINK_SPI_QSPI_INIT : driver_w25qxx.h
- DRIVER_W25QXX_LINK_SPI_QSPI_WRITE_READ : driver_w25qxx.h

### - m -

- MANUFACTURER_NAME : driver_w25qxx.c
- MAX_CURRENT : driver_w25qxx.c

### - s -

- SUPPLY_VOLTAGE_MAX : driver_w25qxx.c
- SUPPLY_VOLTAGE_MIN : driver_w25qxx.c

### - t -

- TEMPERATURE_MAX : driver_w25qxx.c
- TEMPERATURE_MIN : driver_w25qxx.c

### - w -

- W25QXX_COMMAND_BLOCK_ERASE_32K : driver_w25qxx.c
- W25QXX_COMMAND_BLOCK_ERASE_64K : driver_w25qxx.c
- W25QXX_COMMAND_CHIP_ERASE : driver_w25qxx.c
- W25QXX_COMMAND_DEVICE_ID_DUAL_IO : driver_w25qxx.c
- W25QXX_COMMAND_DEVICE_ID_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_ENABLE_RESET : driver_w25qxx.c
- W25QXX_COMMAND_ENTER_QSPI_MODE : driver_w25qxx.c
- W25QXX_COMMAND_ERASE_PROGRAM_RESUME : driver_w25qxx.c
- W25QXX_COMMAND_ERASE_PROGRAM_SUSPEND : driver_w25qxx.c
- W25QXX_COMMAND_ERASE_SECURITY_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_DUAL_IO : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_DUAL_OUTPUT : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_QUAD_OUTPUT : driver_w25qxx.c
- W25QXX_COMMAND_GLOBAL_BLOCK_SECTOR_LOCK : driver_w25qxx.c
- W25QXX_COMMAND_GLOBAL_BLOCK_SECTOR_UNLOCK : driver_w25qxx.c
- W25QXX_COMMAND_INDIVIDUAL_BLOCK_LOCK : driver_w25qxx.c
- W25QXX_COMMAND_INDIVIDUAL_BLOCK_UNLOCK : driver_w25qxx.c
- W25QXX_COMMAND_JEDEC_ID : driver_w25qxx.c
- W25QXX_COMMAND_OCTAL_WORD_READ_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_PAGE_PROGRAM : driver_w25qxx.c
- W25QXX_COMMAND_POWER_DOWN : driver_w25qxx.c
- W25QXX_COMMAND_PROGRAM_SECURITY_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_QUAD_PAGE_PROGRAM : driver_w25qxx.c
- W25QXX_COMMAND_READ_BLOCK_LOCK : driver_w25qxx.c
- W25QXX_COMMAND_READ_DATA : driver_w25qxx.c
- W25QXX_COMMAND_READ_MANUFACTURER : driver_w25qxx.c
- W25QXX_COMMAND_READ_SECURITY_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_READ_SFDP_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_READ_STATUS_REG1 : driver_w25qxx.c
- W25QXX_COMMAND_READ_STATUS_REG2 : driver_w25qxx.c
- W25QXX_COMMAND_READ_STATUS_REG3 : driver_w25qxx.c
- W25QXX_COMMAND_READ_UNIQUE_ID : driver_w25qxx.c
- W25QXX_COMMAND_RELEASE_POWER_DOWN : driver_w25qxx.c
- W25QXX_COMMAND_RESET_DEVICE : driver_w25qxx.c
- W25QXX_COMMAND_SECTOR_ERASE_4K : driver_w25qxx.c
- W25QXX_COMMAND_SET_BURST_WITH_WRAP : driver_w25qxx.c
- W25QXX_COMMAND_VOLATILE_SR_WRITE_ENABLE : driver_w25qxx.c
- W25QXX_COMMAND_WORD_READ_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_DISABLE : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_ENABLE : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_STATUS_REG1 : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_STATUS_REG2 : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_STATUS_REG3 : driver_w25qxx.c
- W25QXX_ENABLE_ERASE_READ_TEST : driver_w25qxx_read_test.h