| LibDriver W25QXX 1.0.0 W25QXX full function driver

Macros | Functions
w25qxx test driver function
w25qxx driver function

w25qxx test driver modules More...

## Macros
#define | W25QXX_ENABLE_ERASE_READ_TEST 1
| w25qxx enable erase read test enumeration definition More...

## Functions
uint8_t | w25qxx_read_test (w25qxx_type_t type, w25qxx_interface_t interface, w25qxx_bool_t dual_quad_spi_enable)
| read test More...
uint8_t | w25qxx_register_test (w25qxx_type_t type, w25qxx_interface_t interface, w25qxx_bool_t dual_quad_spi_enable)
| register test More...

## Detailed Description

w25qxx test driver modules

## Macro Definition Documentation

## ◆ W25QXX_ENABLE_ERASE_READ_TEST

#define W25QXX_ENABLE_ERASE_READ_TEST 1

w25qxx enable erase read test enumeration definition

Definition at line 54 of file driver_w25qxx_read_test.h.

## Function Documentation

## ◆ w25qxx_read_test()

uint8_t w25qxx_read_test | ( | w25qxx_type_t | type,
|  | w25qxx_interface_t | interface,
|  | w25qxx_bool_t | dual_quad_spi_enable
| ) |  |

read test

Parameters

  [in] | type | is the chip type
  [in] | interface | is the chip interface
  [in] | dual_quad_spi_enable | is a bool value

Returns
  status code
  - 0 success
  - 1 test failed

Note
  none

Definition at line 55 of file driver_w25qxx_read_test.c.

## ◆ w25qxx_register_test()

uint8_t w25qxx_register_test | ( | w25qxx_type_t | type,
|  | w25qxx_interface_t | interface,
|  | w25qxx_bool_t | dual_quad_spi_enable
| ) |  |

register test

Parameters

  [in] | type | is the chip type
  [in] | interface | is the chip interface
  [in] | dual_quad_spi_enable | is a bool value

Returns
  status code
  - 0 success
  - 1 test failed

Note
  none

Definition at line 51 of file driver_w25qxx_register_test.c.