| LibDriver W25QXX 1.0.0 W25QXX full function driver

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - w -

- W25Q128 : driver_w25qxx.h
- W25Q16 : driver_w25qxx.h
- W25Q256 : driver_w25qxx.h
- W25Q32 : driver_w25qxx.h
- W25Q64 : driver_w25qxx.h
- W25Q80 : driver_w25qxx.h
- W25QXX_ADDRESS_MODE_3_BYTE : driver_w25qxx.h
- W25QXX_ADDRESS_MODE_4_BYTE : driver_w25qxx.h
- w25qxx_address_mode_t : driver_w25qxx.h
- w25qxx_advance_block_erase_32k() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_block_erase_64k() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_chip_erase() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_deinit() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_fast_read() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_get_get_jedec_id() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_get_id() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_get_status1() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_get_status2() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_get_status3() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_global_block_lock() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_global_block_unlock() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_individual_block_lock() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_individual_block_unlock() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_init() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_qspi_set_read_parameters() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_fast_read_dual_io() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_fast_read_dual_output() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_fast_read_quad_io() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_fast_read_quad_output() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_get_manufacturer_device_id_dual_io() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_get_manufacturer_device_id_quad_io() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_get_sfdp() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_get_unique_id() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_octal_word_read_quad_io() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_page_program_quad_input() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_read() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_read_security_register() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_set_burst_with_wrap() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_word_read_quad_io() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_only_spi_write_security_register() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_page_program() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_power_down() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_read() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_read_block_lock() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_reset() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_sector_erase_4k() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_set_status1() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_set_status2() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_set_status3() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_wake_up() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_advance_write() : driver_w25qxx_advance.c , driver_w25qxx_advance.h
- w25qxx_basic_chip_erase() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_basic_deinit() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_basic_get_id() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_basic_init() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_basic_power_down() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_basic_read() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_basic_wake_up() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_basic_write() : driver_w25qxx_basic.c , driver_w25qxx_basic.h
- w25qxx_block_erase_32k() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_block_erase_64k() : driver_w25qxx.c , driver_w25qxx.h
- W25QXX_BOOL_FALSE : driver_w25qxx.h
- w25qxx_bool_t : driver_w25qxx.h
- W25QXX_BOOL_TRUE : driver_w25qxx.h
- W25QXX_BURST_WRAP_16_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_32_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_64_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_8_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_NONE : driver_w25qxx.h
- w25qxx_burst_wrap_t : driver_w25qxx.h
- w25qxx_chip_erase() : driver_w25qxx.c , driver_w25qxx.h
- W25QXX_COMMAND_BLOCK_ERASE_32K : driver_w25qxx.c
- W25QXX_COMMAND_BLOCK_ERASE_64K : driver_w25qxx.c
- W25QXX_COMMAND_CHIP_ERASE : driver_w25qxx.c
- W25QXX_COMMAND_DEVICE_ID_DUAL_IO : driver_w25qxx.c
- W25QXX_COMMAND_DEVICE_ID_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_ENABLE_RESET : driver_w25qxx.c
- W25QXX_COMMAND_ENTER_QSPI_MODE : driver_w25qxx.c
- W25QXX_COMMAND_ERASE_PROGRAM_RESUME : driver_w25qxx.c
- W25QXX_COMMAND_ERASE_PROGRAM_SUSPEND : driver_w25qxx.c
- W25QXX_COMMAND_ERASE_SECURITY_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_DUAL_IO : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_DUAL_OUTPUT : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_FAST_READ_QUAD_OUTPUT : driver_w25qxx.c
- W25QXX_COMMAND_GLOBAL_BLOCK_SECTOR_LOCK : driver_w25qxx.c
- W25QXX_COMMAND_GLOBAL_BLOCK_SECTOR_UNLOCK : driver_w25qxx.c
- W25QXX_COMMAND_INDIVIDUAL_BLOCK_LOCK : driver_w25qxx.c
- W25QXX_COMMAND_INDIVIDUAL_BLOCK_UNLOCK : driver_w25qxx.c
- W25QXX_COMMAND_JEDEC_ID : driver_w25qxx.c
- W25QXX_COMMAND_OCTAL_WORD_READ_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_PAGE_PROGRAM : driver_w25qxx.c
- W25QXX_COMMAND_POWER_DOWN : driver_w25qxx.c
- W25QXX_COMMAND_PROGRAM_SECURITY_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_QUAD_PAGE_PROGRAM : driver_w25qxx.c
- W25QXX_COMMAND_READ_BLOCK_LOCK : driver_w25qxx.c
- W25QXX_COMMAND_READ_DATA : driver_w25qxx.c
- W25QXX_COMMAND_READ_MANUFACTURER : driver_w25qxx.c
- W25QXX_COMMAND_READ_SECURITY_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_READ_SFDP_REGISTER : driver_w25qxx.c
- W25QXX_COMMAND_READ_STATUS_REG1 : driver_w25qxx.c
- W25QXX_COMMAND_READ_STATUS_REG2 : driver_w25qxx.c
- W25QXX_COMMAND_READ_STATUS_REG3 : driver_w25qxx.c
- W25QXX_COMMAND_READ_UNIQUE_ID : driver_w25qxx.c
- W25QXX_COMMAND_RELEASE_POWER_DOWN : driver_w25qxx.c
- W25QXX_COMMAND_RESET_DEVICE : driver_w25qxx.c
- W25QXX_COMMAND_SECTOR_ERASE_4K : driver_w25qxx.c
- W25QXX_COMMAND_SET_BURST_WITH_WRAP : driver_w25qxx.c
- W25QXX_COMMAND_VOLATILE_SR_WRITE_ENABLE : driver_w25qxx.c
- W25QXX_COMMAND_WORD_READ_QUAD_IO : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_DISABLE : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_ENABLE : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_STATUS_REG1 : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_STATUS_REG2 : driver_w25qxx.c
- W25QXX_COMMAND_WRITE_STATUS_REG3 : driver_w25qxx.c
- w25qxx_deinit() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_disable_write() : driver_w25qxx.c , driver_w25qxx.h
- W25QXX_ENABLE_ERASE_READ_TEST : driver_w25qxx_read_test.h
- w25qxx_enable_reset() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_enable_volatile_sr_write() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_enable_write() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_enter_qspi_mode() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_erase_program_resume() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_erase_program_suspend() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_erase_security_register() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_exit_qspi_mode() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_fast_read() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_fast_read_dual_io() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_fast_read_dual_output() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_fast_read_quad_io() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_fast_read_quad_output() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_address_mode() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_dual_quad_spi() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_interface() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_jedec_id() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_manufacturer_device_id() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_manufacturer_device_id_dual_io() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_manufacturer_device_id_quad_io() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_sfdp() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_status1() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_status2() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_status3() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_type() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_get_unique_id() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_global_block_lock() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_global_block_unlock() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_handle_t : driver_w25qxx.h
- w25qxx_individual_block_lock() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_individual_block_unlock() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_info() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_info_t : driver_w25qxx.h
- w25qxx_init() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_interface_debug_print() : driver_w25qxx_interface.h , driver_w25qxx_interface_template.c
- w25qxx_interface_delay_ms() : driver_w25qxx_interface.h , driver_w25qxx_interface_template.c
- w25qxx_interface_delay_us() : driver_w25qxx_interface.h , driver_w25qxx_interface_template.c
- W25QXX_INTERFACE_QSPI : driver_w25qxx.h
- W25QXX_INTERFACE_SPI : driver_w25qxx.h
- w25qxx_interface_spi_qspi_deinit() : driver_w25qxx_interface.h , driver_w25qxx_interface_template.c
- w25qxx_interface_spi_qspi_init() : driver_w25qxx_interface.h , driver_w25qxx_interface_template.c
- w25qxx_interface_spi_qspi_write_read() : driver_w25qxx_interface.h , driver_w25qxx_interface_template.c
- w25qxx_interface_t : driver_w25qxx.h
- w25qxx_octal_word_read_quad_io() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_only_spi_read() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_page_program() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_page_program_quad_input() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_power_down() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_program_security_register() : driver_w25qxx.c , driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_2_33MHZ : driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_4_55MHZ : driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_6_80MHZ : driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_8_80MHZ : driver_w25qxx.h
- w25qxx_qspi_read_dummy_t : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_16_BYTE : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_32_BYTE : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_64_BYTE : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_8_BYTE : driver_w25qxx.h
- w25qxx_qspi_read_wrap_length_t : driver_w25qxx.h
- w25qxx_read() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_read_block_lock() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_read_security_register() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_read_test() : driver_w25qxx_read_test.c , driver_w25qxx_read_test.h
- w25qxx_register_test() : driver_w25qxx_register_test.c , driver_w25qxx_register_test.h
- w25qxx_release_power_down() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_reset_device() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_sector_erase_4k() : driver_w25qxx.c , driver_w25qxx.h
- W25QXX_SECURITY_REGISTER_1 : driver_w25qxx.h
- W25QXX_SECURITY_REGISTER_2 : driver_w25qxx.h
- W25QXX_SECURITY_REGISTER_3 : driver_w25qxx.h
- w25qxx_security_register_t : driver_w25qxx.h
- w25qxx_set_address_mode() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_burst_with_wrap() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_dual_quad_spi() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_interface() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_read_parameters() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_status1() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_status2() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_status3() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_set_type() : driver_w25qxx.c , driver_w25qxx.h
- W25QXX_STATUS1_BLOCK_PROTECT_0 : driver_w25qxx.h
- W25QXX_STATUS1_BLOCK_PROTECT_1 : driver_w25qxx.h
- W25QXX_STATUS1_BLOCK_PROTECT_2 : driver_w25qxx.h
- W25QXX_STATUS1_ERASE_WRITE_PROGRESS : driver_w25qxx.h
- W25QXX_STATUS1_SECTOR_PROTECT_OR_TOP_BOTTOM_PROTECT : driver_w25qxx.h
- W25QXX_STATUS1_STATUS_REGISTER_PROTECT_0 : driver_w25qxx.h
- w25qxx_status1_t : driver_w25qxx.h
- W25QXX_STATUS1_TOP_BOTTOM_PROTECT_OR_BLOCK_PROTECT_3 : driver_w25qxx.h
- W25QXX_STATUS1_WRITE_ENABLE_LATCH : driver_w25qxx.h
- W25QXX_STATUS2_COMPLEMENT_PROTECT : driver_w25qxx.h
- W25QXX_STATUS2_QUAD_ENABLE : driver_w25qxx.h
- W25QXX_STATUS2_SECURITY_REGISTER_1_LOCK_BITS : driver_w25qxx.h
- W25QXX_STATUS2_SECURITY_REGISTER_2_LOCK_BITS : driver_w25qxx.h
- W25QXX_STATUS2_SECURITY_REGISTER_3_LOCK_BITS : driver_w25qxx.h
- W25QXX_STATUS2_STATUS_REGISTER_PROTECT_1 : driver_w25qxx.h
- W25QXX_STATUS2_SUSPEND_STATUS : driver_w25qxx.h
- w25qxx_status2_t : driver_w25qxx.h
- W25QXX_STATUS3_CURRENT_ADDRESS_MODE : driver_w25qxx.h
- W25QXX_STATUS3_HOLD_RESET_FUNCTION : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_100_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_25_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_50_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_75_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_POWER_UP_ADDRESS_MODE : driver_w25qxx.h
- w25qxx_status3_t : driver_w25qxx.h
- W25QXX_STATUS3_WRITE_PROTECT_SELECTION : driver_w25qxx.h
- w25qxx_type_t : driver_w25qxx.h
- w25qxx_word_read_quad_io() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_write() : driver_w25qxx.c , driver_w25qxx.h
- w25qxx_write_read_reg() : driver_w25qxx.c , driver_w25qxx.h