| LibDriver W25QXX 1.0.0 W25QXX full function driver

Macros
w25qxx link driver function
w25qxx driver function

w25qxx link driver modules More...

## Macros
#define | DRIVER_W25QXX_LINK_INIT(HANDLE, STRUCTURE) memset(HANDLE, 0, sizeof(STRUCTURE))
| initialize w25qxx_handle_t structure More...
#define | DRIVER_W25QXX_LINK_SPI_QSPI_INIT(HANDLE, FUC) (HANDLE)->spi_qspi_init = FUC
| link spi_qspi_init function More...
#define | DRIVER_W25QXX_LINK_SPI_QSPI_DEINIT(HANDLE, FUC) (HANDLE)->spi_qspi_deinit = FUC
| link spi_qspi_deinit function More...
#define | DRIVER_W25QXX_LINK_SPI_QSPI_WRITE_READ(HANDLE, FUC) (HANDLE)->spi_qspi_write_read = FUC
| link spi_qspi_write_read function More...
#define | DRIVER_W25QXX_LINK_DELAY_MS(HANDLE, FUC) (HANDLE)->delay_ms = FUC
| link delay_ms function More...
#define | DRIVER_W25QXX_LINK_DELAY_US(HANDLE, FUC) (HANDLE)->delay_us = FUC
| link delay_us function More...
#define | DRIVER_W25QXX_LINK_DEBUG_PRINT(HANDLE, FUC) (HANDLE)->debug_print = FUC
| link debug_print function More...

## Detailed Description

w25qxx link driver modules

## Macro Definition Documentation

## ◆ DRIVER_W25QXX_LINK_DEBUG_PRINT

#define DRIVER_W25QXX_LINK_DEBUG_PRINT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->debug_print = FUC

link debug_print function

Parameters

  [in] | HANDLE | points to a w25qxx handle structure
  [in] | FUC | points to a debug_print function address

Note
  none

Definition at line 313 of file driver_w25qxx.h.

## ◆ DRIVER_W25QXX_LINK_DELAY_MS

#define DRIVER_W25QXX_LINK_DELAY_MS | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->delay_ms = FUC

link delay_ms function

Parameters

  [in] | HANDLE | points to a w25qxx handle structure
  [in] | FUC | points to a delay_ms function address

Note
  none

Definition at line 297 of file driver_w25qxx.h.

## ◆ DRIVER_W25QXX_LINK_DELAY_US

#define DRIVER_W25QXX_LINK_DELAY_US | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->delay_us = FUC

link delay_us function

Parameters

  [in] | HANDLE | points to a w25qxx handle structure
  [in] | FUC | points to a delay_us function address

Note
  none

Definition at line 305 of file driver_w25qxx.h.

## ◆ DRIVER_W25QXX_LINK_INIT

#define DRIVER_W25QXX_LINK_INIT | ( |  | HANDLE,
|  |  | STRUCTURE
| ) |  | memset(HANDLE, 0, sizeof(STRUCTURE))

initialize w25qxx_handle_t structure

Parameters

  [in] | HANDLE | points to a w25qxx handle structure
  [in] | STRUCTURE | is w25qxx_handle_t

Note
  none

Definition at line 265 of file driver_w25qxx.h.

## ◆ DRIVER_W25QXX_LINK_SPI_QSPI_DEINIT

#define DRIVER_W25QXX_LINK_SPI_QSPI_DEINIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_qspi_deinit = FUC

link spi_qspi_deinit function

Parameters

  [in] | HANDLE | points to a w25qxx handle structure
  [in] | FUC | points to a spi_qspi_deinit function address

Note
  none

Definition at line 281 of file driver_w25qxx.h.

## ◆ DRIVER_W25QXX_LINK_SPI_QSPI_INIT

#define DRIVER_W25QXX_LINK_SPI_QSPI_INIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_qspi_init = FUC

link spi_qspi_init function

Parameters

  [in] | HANDLE | points to a w25qxx handle structure
  [in] | FUC | points to a spi_qspi_init function address

Note
  none

Definition at line 273 of file driver_w25qxx.h.

## ◆ DRIVER_W25QXX_LINK_SPI_QSPI_WRITE_READ

#define DRIVER_W25QXX_LINK_SPI_QSPI_WRITE_READ | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_qspi_write_read = FUC

link spi_qspi_write_read function

Parameters

  [in] | HANDLE | points to a w25qxx handle structure
  [in] | FUC | points to a spi_qspi_write_read function address

Note
  none

Definition at line 289 of file driver_w25qxx.h.