| LibDriver W25QXX 1.0.0 W25QXX full function driver

### - w -

- W25Q128 : driver_w25qxx.h
- W25Q16 : driver_w25qxx.h
- W25Q256 : driver_w25qxx.h
- W25Q32 : driver_w25qxx.h
- W25Q64 : driver_w25qxx.h
- W25Q80 : driver_w25qxx.h
- W25QXX_ADDRESS_MODE_3_BYTE : driver_w25qxx.h
- W25QXX_ADDRESS_MODE_4_BYTE : driver_w25qxx.h
- W25QXX_BOOL_FALSE : driver_w25qxx.h
- W25QXX_BOOL_TRUE : driver_w25qxx.h
- W25QXX_BURST_WRAP_16_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_32_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_64_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_8_BYTE : driver_w25qxx.h
- W25QXX_BURST_WRAP_NONE : driver_w25qxx.h
- W25QXX_INTERFACE_QSPI : driver_w25qxx.h
- W25QXX_INTERFACE_SPI : driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_2_33MHZ : driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_4_55MHZ : driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_6_80MHZ : driver_w25qxx.h
- W25QXX_QSPI_READ_DUMMY_8_80MHZ : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_16_BYTE : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_32_BYTE : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_64_BYTE : driver_w25qxx.h
- W25QXX_QSPI_READ_WRAP_LENGTH_8_BYTE : driver_w25qxx.h
- W25QXX_SECURITY_REGISTER_1 : driver_w25qxx.h
- W25QXX_SECURITY_REGISTER_2 : driver_w25qxx.h
- W25QXX_SECURITY_REGISTER_3 : driver_w25qxx.h
- W25QXX_STATUS1_BLOCK_PROTECT_0 : driver_w25qxx.h
- W25QXX_STATUS1_BLOCK_PROTECT_1 : driver_w25qxx.h
- W25QXX_STATUS1_BLOCK_PROTECT_2 : driver_w25qxx.h
- W25QXX_STATUS1_ERASE_WRITE_PROGRESS : driver_w25qxx.h
- W25QXX_STATUS1_SECTOR_PROTECT_OR_TOP_BOTTOM_PROTECT : driver_w25qxx.h
- W25QXX_STATUS1_STATUS_REGISTER_PROTECT_0 : driver_w25qxx.h
- W25QXX_STATUS1_TOP_BOTTOM_PROTECT_OR_BLOCK_PROTECT_3 : driver_w25qxx.h
- W25QXX_STATUS1_WRITE_ENABLE_LATCH : driver_w25qxx.h
- W25QXX_STATUS2_COMPLEMENT_PROTECT : driver_w25qxx.h
- W25QXX_STATUS2_QUAD_ENABLE : driver_w25qxx.h
- W25QXX_STATUS2_SECURITY_REGISTER_1_LOCK_BITS : driver_w25qxx.h
- W25QXX_STATUS2_SECURITY_REGISTER_2_LOCK_BITS : driver_w25qxx.h
- W25QXX_STATUS2_SECURITY_REGISTER_3_LOCK_BITS : driver_w25qxx.h
- W25QXX_STATUS2_STATUS_REGISTER_PROTECT_1 : driver_w25qxx.h
- W25QXX_STATUS2_SUSPEND_STATUS : driver_w25qxx.h
- W25QXX_STATUS3_CURRENT_ADDRESS_MODE : driver_w25qxx.h
- W25QXX_STATUS3_HOLD_RESET_FUNCTION : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_100_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_25_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_50_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_OUTPUT_DRIVER_STRENGTH_75_PERCENTAGE : driver_w25qxx.h
- W25QXX_STATUS3_POWER_UP_ADDRESS_MODE : driver_w25qxx.h
- W25QXX_STATUS3_WRITE_PROTECT_SELECTION : driver_w25qxx.h