# Hardware list
Gateway. The gateway is not LoRaWAN compatible. We will operate on our own LoRa protocol:
* Dragino LoRa Gateway LG01-P  868Mhz Europe version [Spec](https://www.dragino.com/products/lora-lorawan-gateway/item/117-lg01-p.html) - [Datasheet](https://raw.github.com/luigi1809/connectedHives/master/pdf/Datasheet_LG01.pdf)

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/gateway.jpg" width="200">

Hive scale:
* Arduino Uno R3 [Spec](https://store.arduino.cc/arduino-uno-rev3) - 
 [Doc](https://raw.github.com/luigi1809/connectedHives/master/pdf/LG01_LoRa_Gateway_User_Manual.pdf)
 
 <img src="https://raw.github.com/luigi1809/connectedHives/master/img/arduino.jpg" width="200">
 
* Dragino LoRa Shield for Arduino Uno 868Mhz Europe version [Spec](https://www.dragino.com/products/lora/item/102-lora-shield.html) - [Pin Mapping](https://raw.github.com/luigi1809/connectedHives/master/img/LoRa_Shield_Pin_Mapping.png)

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/shield.png" width="200">

* 200kg electronic platform scale load cell. Don't buy cheap load cells. They are not made for heavy load and accuracy will shortly decline (several Kg difference).

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/load-weight-sensor.jpg" width="200">

* HX711 load-cell voltage amplifier module [Pin Mapping](https://raw.github.com/luigi1809/connectedHives/master/img/hx711.jpg)

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/hx711-card.jpg" width="100">

* Adafruit TPL5110 circuit breakout (for power saving) [Doc](https://raw.github.com/luigi1809/connectedHives/master/pdf/adafruit-tpl5110-power-timer-breakout.pdf)

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/tpl5110.jpg" width="100">

* DHT22 temperature and humidity sensor

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/dht22.jpg" width="200">

* lux sensor OPT3001
    
<img src="https://raw.github.com/luigi1809/connectedHives/master/img/opt3001.jpg" width="100">

* In different sizes, Male to Male, Male to Female and Female to Female Jumper Wire Dupont Cable for Arduino

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/dupont.jpg" width="100">

* USB cable Male A to Male B

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/usb.jpg" width="100">

* 4 x AA Alkaline battery Box (4 x 1.5V = 6V) or 5 x AA ni-mh/li-ion rechargeable battery Box (5 x 1.2V = 6V). More than one year autonomy with standard battery quality.

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/4xAA_box.jpg" width="200"><img src="https://raw.github.com/luigi1809/connectedHives/master/img/5xAA_box.jpg" width="200">

* 4 x AA Alkaline or 5 x AA ni-mh/li-ion rechargeable battery

* 2.5x5.5x9mm DC power male plug jack.

<img src="https://raw.github.com/luigi1809/connectedHives/master/img/jack.jpg" width="200">

* optionaly some resistances