# [−][src]Function cortex_m::asm::delay

    pub fn delay(_n: u32)

Blocks the program for at least `n` instruction cycles

This is implemented in assembly so its execution time is the same regardless of the optimization level.

NOTE that the delay can take much longer if interrupts are serviced during its execution.

# Help

## Keyboard Shortcuts

`?`
  Show this help dialog
`S`
  Focus the search field
`↑`
  Move up in search results
`↓`
  Move down in search results
`↹`
  Switch tab
`⏎`
  Go to active search result
`+`
  Expand all sections
`-`
  Collapse all sections

## Search Tricks

Prefix searches with a type followed by a colon (e.g., `fn:`) to restrict the search to a given type.

Accepted types are: `fn`, `mod`, `struct`, `enum`, `trait`, `type`, `macro`, and `const`.

Search functions by type signature (e.g., `vec -> usize` or `* -> vec`)

Search multiple things at once by splitting your query with comma (e.g., `str,u8` or `String,struct:Vec,test`)