       1
       2
       3
       4
       5
       6
       7
       8
       9
      10
      11
      12
      13
      14
      15
      16
      17
      18
      19
      20
      21
      22
      23
      24
      25
      26
      27
      28
      29
      30
      31
      32
      33
      34
      35
      36
      37
      38
      39
      40
      41
      42
      43
      44
      45
      46
      47
      48
      49
      50
      51
      52
      53
      54
      55
      56
      57
      58
      59
      60
      61
      62
      63
      64
      65
      66
      67
      68
      69
      70
      71
      72
      73
      74
      75
      76
      77
      78
      79
      80
      81
      82
      83
      84
      85
      86
      87
      88
      89
      90
      91
      92
      93
      94
      95
      96
      97
      98
      99
     100
     101
     102
     103
     104
     105
     106
     107
     108
     109
     110
     111
     112
     113
     114
     115
     116
     117
     118
     119
     120
     121
     122
     123
     124
     125
     126
     127
     128
     129
     130
     131
     132
     133
     134
     135
     136
     137
     138
     139
     140
     141
     142
     143
     144
     145
     146
     147
     148
     149
     150
     151
     152
     153
     154
     155
     156
     157
     158
     159
     160
     161
     162
     163
     164
     165
     166
     167
     168
     169
     170
     171
     172
     173
     174
     175
     176
     177
     178
     179
     180
     181
     182
     183
     184
     185
     186
     187
     188
     189
     190
     191
     192
     193
     194
     195
     196
     197
     198
     199
     200
     201
     202
     203
     204
     205
     206
     207
     208
     209
     210
     211
     212
     213
     214
     215
     216
     217
     218
     219
     220
     221
     222
     223
     224
     225
     226
     227
     228
     229
     230
     231
     232
     233
     234
     235
     236
     237
     238
     239
     240
     241
     242
     243
     244
     245
     246
     247
     248
     249
     250
     251
     252
     253
     254
     255
     256
     257
     258
     259
     260
     261
     262
     263
     264
     265
     266
     267
     268
     269
     270
     271
     272
     273
     274
     275
     276
     277
     278
     279
     280
     281
     282
     283
     284
     285
     286
     287
     288
     289
     290
     291
     292
     293
     294
     295
     296
     297
     298
     299
     300
     301
     302
     303
     304
     305
     306
     307
     308
     309
     310
     311
     312
     313
     314
     315
     316
     317
     318
     319
     320
     321
     322
     323
     324
     325
     326
     327
     328
     329
     330
     331
     332
     333
     334
     335
     336
     337
     338
     339
     340
     341
     342
     343
     344
     345
     346
     347
     348
     349
     350
     351
     352
     353
     354
     355
     356
     357
     358
     359
     360
     361
     362
     363
     364
     365
     366
     367
     368
     369
     370
     371
     372
     373
     374
     375
     376
     377
     378
     379
     380
     381
     382
     383
     384
     385
     386
     387
     388
     389
     390
     391
     392
     393
     394
     395
     396
     397
     398
     399
     400
     401
     402
     403
     404
     405
     406
     407
     408
     409
     410
     411
     412
     413
     414
     415
     416
     417
     418
     419
     420
     421
     422
     423
     424
     425
     426
     427
     428
     429
     430
     431
     432
     433
     434
     435
     436
     437
     438
     439
     440
     441
     442
     443
     444
     445
     446
     447
     448
     449
     450
     451
     452
     453
     454
     455
     456
     457
     458
     459
     460
     461
     462
     463
     464
     465
     466
     467
     468
     469
     470
     471
     472
     473
     474
     475
     476
     477
     478
     479
     480
     481
     482
     483
     484
     485
     486
     487
     488
     489
     490
     491
     492
     493
     494
     495
     496
     497
     498
     499
     500
     501
     502
     503
     504
     505
     506
     507
     508
     509
     510
     511
     512
     513
     514
     515
     516
     517
     518
     519
     520
     521
     522
     523
     524
     525
     526
     527
     528
     529
     530
     531
     532
     533
     534
     535
     536
     537
     538
     539
     540
     541
     542
     543
     544
     545
     546
     547
     548
     549
     550
     551
     552
     553
     554
     555
     556
     557
     558
     559
     560
     561
     562
     563
     564
     565
     566
     567
     568
     569
     570
     571
     572
     573
     574
     575
     576
     577
     578
     579
     580
     581
     582
     583
     584
     585
     586
     587
     588
     589
     590
     591
     592
     593
     594
     595
     596
     597
     598
     599
     600
     601
     602
     603
     604
     605
     606
     607
     608
     609
     610
     611
     612
     613
     614
     615
     616
     617
     618
     619
     620
     621
     622
     623
     624
     625
     626
     627
     628
     629
     630
     631
     632
     633
     634
     635
     636
     637
     638
     639
     640
     641
     642
     643
     644
     645
     646
     647
     648
     649
     650
     651
     652
     653
     654
     655
     656
     657
     658
     659
     660
     661
     662
     663
     664
     665
     666
     667
     668
     669
     670
     671
     672
     673
     674
     675
     676
     677
     678
     679
     680
     681
     682
     683
     684
     685
     686
     687
     688
     689
     690
     691
     692
     693
     694
     695
     696
     697
     698
     699
     700
     701
     702
     703
     704
     705
     706
     707
     708
     709
     710
     711
     712
     713
     714
     715
     716
     717
     718
     719
     720
     721
     722
     723
     724
     725
     726
     727
     728
     729
     730
     731
     732
     733
     734
     735
     736
     737
     738
     739
     740
     741
     742
     743
     744
     745
     746
     747
     748
     749
     750
     751
     752
     753
     754
     755
     756
     757
     758
     759
     760
     761
     762
     763
     764
     765
     766
     767
     768
     769
     770
     771
     772
     773
     774
     775
     776
     777
     778
     779
     780
     781
     782
     783
     784
     785
     786
     787
     788
     789
     790
     791
     792
     793
     794
     795
     796
     797
     798
     799
     800
     801
     802
     803
     804
     805
     806
     807
     808
     809
     810
     811
     812
     813
     814
     815
     816
     817
     818
     819
     820
     821
     822
     823
     824
     825
     826
     827
     828
     829
     830
     831
     832
     833
     834
     835
     836
     837
     838
     839
     840
     841
     842
     843
     844
     845
     846
     847
     848
     849
     850
     851
     852
     853
     854
     855
     856
     857
     858
     859
     860
     861
     862
     863
     864
     865
     866
     867
     868
     869
     870
     871
     872
     873
     874
     875
     876
     877
     878
     879
     880
     881
     882
     883
     884
     885
     886
     887
     888
     889
     890
     891
     892
     893
     894
     895
     896
     897
     898
     899
     900
     901
     902
     903
     904
     905
     906
     907
     908
     909
     910
     911
     912
     913
     914
     915
     916
     917
     918
     919
     920
     921
     922
     923
     924
     925
     926
     927
     928
     929
     930
     931
     932
     933
     934
     935
     936
     937
     938
     939
     940
     941
     942
     943
     944
     945
     946
     947
     948
     949
     950
     951
     952
     953
     954
     955
     956
     957
     958
     959
     960
     961
     962
     963
     964
     965
     966
     967
     968
     969
     970
     971
     972
     973
     974
     975
     976
     977
     978
     979
     980
     981
     982
     983
     984
     985
     986
     987
     988
     989
     990
     991
     992
     993
     994
     995
     996
     997
     998
     999
    1000
    1001
    1002
    1003
    1004
    1005
    1006
    1007
    1008
    1009
    1010
    1011
    1012
    1013
    1014
    1015
    1016
    1017
    1018
    1019
    1020
    1021
    1022
    1023
    1024
    1025
    1026
    1027
    1028
    1029
    1030
    1031
    1032
    1033
    1034
    1035
    1036
    1037
    1038
    1039
    1040
    1041
    1042
    1043
    1044
    1045
    1046
    1047
    1048
    1049
    1050
    1051
    1052
    1053
    1054
    1055
    1056
    1057
    1058
    1059
    1060
    1061
    1062
    1063
    1064
    1065
    1066
    1067
    1068
    1069
    1070
    1071
    1072
    1073
    1074
    1075
    1076
    1077
    1078
    1079
    1080
    1081
    1082
    1083
    1084
    1085
    1086
    1087
    1088
    1089
    1090
    1091
    1092
    1093
    1094
    1095
    1096
    1097
    1098
    1099
    1100
    1101
    1102
    1103
    1104
    1105
    1106
    1107
    1108
    1109
    1110
    1111
    1112
    1113
    1114
    1115
    1116
    1117
    1118
    1119
    1120
    1121
    1122
    1123
    1124
    1125
    1126
    1127
    1128
    1129
    1130
    1131
    1132
    1133
    1134
    1135
    1136
    1137
    1138
    1139
    1140
    1141
    1142
    1143
    1144
    1145
    1146
    1147
    1148
    1149
    1150
    1151
    1152
    1153
    1154
    1155
    1156
    1157
    1158
    1159
    1160
    1161
    1162
    1163
    1164
    1165
    1166
    1167
    1168
    1169
    1170
    1171
    1172
    1173
    1174
    1175
    1176
    1177
    1178
    1179
    1180
    1181
    1182
    1183
    1184
    1185
    1186
    1187
    1188
    1189
    1190
    1191
    1192
    1193
    1194
    1195
    1196
    1197
    1198
    1199
    1200
    1201
    1202
    1203
    1204
    1205
    1206
    1207
    1208
    1209
    1210
    1211
    1212
    1213
    1214
    1215
    1216
    1217
    1218
    1219
    1220
    1221
    1222
    1223
    1224
    1225
    1226
    1227
    1228
    1229
    1230
    1231
    1232
    1233
    1234
    1235
    1236
    1237
    1238
    1239
    1240
    1241
    1242
    1243
    1244
    1245
    1246
    1247
    1248
    1249
    1250
    1251
    1252
    1253
    1254
    1255
    1256
    1257
    1258
    1259
    1260
    1261
    1262
    1263
    1264
    1265
    1266
    1267
    1268
    1269
    1270
    1271
    1272
    1273
    1274
    1275
    1276
    1277
    1278
    1279
    1280
    1281
    1282
    1283
    1284
    1285
    1286
    1287
    1288
    1289
    1290
    1291
    1292
    1293
    1294
    1295
    1296
    1297
    1298
    1299
    1300
    1301
    1302
    1303
    1304
    1305
    1306
    1307
    1308
    1309
    1310
    1311
    1312
    1313
    1314
    1315
    1316
    1317
    1318
    1319
    1320
    1321
    1322
    1323
    1324
    1325
    1326
    1327
    1328
    1329
    1330
    1331
    1332
    1333
    1334
    1335
    1336
    1337
    1338
    1339
    1340
    1341
    1342
    1343
    1344
    1345
    1346
    1347
    1348
    1349
    1350
    1351
    1352
    1353
    1354
    1355
    1356
    1357
    1358
    1359
    1360
    1361
    1362
    1363
    1364
    1365
    1366
    1367
    1368
    1369
    1370
    1371
    1372
    1373
    1374
    1375
    1376
    1377
    1378
    1379
    1380
    1381
    1382
    1383
    1384
    1385
    1386
    1387
    1388
    1389
    1390
    1391
    1392
    1393
    1394
    1395
    1396
    1397
    1398
    1399
    1400
    1401
    1402
    1403
    1404
    1405
    1406
    1407
    1408
    1409
    1410
    1411
    1412
    1413
    1414
    1415
    1416
    1417
    1418
    1419
    1420
    1421
    1422
    1423
    1424
    1425
    1426
    1427
    1428
    1429
    1430
    1431
    1432
    1433
    1434
    1435
    1436
    1437
    1438
    1439
    1440
    1441
    1442
    1443
    1444
    1445
    1446
    1447
    1448
    1449
    1450
    1451
    1452
    1453
    1454
    1455
    1456
    1457
    1458
    1459
    1460
    1461
    1462
    1463
    1464
    1465
    1466
    1467
    1468
    1469
    1470
    1471
    1472
    1473
    1474
    1475
    1476
    1477
    1478
    1479
    1480
    1481
    1482
    1483
    1484
    1485
    1486
    1487
    1488
    1489
    1490
    1491
    1492
    1493
    1494
    1495
    1496
    1497
    1498
    1499
    1500
    1501
    1502
    1503
    1504
    1505
    1506
    1507
    1508
    1509
    1510
    1511
    1512
    1513
    1514
    1515
    1516
    1517
    1518
    1519
    1520
    1521
    1522
    1523
    1524
    1525
    1526
    1527
    1528
    1529
    1530
    1531
    1532
    1533
    1534
    1535
    1536
    1537
    1538
    1539
    1540
    1541
    1542
    1543
    1544
    1545
    1546
    1547
    1548
    1549
    1550
    1551
    1552
    1553
    1554
    1555
    1556
    1557
    1558
    1559
    1560
    1561
    1562
    1563
    1564
    1565
    1566
    1567
    1568
    1569
    1570
    1571
    1572
    1573
    1574
    1575
    1576
    1577
    1578
    1579
    1580
    1581
    1582
    1583
    1584
    1585
    1586
    1587
    1588
    1589
    1590
    1591
    1592
    1593
    1594
    1595
    1596
    1597
    1598
    1599
    1600
    1601
    1602
    1603
    1604
    1605
    1606
    1607
    1608
    1609
    1610
    1611
    1612
    1613
    1614
    1615
    1616
    1617
    1618
    1619
    1620
    1621
    1622
    1623
    1624
    1625
    1626
    1627
    1628
    1629
    1630
    1631
    1632
    1633
    1634
    1635
    1636
    1637
    1638
    1639
    1640
    1641
    1642
    1643
    1644
    1645
    1646
    1647
    1648
    1649
    1650
    1651
    1652
    1653
    1654
    1655
    1656
    1657
    1658
    1659
    1660
    1661
    1662
    1663
    1664
    1665
    1666
    1667
    1668
    1669
    1670
    1671
    1672
    1673
    1674
    1675
    1676
    1677
    1678
    1679
    1680
    1681
    1682
    1683
    1684
    1685
    1686
    1687
    1688
    1689
    1690
    1691
    1692
    1693
    1694
    1695
    1696
    1697
    1698
    1699
    1700
    1701
    1702
    1703
    1704
    1705
    1706
    1707
    1708
    1709
    1710
    1711
    1712
    1713
    1714
    1715
    1716
    1717
    1718
    1719
    1720
    1721
    1722
    1723
    1724
    1725
    1726
    1727
    1728
    1729
    1730
    1731
    1732
    1733
    1734
    1735
    1736
    1737
    1738
    1739
    1740
    1741
    1742
    1743
    1744
    1745
    1746
    1747
    1748
    1749
    1750
    1751
    1752
    1753
    1754
    1755
    1756
    1757
    1758
    1759
    1760
    1761
    1762
    1763
    1764
    1765
    1766
    1767
    1768
    1769
    1770
    1771
    1772
    1773
    1774
    1775
    1776
    1777
    1778
    1779
    1780
    1781
    1782
    1783
    1784
    1785
    1786
    1787
    1788
    1789
    1790
    1791
    1792
    1793
    1794
    1795
    1796
    1797
    1798
    1799
    1800
    1801
    1802
    1803
    1804
    1805
    1806
    1807
    1808
    1809
    1810
    1811
    1812
    1813
    1814
    1815
    1816
    1817
    1818
    1819
    1820
    1821
    1822
    1823
    1824
    1825
    1826
    1827
    1828
    1829
    1830
    1831
    1832
    1833
    1834
    1835
    1836
    1837
    1838
    1839
    1840
    1841
    1842
    1843
    1844
    1845
    1846
    1847
    1848
    1849
    1850
    1851

    /* automatically generated by rust-bindgen */

    use
    super::*;

    #[repr(C)]
    #[derive(Copy, Clone, Debug, Default, Eq, Hash, Ord, PartialEq, PartialOrd)]
    pub struct __BindgenBitfieldUnit<Storage, Align>
    where
        Storage: AsRef<[u8]> + AsMut<[u8]>,
    {
        storage: Storage,
        align: [Align; 0],
    }
    impl<Storage, Align> __BindgenBitfieldUnit<Storage, Align>
    where
        Storage: AsRef<[u8]> + AsMut<[u8]>,
    {
        #[inline]
        pub fn new(storage: Storage) -> Self {
            Self { storage, align: [] }
        }
        #[inline]
        pub fn get_bit(&self, index: usize) -> bool {
            debug_assert!(index / 8 < self.storage.as_ref().len());
            let byte_index = index / 8;
            let byte = self.storage.as_ref()[byte_index];
            let bit_index = if cfg!(target_endian = "big") {
                7 - (index % 8)
            } else {
                index % 8
            };
            let mask = 1 << bit_index;
            byte & mask == mask
        }
        #[inline]
        pub fn set_bit(&mut self, index: usize, val: bool) {
            debug_assert!(index / 8 < self.storage.as_ref().len());
            let byte_index = index / 8;
            let byte = &mut self.storage.as_mut()[byte_index];
            let bit_index = if cfg!(target_endian = "big") {
                7 - (index % 8)
            } else {
                index % 8
            };
            let mask = 1 << bit_index;
            if val {
                *byte |= mask;
            } else {
                *byte &= !mask;
            }
        }
        #[inline]
        pub fn get(&self, bit_offset: usize, bit_width: u8) -> u64 {
            debug_assert!(bit_width <= 64);
            debug_assert!(bit_offset / 8 < self.storage.as_ref().len());
            debug_assert!((bit_offset + (bit_width as usize)) / 8 <= self.storage.as_ref().len());
            let mut val = 0;
            for i in 0..(bit_width as usize) {
                if self.get_bit(i + bit_offset) {
                    let index = if cfg!(target_endian = "big") {
                        bit_width as usize - 1 - i
                    } else {
                        i
                    };
                    val |= 1 << index;
                }
            }
            val
        }
        #[inline]
        pub fn set(&mut self, bit_offset: usize, bit_width: u8, val: u64) {
            debug_assert!(bit_width <= 64);
            debug_assert!(bit_offset / 8 < self.storage.as_ref().len());
            debug_assert!((bit_offset + (bit_width as usize)) / 8 <= self.storage.as_ref().len());
            for i in 0..(bit_width as usize) {
                let mask = 1 << i;
                let val_bit_is_set = val & mask == mask;
                let index = if cfg!(target_endian = "big") {
                    bit_width as usize - 1 - i
                } else {
                    i
                };
                self.set_bit(index + bit_offset, val_bit_is_set);
            }
        }
    }
    #[repr(C)]
    pub struct __BindgenUnionField<T>(::core::marker::PhantomData<T>);
    impl<T> __BindgenUnionField<T> {
        #[inline]
        pub fn new() -> Self {
            __BindgenUnionField(::core::marker::PhantomData)
        }
        #[inline]
        pub unsafe fn as_ref(&self) -> &T {
            ::core::mem::transmute(self)
        }
        #[inline]
        pub unsafe fn as_mut(&mut self) -> &mut T {
            ::core::mem::transmute(self)
        }
    }
    impl<T> ::core::default::Default for __BindgenUnionField<T> {
        #[inline]
        fn default() -> Self {
            Self::new()
        }
    }
    impl<T> ::core::clone::Clone for __BindgenUnionField<T> {
        #[inline]
        fn clone(&self) -> Self {
            Self::new()
        }
    }
    impl<T> ::core::marker::Copy for __BindgenUnionField<T> {}
    impl<T> ::core::fmt::Debug for __BindgenUnionField<T> {
        fn fmt(&self, fmt: &mut ::core::fmt::Formatter<'_>) -> ::core::fmt::Result {
            fmt.write_str("__BindgenUnionField")
        }
    }
    impl<T> ::core::hash::Hash for __BindgenUnionField<T> {
        fn hash<H: ::core::hash::Hasher>(&self, _state: &mut H) {}
    }
    impl<T> ::core::cmp::PartialEq for __BindgenUnionField<T> {
        fn eq(&self, _other: &__BindgenUnionField<T>) -> bool {
            true
        }
    }
    impl<T> ::core::cmp::Eq for __BindgenUnionField<T> {}
    pub const SENSOR_VALUE_TYPE_OPAQUE: u32 = 0;
    pub const SENSOR_VALUE_TYPE_INT32: u32 = 1;
    pub const SENSOR_VALUE_TYPE_FLOAT: u32 = 2;
    pub const SENSOR_VALUE_TYPE_INT32_TRIPLET: u32 = 3;
    pub const SENSOR_VALUE_TYPE_FLOAT_TRIPLET: u32 = 4;
    pub const SENSOR_ITF_SPI: u32 = 0;
    pub const SENSOR_ITF_I2C: u32 = 1;
    pub const SENSOR_ITF_UART: u32 = 2;
    pub const SENSOR_THRESH_ALGO_WINDOW: u32 = 1;
    pub const SENSOR_THRESH_ALGO_WATERMARK: u32 = 2;
    pub const SENSOR_THRESH_ALGO_USERDEF: u32 = 3;
    pub const SENSOR_IGN_LISTENER: u32 = 1;
    pub type __uint8_t = ::cty::c_uchar;
    pub type __int16_t = ::cty::c_short;
    pub type __uint16_t = ::cty::c_ushort;
    pub type __int32_t = ::cty::c_long;
    pub type __uint32_t = ::cty::c_ulong;
    pub type __int64_t = ::cty::c_longlong;
    pub type os_stack_t = u32;
    pub type os_time_t = u32;
    pub type os_event_fn = ::core::option::Option<unsafe extern "C" fn(ev: *mut os_event)>;
    #[repr(C)]
    pub struct os_event__bindgen_ty_1 {
        pub stqe_next: *mut os_event,
    }
    impl Default for os_event__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct os_eventq__bindgen_ty_1 {
        pub stqh_first: *mut os_event,
        pub stqh_last: *mut *mut os_event,
    }
    impl Default for os_eventq__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct os_callout__bindgen_ty_1 {
        pub tqe_next: *mut os_callout,
        pub tqe_prev: *mut *mut os_callout,
    }
    impl Default for os_callout__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[doc = " Initialize a device."]
    #[doc = ""]
    #[doc = " - __`dev`__: The device to initialize."]
    #[doc = " - __`arg`__: User defined argument to pass to the device initalization"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type os_dev_init_func_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut os_dev, arg2: *mut ::cty::c_void) -> ::cty::c_int,
    >;
    pub type os_dev_open_func_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut os_dev, arg2: u32, arg3: *mut ::cty::c_void) -> ::cty::c_int,
    >;
    pub type os_dev_suspend_func_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut os_dev, arg2: os_time_t, arg3: ::cty::c_int) -> ::cty::c_int,
    >;
    pub type os_dev_resume_func_t =
        ::core::option::Option<unsafe extern "C" fn(arg1: *mut os_dev) -> ::cty::c_int>;
    pub type os_dev_close_func_t =
        ::core::option::Option<unsafe extern "C" fn(arg1: *mut os_dev) -> ::cty::c_int>;
    #[repr(C)]
    pub struct os_dev__bindgen_ty_1 {
        pub stqe_next: *mut os_dev,
    }
    impl Default for os_dev__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct os_memblock__bindgen_ty_1 {
        pub sle_next: *mut os_memblock,
    }
    impl Default for os_memblock__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct os_mempool__bindgen_ty_1 {
        pub stqe_next: *mut os_mempool,
    }
    impl Default for os_mempool__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct os_mempool__bindgen_ty_2 {
        pub slh_first: *mut os_memblock,
    }
    impl Default for os_mempool__bindgen_ty_2 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    pub type os_membuf_t = u32;
    #[repr(C)]
    pub struct os_mutex__bindgen_ty_1 {
        pub slh_first: *mut os_task,
    }
    impl Default for os_mutex__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    pub type os_sanity_check_func_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut os_sanity_check, arg2: *mut ::cty::c_void) -> ::cty::c_int,
    >;
    #[repr(C)]
    pub struct os_sanity_check__bindgen_ty_1 {
        pub sle_next: *mut os_sanity_check,
    }
    impl Default for os_sanity_check__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    pub type os_task_func_t = ::core::option::Option<unsafe extern "C" fn(arg1: *mut ::cty::c_void)>;
    #[repr(C)]
    pub struct os_task__bindgen_ty_1 {
        pub stqe_next: *mut os_task,
    }
    impl Default for os_task__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct os_task__bindgen_ty_2 {
        pub tqe_next: *mut os_task,
        pub tqe_prev: *mut *mut os_task,
    }
    impl Default for os_task__bindgen_ty_2 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct os_task__bindgen_ty_3 {
        pub sle_next: *mut os_task,
    }
    impl Default for os_task__bindgen_ty_3 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Package init function. Remove when we have post-kernel init stages."]
        pub fn sensor_pkg_init();
    }
    pub const sensor_type_t_SENSOR_TYPE_NONE: sensor_type_t = 0;
    pub const sensor_type_t_SENSOR_TYPE_ACCELEROMETER: sensor_type_t = 1;
    pub const sensor_type_t_SENSOR_TYPE_MAGNETIC_FIELD: sensor_type_t = 2;
    pub const sensor_type_t_SENSOR_TYPE_GYROSCOPE: sensor_type_t = 4;
    pub const sensor_type_t_SENSOR_TYPE_LIGHT: sensor_type_t = 8;
    pub const sensor_type_t_SENSOR_TYPE_TEMPERATURE: sensor_type_t = 16;
    pub const sensor_type_t_SENSOR_TYPE_AMBIENT_TEMPERATURE: sensor_type_t = 32;
    pub const sensor_type_t_SENSOR_TYPE_PRESSURE: sensor_type_t = 64;
    pub const sensor_type_t_SENSOR_TYPE_PROXIMITY: sensor_type_t = 128;
    pub const sensor_type_t_SENSOR_TYPE_RELATIVE_HUMIDITY: sensor_type_t = 256;
    pub const sensor_type_t_SENSOR_TYPE_ROTATION_VECTOR: sensor_type_t = 512;
    pub const sensor_type_t_SENSOR_TYPE_ALTITUDE: sensor_type_t = 1024;
    pub const sensor_type_t_SENSOR_TYPE_WEIGHT: sensor_type_t = 2048;
    pub const sensor_type_t_SENSOR_TYPE_LINEAR_ACCEL: sensor_type_t = 4096;
    pub const sensor_type_t_SENSOR_TYPE_GRAVITY: sensor_type_t = 8192;
    pub const sensor_type_t_SENSOR_TYPE_EULER: sensor_type_t = 16384;
    pub const sensor_type_t_SENSOR_TYPE_COLOR: sensor_type_t = 32768;
    pub const sensor_type_t_SENSOR_TYPE_USER_DEFINED_1: sensor_type_t = 67108864;
    pub const sensor_type_t_SENSOR_TYPE_USER_DEFINED_2: sensor_type_t = 134217728;
    pub const sensor_type_t_SENSOR_TYPE_USER_DEFINED_3: sensor_type_t = 268435456;
    pub const sensor_type_t_SENSOR_TYPE_USER_DEFINED_4: sensor_type_t = 536870912;
    pub const sensor_type_t_SENSOR_TYPE_USER_DEFINED_5: sensor_type_t = 1073741824;
    pub const sensor_type_t_SENSOR_TYPE_USER_DEFINED_6: sensor_type_t = -2147483648;
    pub const sensor_type_t_SENSOR_TYPE_ALL: sensor_type_t = 4294967295;
    pub type sensor_type_t = i64;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_DOUBLE_TAP: sensor_event_type_t = 1;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_SINGLE_TAP: sensor_event_type_t = 2;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_FREE_FALL: sensor_event_type_t = 4;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_SLEEP_CHANGE: sensor_event_type_t = 8;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_WAKEUP: sensor_event_type_t = 16;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_SLEEP: sensor_event_type_t = 32;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_CHANGE: sensor_event_type_t = 64;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_X_CHANGE: sensor_event_type_t = 128;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_Y_CHANGE: sensor_event_type_t = 256;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_Z_CHANGE: sensor_event_type_t = 512;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_X_L_CHANGE: sensor_event_type_t = 1024;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_Y_L_CHANGE: sensor_event_type_t = 2048;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_Z_L_CHANGE: sensor_event_type_t = 4096;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_X_H_CHANGE: sensor_event_type_t = 8192;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_Y_H_CHANGE: sensor_event_type_t = 16384;
    pub const sensor_event_type_t_SENSOR_EVENT_TYPE_ORIENT_Z_H_CHANGE: sensor_event_type_t = 32768;
    pub type sensor_event_type_t = u32;
    #[doc = " Configuration structure, describing a specific sensor type off of"]
    #[doc = " an existing sensor."]
    #[repr(C)]
    #[derive(Default)]
    pub struct sensor_cfg {
        pub sc_valtype: u8,
        pub _reserved: [u8; 3usize],
    }
    #[repr(C)]
    pub struct sensor_data_t {
        pub smd: __BindgenUnionField<*mut sensor_mag_data>,
        pub sad: __BindgenUnionField<*mut sensor_accel_data>,
        pub sed: __BindgenUnionField<*mut sensor_euler_data>,
        pub sqd: __BindgenUnionField<*mut sensor_quat_data>,
        pub slad: __BindgenUnionField<*mut sensor_accel_data>,
        pub sgrd: __BindgenUnionField<*mut sensor_accel_data>,
        pub sgd: __BindgenUnionField<*mut sensor_gyro_data>,
        pub std: __BindgenUnionField<*mut sensor_temp_data>,
        pub satd: __BindgenUnionField<*mut sensor_temp_data>,
        pub sld: __BindgenUnionField<*mut sensor_light_data>,
        pub scd: __BindgenUnionField<*mut sensor_color_data>,
        pub spd: __BindgenUnionField<*mut sensor_press_data>,
        pub srhd: __BindgenUnionField<*mut sensor_humid_data>,
        pub bindgen_union_field: u64,
    }
    impl Default for sensor_data_t {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[doc = " Callback for handling sensor data, specified in a sensor listener."]
    #[doc = ""]
    #[doc = " - __`sensor`__: The sensor for which data is being returned"]
    #[doc = " - __`arg`__: The argument provided to sensor_read() function."]
    #[doc = " - __`data`__: A single sensor reading for that sensor listener"]
    #[doc = " - __`type`__: The sensor type for the data function"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_data_func_t = ::core::option::Option<
        unsafe extern "C" fn(
            arg1: *mut sensor,
            arg2: *mut ::cty::c_void,
            arg3: *mut ::cty::c_void,
            arg4: sensor_type_t,
        ) -> ::cty::c_int,
    >;
    #[doc = " Callback for sending trigger notification."]
    #[doc = ""]
    #[doc = " - __`sensor`__: Ptr to the sensor"]
    #[doc = " - __`data`__: Ptr to sensor data"]
    #[doc = " - __`type`__: The sensor type"]
    pub type sensor_trigger_notify_func_t = ::core::option::Option<
        unsafe extern "C" fn(
            arg1: *mut sensor,
            arg2: *mut ::cty::c_void,
            arg3: sensor_type_t,
        ) -> ::cty::c_int,
    >;
    #[doc = " Callback for trigger compare functions."]
    #[doc = ""]
    #[doc = " - __`type`__: Type of sensor"]
    #[doc = " - __`low_thresh`__: The sensor low threshold"]
    #[doc = " - __`high_thresh`__: The sensor high threshold"]
    #[doc = " - __`arg`__: Ptr to data"]
    pub type sensor_trigger_cmp_func_t = ::core::option::Option<
        unsafe extern "C" fn(
            arg1: sensor_type_t,
            arg2: *mut sensor_data_t,
            arg3: *mut sensor_data_t,
            arg4: *mut ::cty::c_void,
        ) -> ::cty::c_int,
    >;
    #[doc = " Callback for event notifications."]
    #[doc = ""]
    #[doc = " - __`sensor`__: The sensor that observed the event"]
    #[doc = " - __`arg`__: The opaque argument provided during registration"]
    #[doc = " - __`event`__: The sensor event type that was observed"]
    pub type sensor_notifier_func_t = ::core::option::Option<
        unsafe extern "C" fn(
            arg1: *mut sensor,
            arg2: *mut ::cty::c_void,
            arg3: sensor_event_type_t,
        ) -> ::cty::c_int,
    >;
    #[doc = " Callback for reporting a sensor read error."]
    #[doc = ""]
    #[doc = " - __`sensor`__: The sensor for which a read failed."]
    #[doc = " - __`arg`__: The optional argument registered with the callback."]
    #[doc = " - __`status`__: Indicates the cause of the read failure.  Determined by the"]
    #[doc = "               underlying sensor driver."]
    pub type sensor_error_func_t = ::core::option::Option<
        unsafe extern "C" fn(sensor: *mut sensor, arg: *mut ::cty::c_void, status: ::cty::c_int),
    >;
    #[repr(C)]
    pub struct sensor_listener {
        pub sl_sensor_type: sensor_type_t,
        pub sl_func: sensor_data_func_t,
        pub sl_arg: *mut ::cty::c_void,
        pub sl_next: sensor_listener__bindgen_ty_1,
    }
    #[repr(C)]
    pub struct sensor_listener__bindgen_ty_1 {
        pub sle_next: *mut sensor_listener,
    }
    impl Default for sensor_listener__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    impl Default for sensor_listener {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[doc = " Registration for sensor event notifications"]
    #[repr(C)]
    pub struct sensor_notifier {
        pub sn_sensor_event_type: sensor_event_type_t,
        pub sn_func: sensor_notifier_func_t,
        pub sn_arg: *mut ::cty::c_void,
        pub sn_next: sensor_notifier__bindgen_ty_1,
    }
    #[repr(C)]
    pub struct sensor_notifier__bindgen_ty_1 {
        pub sle_next: *mut sensor_notifier,
    }
    impl Default for sensor_notifier__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    impl Default for sensor_notifier {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[doc = " Context for sensor read events"]
    #[repr(C)]
    pub struct sensor_read_ev_ctx {
        pub srec_sensor: *mut sensor,
        pub srec_type: sensor_type_t,
    }
    impl Default for sensor_read_ev_ctx {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[doc = " Sensor type traits list"]
    #[repr(C)]
    pub struct sensor_type_traits {
        pub stt_sensor_type: sensor_type_t,
        pub stt_low_thresh: sensor_data_t,
        pub stt_high_thresh: sensor_data_t,
        pub stt_algo: u8,
        pub stt_poll_n: u16,
        pub stt_polls_left: u16,
        pub stt_trigger_cmp_algo: sensor_trigger_cmp_func_t,
        pub stt_sensor: *mut sensor,
        pub stt_next: sensor_type_traits__bindgen_ty_1,
    }
    #[repr(C)]
    pub struct sensor_type_traits__bindgen_ty_1 {
        pub sle_next: *mut sensor_type_traits,
    }
    impl Default for sensor_type_traits__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    impl Default for sensor_type_traits {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct sensor_notify_ev_ctx {
        pub snec_sensor: *mut sensor,
        pub snec_evtype: sensor_event_type_t,
    }
    impl Default for sensor_notify_ev_ctx {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct sensor_notify_os_ev {
        pub snoe_evt: os_event,
        pub snoe_evtype: sensor_event_type_t,
        pub snoe_sensor: *mut sensor,
    }
    impl Default for sensor_notify_os_ev {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[doc = " Read a single value from a sensor, given a specific sensor type"]
    #[doc = " (e.g. SENSOR_TYPE_PROXIMITY)."]
    #[doc = ""]
    #[doc = " - __`sensor`__: The sensor to read from"]
    #[doc = " - __`type`__: The type(s) of sensor values to read.  Mask containing that type, provide"]
    #[doc = "        all, to get all values."]
    #[doc = " - __`data_func`__: The function to call with each value read.  If NULL, it calls all"]
    #[doc = "        sensor listeners associated with this function."]
    #[doc = " - __`arg`__: The argument to pass to the read callback."]
    #[doc = " - __`timeout`__: Timeout. If block until result, specify OS_TIMEOUT_NEVER, 0 returns"]
    #[doc = "        immediately (no wait.)"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_read_func_t = ::core::option::Option<
        unsafe extern "C" fn(
            arg1: *mut sensor,
            arg2: sensor_type_t,
            arg3: sensor_data_func_t,
            arg4: *mut ::cty::c_void,
            arg5: u32,
        ) -> ::cty::c_int,
    >;
    #[doc = " Get the configuration of the sensor for the sensor type.  This includes"]
    #[doc = " the value type of the sensor."]
    #[doc = ""]
    #[doc = " - __`sensor`__: Ptr to the sensor"]
    #[doc = " - __`type`__: The type of sensor value to get configuration for"]
    #[doc = " - __`cfg`__: A pointer to the sensor value to place the returned result into."]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_get_config_func_t = ::core::option::Option<
        unsafe extern "C" fn(
            arg1: *mut sensor,
            arg2: sensor_type_t,
            arg3: *mut sensor_cfg,
        ) -> ::cty::c_int,
    >;
    #[doc = " Send a new configuration register set to the sensor."]
    #[doc = ""]
    #[doc = " - __`sensor`__: Ptr to the sensor-specific stucture"]
    #[doc = " - __`arg`__: Ptr to the sensor-specific configuration structure"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_set_config_func_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut sensor, arg2: *mut ::cty::c_void) -> ::cty::c_int,
    >;
    #[doc = " Set the trigger and threshold values for a specific sensor for the sensor"]
    #[doc = " type."]
    #[doc = ""]
    #[doc = " - __`sensor`__: Ptr to the sensor"]
    #[doc = " - __`type`__: type of sensor"]
    #[doc = " - __`stt`__: Ptr to teh sensor traits"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_set_trigger_thresh_t = ::core::option::Option<
        unsafe extern "C" fn(
            arg1: *mut sensor,
            arg2: sensor_type_t,
            stt: *mut sensor_type_traits,
        ) -> ::cty::c_int,
    >;
    #[doc = " Clear the high/low threshold values for a specific sensor for the sensor"]
    #[doc = " type."]
    #[doc = ""]
    #[doc = " - __`sensor`__: Ptr to the sensor"]
    #[doc = " - __`type`__: Type of sensor"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_clear_trigger_thresh_t = ::core::option::Option<
        unsafe extern "C" fn(sensor: *mut sensor, type_: sensor_type_t) -> ::cty::c_int,
    >;
    #[doc = " Set the notification expectation for a targeted set of events for the"]
    #[doc = " specific sensor. After this function returns successfully, the implementer"]
    #[doc = " shall post corresponding event notifications to the sensor manager."]
    #[doc = ""]
    #[doc = " - __`sensor`__: The sensor to expect notifications from."]
    #[doc = " - __`event`__: The mask of event types to expect notifications from."]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_set_notification_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut sensor, arg2: sensor_event_type_t) -> ::cty::c_int,
    >;
    #[doc = " Unset the notification expectation for a targeted set of events for the"]
    #[doc = " specific sensor."]
    #[doc = ""]
    #[doc = " - __`sensor`__: The sensor."]
    #[doc = " - __`event`__: The mask of event types."]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_unset_notification_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut sensor, arg2: sensor_event_type_t) -> ::cty::c_int,
    >;
    #[doc = " Let driver handle interrupt in the sensor context"]
    #[doc = ""]
    #[doc = " - __`sensor`__: Ptr to the sensor"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero error code on failure."]
    pub type sensor_handle_interrupt_t =
        ::core::option::Option<unsafe extern "C" fn(sensor: *mut sensor) -> ::cty::c_int>;
    #[doc = " Reset Sensor function Ptr"]
    #[doc = ""]
    #[doc = " - __`Ptr`__: to the sensor"]
    #[doc = ""]
    #[doc = " Return: 0 on success, non-zero on failure"]
    pub type sensor_reset_t =
        ::core::option::Option<unsafe extern "C" fn(arg1: *mut sensor) -> ::cty::c_int>;
    #[repr(C)]
    #[derive(Default)]
    pub struct sensor_driver {
        pub sd_read: sensor_read_func_t,
        pub sd_get_config: sensor_get_config_func_t,
        pub sd_set_config: sensor_set_config_func_t,
        pub sd_set_trigger_thresh: sensor_set_trigger_thresh_t,
        pub sd_clear_low_trigger_thresh: sensor_clear_trigger_thresh_t,
        pub sd_clear_high_trigger_thresh: sensor_clear_trigger_thresh_t,
        pub sd_set_notification: sensor_set_notification_t,
        pub sd_unset_notification: sensor_unset_notification_t,
        pub sd_handle_interrupt: sensor_handle_interrupt_t,
        pub sd_reset: sensor_reset_t,
    }
    #[repr(C)]
    pub struct sensor_timestamp {
        pub st_ostv: os_timeval,
        pub st_ostz: os_timezone,
        pub st_cputime: u32,
    }
    impl Default for sensor_timestamp {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    #[derive(Default)]
    pub struct sensor_int {
        pub host_pin: u8,
        pub device_pin: u8,
        pub active: u8,
    }
    #[repr(C)]
    pub struct sensor_itf {
        pub si_type: u8,
        pub si_num: u8,
        pub si_cs_pin: u8,
        pub si_addr: u16,
        pub si_lock: *mut os_mutex,
        pub si_low_pin: u8,
        pub si_high_pin: u8,
        pub si_ints: [sensor_int; 2usize],
    }
    impl Default for sensor_itf {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct sensor {
        pub s_dev: *mut os_dev,
        pub s_lock: os_mutex,
        pub s_types: sensor_type_t,
        pub s_mask: sensor_type_t,
        #[doc = " Poll rate in MS for this sensor."]
        pub s_poll_rate: u32,
        pub s_next_run: os_time_t,
        pub s_funcs: *mut sensor_driver,
        pub s_sts: sensor_timestamp,
        pub s_itf: sensor_itf,
        pub s_interrupt_evt: os_event,
        pub s_listener_list: sensor__bindgen_ty_1,
        pub s_err_fn: sensor_error_func_t,
        pub s_err_arg: *mut ::cty::c_void,
        pub s_notifier_list: sensor__bindgen_ty_2,
        pub s_type_traits_list: sensor__bindgen_ty_3,
        pub s_next: sensor__bindgen_ty_4,
    }
    #[repr(C)]
    pub struct sensor__bindgen_ty_1 {
        pub slh_first: *mut sensor_listener,
    }
    impl Default for sensor__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct sensor__bindgen_ty_2 {
        pub slh_first: *mut sensor_notifier,
    }
    impl Default for sensor__bindgen_ty_2 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct sensor__bindgen_ty_3 {
        pub slh_first: *mut sensor_type_traits,
    }
    impl Default for sensor__bindgen_ty_3 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[repr(C)]
    pub struct sensor__bindgen_ty_4 {
        pub sle_next: *mut sensor,
    }
    impl Default for sensor__bindgen_ty_4 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    impl Default for sensor {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[doc = " Read context for calling user function with argument"]
    #[repr(C)]
    pub struct sensor_read_ctx {
        pub user_func: sensor_data_func_t,
        pub user_arg: *mut ::cty::c_void,
    }
    impl Default for sensor_read_ctx {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Lock access to the sensor_itf specified by si.  Blocks until lock acquired."]
        #[doc = ""]
        #[doc = " - __`si`__: The sensor_itf to lock"]
        #[doc = " - __`timeout`__: The timeout"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero on failure."]
        pub fn sensor_itf_lock(si: *mut sensor_itf, timeout: os_time_t) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Unlock access to the sensor_itf specified by si."]
        #[doc = ""]
        #[doc = " - __`si`__: The sensor_itf to unlock access to"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero on failure."]
        pub fn sensor_itf_unlock(si: *mut sensor_itf);
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Initialize a sensor"]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to initialize"]
        #[doc = " - __`dev`__: The device to associate with this sensor."]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure."]
        pub fn sensor_init(sensor: *mut sensor, dev: *mut os_dev) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Lock access to the sensor specified by sensor.  Blocks until lock acquired."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to lock"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero on failure."]
        pub fn sensor_lock(sensor: *mut sensor) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Unlock access to the sensor specified by sensor."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to unlock access to."]
        pub fn sensor_unlock(sensor: *mut sensor);
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Register a sensor listener. This allows a calling application to receive"]
        #[doc = " callbacks for data from a given sensor object."]
        #[doc = ""]
        #[doc = " For more information on the type of callbacks available, see the documentation"]
        #[doc = " for the sensor listener structure."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to register a listener on"]
        #[doc = " - __`listener`__: The listener to register onto the sensor"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure."]
        pub fn sensor_register_listener(
            sensor: *mut sensor,
            listener: *mut sensor_listener,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Un-register a sensor listener. This allows a calling application to clear"]
        #[doc = " callbacks for a given sensor object."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor object"]
        #[doc = " - __`listener`__: The listener to remove from the sensor listener list"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure."]
        pub fn sensor_unregister_listener(
            sensor: *mut sensor,
            listener: *mut sensor_listener,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Register a sensor error callback.  The callback is executed when the sensor"]
        #[doc = " manager fails to read from the given sensor."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to register an error callback on."]
        #[doc = " - __`err_fn`__: The function to execute when a read fails."]
        #[doc = " - __`arg`__: Optional argument to pass to the callback."]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure."]
        pub fn sensor_register_err_func(
            sensor: *mut sensor,
            err_fn: sensor_error_func_t,
            arg: *mut ::cty::c_void,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Register a sensor notifier. This allows a calling application to receive"]
        #[doc = " callbacks any time a requested event is observed."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to register the notifier on"]
        #[doc = " - __`notifier`__: The notifier to register"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure."]
        pub fn sensor_register_notifier(
            sensor: *mut sensor,
            notifier: *mut sensor_notifier,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Un-register a sensor notifier. This allows a calling application to stop"]
        #[doc = " receiving callbacks for events on the sensor object."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor object to un-register the notifier on"]
        #[doc = " - __`notifier`__: The notifier to remove from the notification list"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure."]
        pub fn sensor_unregister_notifier(
            sensor: *mut sensor,
            notifier: *mut sensor_notifier,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Read the data for sensor type \"type,\" from the given sensor and"]
        #[doc = " return the result into the \"value\" parameter."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to read data from"]
        #[doc = " - __`type`__: The type of sensor data to read from the sensor"]
        #[doc = " - __`data_func`__: The callback to call for data returned from that sensor"]
        #[doc = " - __`arg`__: The argument to pass to this callback."]
        #[doc = " - __`timeout`__: Timeout before aborting sensor read"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero on failure."]
        pub fn sensor_read(
            sensor: *mut sensor,
            type_: sensor_type_t,
            data_func: sensor_data_func_t,
            arg: *mut ::cty::c_void,
            timeout: u32,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Lock sensor manager to access the list of sensors"]
        pub fn sensor_mgr_lock() -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Unlock sensor manager once the list of sensors has been accessed"]
        pub fn sensor_mgr_unlock();
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Register the sensor with the global sensor list. This makes the sensor"]
        #[doc = " searchable by other packages, who may want to look it up by type."]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor to register"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure."]
        pub fn sensor_mgr_register(sensor: *mut sensor) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Get the current eventq, the system is misconfigured if there is still"]
        #[doc = " no parent eventq."]
        #[doc = ""]
        #[doc = " Return: Ptr OS eventq that the sensor mgr is set to"]
        pub fn sensor_mgr_evq_get() -> *mut os_eventq;
    }
    pub type sensor_mgr_compare_func_t = ::core::option::Option<
        unsafe extern "C" fn(arg1: *mut sensor, arg2: *mut ::cty::c_void) -> ::cty::c_int,
    >;
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " The sensor manager contains a list of sensors, this function returns"]
        #[doc = " the next sensor in that list, for which compare_func() returns successful"]
        #[doc = " (one).  If prev_cursor is provided, the function starts at that point"]
        #[doc = " in the sensor list."]
        #[doc = ""]
        #[doc = " @warn This function MUST be locked by sensor_mgr_lock/unlock() if the goal is"]
        #[doc = " to iterate through sensors (as opposed to just finding one.)  As the"]
        #[doc = " \"prev_cursor\" may be resorted in the sensor list, in between calls."]
        #[doc = ""]
        #[doc = " - __`compare_func`__: The comparison function to use against sensors in the list."]
        #[doc = " - __`arg`__: The argument to provide to that comparison function"]
        #[doc = " - __`prev_cursor`__: The previous sensor in the sensor manager list, in case of"]
        #[doc = "        iteration.  If desire is to find first matching sensor, provide a"]
        #[doc = "        NULL value."]
        #[doc = ""]
        #[doc = " Return: A pointer to the first sensor found from prev_cursor, or"]
        #[doc = "         NULL, if none found."]
        #[doc = ""]
        pub fn sensor_mgr_find_next(
            arg1: sensor_mgr_compare_func_t,
            arg2: *mut ::cty::c_void,
            arg3: *mut sensor,
        ) -> *mut sensor;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Find the \"next\" sensor available for a given sensor type."]
        #[doc = ""]
        #[doc = " If the sensor parameter, is present find the next entry from that"]
        #[doc = " parameter.  Otherwise, find the first matching sensor."]
        #[doc = ""]
        #[doc = " - __`type`__: The type of sensor to search for"]
        #[doc = " - __`sensor`__: The cursor to search from, or NULL to start from the beginning."]
        #[doc = ""]
        #[doc = " Return: A pointer to the sensor object matching that sensor type, or NULL if"]
        #[doc = "         none found."]
        pub fn sensor_mgr_find_next_bytype(type_: sensor_type_t, sensor: *mut sensor) -> *mut sensor;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Search the sensor list and find the next sensor that corresponds"]
        #[doc = " to a given device name."]
        #[doc = ""]
        #[doc = " - __`devname`__: The device name to search for"]
        #[doc = " - __`sensor`__: The previous sensor found with this device name"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero error code on failure"]
        pub fn sensor_mgr_find_next_bydevname(
            devname: *const ::cty::c_char,
            prev_cursor: *mut sensor,
        ) -> *mut sensor;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Check if sensor type matches"]
        #[doc = ""]
        #[doc = " - __`sensor`__: The sensor object"]
        #[doc = " - __`arg`__: type to check"]
        #[doc = ""]
        #[doc = " Return: 1 if matches, 0 if it doesn't match."]
        pub fn sensor_mgr_match_bytype(sensor: *mut sensor, arg1: *mut ::cty::c_void) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Set the sensor poll rate"]
        #[doc = ""]
        #[doc = " - __`devname`__: Name of the sensor"]
        #[doc = " - __`poll_rate`__: The poll rate in milli seconds"]
        pub fn sensor_set_poll_rate_ms(devname: *const ::cty::c_char, poll_rate: u32) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Set the sensor poll rate multiple based on the device name, sensor type"]
        #[doc = ""]
        #[doc = " - __`devname`__: Name of the sensor"]
        #[doc = " - __`stt`__: The sensor type trait"]
        pub fn sensor_set_n_poll_rate(
            devname: *const ::cty::c_char,
            stt: *mut sensor_type_traits,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Transmit OIC trigger"]
        #[doc = ""]
        #[doc = " - __`sensor`__: Ptr to the sensor"]
        #[doc = " - __`arg`__: Ptr to sensor data"]
        #[doc = " - __`type`__: The sensor type"]
        #[doc = ""]
        #[doc = " Return: 0 on sucess, non-zero on failure"]
        pub fn sensor_oic_tx_trigger(
            sensor: *mut sensor,
            arg: *mut ::cty::c_void,
            type_: sensor_type_t,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Sensor trigger initialization"]
        #[doc = ""]
        #[doc = " - __`sensor`__: Ptr to the sensor"]
        #[doc = " - __`type`__: Sensor type to enable trigger for"]
        #[doc = " - __`notify`__: the function to call if the trigger condition is satisfied"]
        pub fn sensor_trigger_init(
            sensor: *mut sensor,
            type_: sensor_type_t,
            notify: sensor_trigger_notify_func_t,
        );
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Search the sensor type traits list for specific type of sensor"]
        #[doc = ""]
        #[doc = " - __`type`__: The sensor type to search for"]
        #[doc = " - __`sensor`__: Ptr to a sensor"]
        #[doc = ""]
        #[doc = " Return: NULL when no sensor type is found, ptr to sensor_type_traits structure"]
        #[doc = " when found"]
        pub fn sensor_get_type_traits_bytype(
            type_: sensor_type_t,
            sensor: *mut sensor,
        ) -> *mut sensor_type_traits;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Get the type traits for a sensor"]
        #[doc = ""]
        #[doc = " - __`devname`__: Name of the sensor"]
        #[doc = " - __`stt`__: Ptr to sensor types trait struct"]
        #[doc = " - __`type`__: The sensor type"]
        #[doc = ""]
        #[doc = " Return: NULL on failure, sensor struct on success"]
        pub fn sensor_get_type_traits_byname(
            arg1: *const ::cty::c_char,
            arg2: *mut *mut sensor_type_traits,
            arg3: sensor_type_t,
        ) -> *mut sensor;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Set the thresholds along with the comparison algo for a sensor"]
        #[doc = ""]
        #[doc = " - __`devname`__: Name of the sensor"]
        #[doc = " - __`stt`__: Ptr to sensor type traits containing thresholds"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero on failure"]
        pub fn sensor_set_thresh(
            devname: *const ::cty::c_char,
            stt: *mut sensor_type_traits,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Clears the low threshold for a sensor"]
        #[doc = ""]
        #[doc = " - __`devname`__: Name of the sensor"]
        #[doc = " - __`type`__: The sensor type"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero on failure"]
        pub fn sensor_clear_low_thresh(
            devname: *const ::cty::c_char,
            type_: sensor_type_t,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Clears the high threshold for a sensor"]
        #[doc = ""]
        #[doc = " - __`devname`__: Name of the sensor"]
        #[doc = " - __`type`__: The sensor type"]
        #[doc = ""]
        #[doc = " Return: 0 on success, non-zero on failure"]
        pub fn sensor_clear_high_thresh(
            devname: *const ::cty::c_char,
            type_: sensor_type_t,
        ) -> ::cty::c_int;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Puts a notification event on the sensor manager evq"]
        #[doc = ""]
        #[doc = " - __`ctx`__: Notification event context"]
        #[doc = " - __`evtype`__: The notification event type"]
        pub fn sensor_mgr_put_notify_evt(ctx: *mut sensor_notify_ev_ctx, evtype: sensor_event_type_t);
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Puts a interrupt event on the sensor manager evq"]
        #[doc = ""]
        #[doc = " - __`sensor`__: Sensor Ptr as interrupt event context"]
        pub fn sensor_mgr_put_interrupt_evt(sensor: *mut sensor);
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Puts read event on the sensor manager evq"]
        #[doc = ""]
        #[doc = " - __`arg`__: Argument"]
        pub fn sensor_mgr_put_read_evt(arg: *mut ::cty::c_void);
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        #[doc = " Resets the sensor"]
        #[doc = ""]
        #[doc = " - __`Ptr`__: to sensor"]
        pub fn sensor_reset(sensor: *mut sensor) -> ::cty::c_int;
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_accel_data {
        pub sad_x: f32,
        pub sad_y: f32,
        pub sad_z: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_accel_data {
        #[inline]
        pub fn sad_x_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sad_x_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sad_y_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(1usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sad_y_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(1usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sad_z_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(2usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sad_z_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(2usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(
            sad_x_is_valid: u8,
            sad_y_is_valid: u8,
            sad_z_is_valid: u8,
        ) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let sad_x_is_valid: u8 = unsafe { ::core::mem::transmute(sad_x_is_valid) };
                sad_x_is_valid as u64
            });
            __bindgen_bitfield_unit.set(1usize, 1u8, {
                let sad_y_is_valid: u8 = unsafe { ::core::mem::transmute(sad_y_is_valid) };
                sad_y_is_valid as u64
            });
            __bindgen_bitfield_unit.set(2usize, 1u8, {
                let sad_z_is_valid: u8 = unsafe { ::core::mem::transmute(sad_z_is_valid) };
                sad_z_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_mag_data {
        pub smd_x: f32,
        pub smd_y: f32,
        pub smd_z: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_mag_data {
        #[inline]
        pub fn smd_x_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_smd_x_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn smd_y_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(1usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_smd_y_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(1usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn smd_z_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(2usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_smd_z_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(2usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(
            smd_x_is_valid: u8,
            smd_y_is_valid: u8,
            smd_z_is_valid: u8,
        ) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let smd_x_is_valid: u8 = unsafe { ::core::mem::transmute(smd_x_is_valid) };
                smd_x_is_valid as u64
            });
            __bindgen_bitfield_unit.set(1usize, 1u8, {
                let smd_y_is_valid: u8 = unsafe { ::core::mem::transmute(smd_y_is_valid) };
                smd_y_is_valid as u64
            });
            __bindgen_bitfield_unit.set(2usize, 1u8, {
                let smd_z_is_valid: u8 = unsafe { ::core::mem::transmute(smd_z_is_valid) };
                smd_z_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_light_data {
        pub sld_full: u16,
        pub sld_ir: u16,
        pub sld_lux: u32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_light_data {
        #[inline]
        pub fn sld_full_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sld_full_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sld_ir_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(1usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sld_ir_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(1usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sld_lux_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(2usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sld_lux_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(2usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(
            sld_full_is_valid: u8,
            sld_ir_is_valid: u8,
            sld_lux_is_valid: u8,
        ) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let sld_full_is_valid: u8 = unsafe { ::core::mem::transmute(sld_full_is_valid) };
                sld_full_is_valid as u64
            });
            __bindgen_bitfield_unit.set(1usize, 1u8, {
                let sld_ir_is_valid: u8 = unsafe { ::core::mem::transmute(sld_ir_is_valid) };
                sld_ir_is_valid as u64
            });
            __bindgen_bitfield_unit.set(2usize, 1u8, {
                let sld_lux_is_valid: u8 = unsafe { ::core::mem::transmute(sld_lux_is_valid) };
                sld_lux_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_quat_data {
        pub sqd_x: f32,
        pub sqd_y: f32,
        pub sqd_z: f32,
        pub sqd_w: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_quat_data {
        #[inline]
        pub fn sqd_x_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sqd_x_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sqd_y_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(1usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sqd_y_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(1usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sqd_z_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(2usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sqd_z_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(2usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sqd_w_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(3usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sqd_w_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(3usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(
            sqd_x_is_valid: u8,
            sqd_y_is_valid: u8,
            sqd_z_is_valid: u8,
            sqd_w_is_valid: u8,
        ) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let sqd_x_is_valid: u8 = unsafe { ::core::mem::transmute(sqd_x_is_valid) };
                sqd_x_is_valid as u64
            });
            __bindgen_bitfield_unit.set(1usize, 1u8, {
                let sqd_y_is_valid: u8 = unsafe { ::core::mem::transmute(sqd_y_is_valid) };
                sqd_y_is_valid as u64
            });
            __bindgen_bitfield_unit.set(2usize, 1u8, {
                let sqd_z_is_valid: u8 = unsafe { ::core::mem::transmute(sqd_z_is_valid) };
                sqd_z_is_valid as u64
            });
            __bindgen_bitfield_unit.set(3usize, 1u8, {
                let sqd_w_is_valid: u8 = unsafe { ::core::mem::transmute(sqd_w_is_valid) };
                sqd_w_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_euler_data {
        pub sed_h: f32,
        pub sed_r: f32,
        pub sed_p: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_euler_data {
        #[inline]
        pub fn sed_h_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sed_h_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sed_r_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(1usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sed_r_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(1usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sed_p_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(2usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sed_p_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(2usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(
            sed_h_is_valid: u8,
            sed_r_is_valid: u8,
            sed_p_is_valid: u8,
        ) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let sed_h_is_valid: u8 = unsafe { ::core::mem::transmute(sed_h_is_valid) };
                sed_h_is_valid as u64
            });
            __bindgen_bitfield_unit.set(1usize, 1u8, {
                let sed_r_is_valid: u8 = unsafe { ::core::mem::transmute(sed_r_is_valid) };
                sed_r_is_valid as u64
            });
            __bindgen_bitfield_unit.set(2usize, 1u8, {
                let sed_p_is_valid: u8 = unsafe { ::core::mem::transmute(sed_p_is_valid) };
                sed_p_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_color_data {
        pub scd_r: u16,
        pub scd_g: u16,
        pub scd_b: u16,
        pub scd_c: u16,
        pub scd_lux: u16,
        pub scd_colortemp: u16,
        pub scd_saturation: u16,
        pub scd_saturation75: u16,
        pub scd_is_sat: u8,
        pub scd_cratio: f32,
        pub scd_maxlux: u16,
        pub scd_ir: u16,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 2usize], u8>,
    }
    impl sensor_color_data {
        #[inline]
        pub fn scd_r_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_r_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_g_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(1usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_g_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(1usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_b_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(2usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_b_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(2usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_c_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(3usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_c_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(3usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_lux_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(4usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_lux_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(4usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_colortemp_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(5usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_colortemp_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(5usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_saturation_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(6usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_saturation_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(6usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_saturation75_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(7usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_saturation75_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(7usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_is_sat_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(8usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_is_sat_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(8usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_cratio_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(9usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_cratio_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(9usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_maxlux_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(10usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_maxlux_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(10usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn scd_ir_is_valid(&self) -> u16 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(11usize, 1u8) as u16) }
        }
        #[inline]
        pub fn set_scd_ir_is_valid(&mut self, val: u16) {
            unsafe {
                let val: u16 = ::core::mem::transmute(val);
                self._bitfield_1.set(11usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(
            scd_r_is_valid: u16,
            scd_g_is_valid: u16,
            scd_b_is_valid: u16,
            scd_c_is_valid: u16,
            scd_lux_is_valid: u16,
            scd_colortemp_is_valid: u16,
            scd_saturation_is_valid: u16,
            scd_saturation75_is_valid: u16,
            scd_is_sat_is_valid: u16,
            scd_cratio_is_valid: u16,
            scd_maxlux_is_valid: u16,
            scd_ir_is_valid: u16,
        ) -> __BindgenBitfieldUnit<[u8; 2usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 2usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let scd_r_is_valid: u16 = unsafe { ::core::mem::transmute(scd_r_is_valid) };
                scd_r_is_valid as u64
            });
            __bindgen_bitfield_unit.set(1usize, 1u8, {
                let scd_g_is_valid: u16 = unsafe { ::core::mem::transmute(scd_g_is_valid) };
                scd_g_is_valid as u64
            });
            __bindgen_bitfield_unit.set(2usize, 1u8, {
                let scd_b_is_valid: u16 = unsafe { ::core::mem::transmute(scd_b_is_valid) };
                scd_b_is_valid as u64
            });
            __bindgen_bitfield_unit.set(3usize, 1u8, {
                let scd_c_is_valid: u16 = unsafe { ::core::mem::transmute(scd_c_is_valid) };
                scd_c_is_valid as u64
            });
            __bindgen_bitfield_unit.set(4usize, 1u8, {
                let scd_lux_is_valid: u16 = unsafe { ::core::mem::transmute(scd_lux_is_valid) };
                scd_lux_is_valid as u64
            });
            __bindgen_bitfield_unit.set(5usize, 1u8, {
                let scd_colortemp_is_valid: u16 =
                    unsafe { ::core::mem::transmute(scd_colortemp_is_valid) };
                scd_colortemp_is_valid as u64
            });
            __bindgen_bitfield_unit.set(6usize, 1u8, {
                let scd_saturation_is_valid: u16 =
                    unsafe { ::core::mem::transmute(scd_saturation_is_valid) };
                scd_saturation_is_valid as u64
            });
            __bindgen_bitfield_unit.set(7usize, 1u8, {
                let scd_saturation75_is_valid: u16 =
                    unsafe { ::core::mem::transmute(scd_saturation75_is_valid) };
                scd_saturation75_is_valid as u64
            });
            __bindgen_bitfield_unit.set(8usize, 1u8, {
                let scd_is_sat_is_valid: u16 = unsafe { ::core::mem::transmute(scd_is_sat_is_valid) };
                scd_is_sat_is_valid as u64
            });
            __bindgen_bitfield_unit.set(9usize, 1u8, {
                let scd_cratio_is_valid: u16 = unsafe { ::core::mem::transmute(scd_cratio_is_valid) };
                scd_cratio_is_valid as u64
            });
            __bindgen_bitfield_unit.set(10usize, 1u8, {
                let scd_maxlux_is_valid: u16 = unsafe { ::core::mem::transmute(scd_maxlux_is_valid) };
                scd_maxlux_is_valid as u64
            });
            __bindgen_bitfield_unit.set(11usize, 1u8, {
                let scd_ir_is_valid: u16 = unsafe { ::core::mem::transmute(scd_ir_is_valid) };
                scd_ir_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_temp_data {
        pub std_temp: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_temp_data {
        #[inline]
        pub fn std_temp_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_std_temp_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(std_temp_is_valid: u8) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let std_temp_is_valid: u8 = unsafe { ::core::mem::transmute(std_temp_is_valid) };
                std_temp_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_press_data {
        pub spd_press: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_press_data {
        #[inline]
        pub fn spd_press_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_spd_press_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(spd_press_is_valid: u8) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let spd_press_is_valid: u8 = unsafe { ::core::mem::transmute(spd_press_is_valid) };
                spd_press_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_humid_data {
        pub shd_humid: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_humid_data {
        #[inline]
        pub fn shd_humid_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_shd_humid_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(shd_humid_is_valid: u8) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let shd_humid_is_valid: u8 = unsafe { ::core::mem::transmute(shd_humid_is_valid) };
                shd_humid_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C, packed)]
    #[derive(Default)]
    pub struct sensor_gyro_data {
        pub sgd_x: f32,
        pub sgd_y: f32,
        pub sgd_z: f32,
        pub _bitfield_1: __BindgenBitfieldUnit<[u8; 1usize], u8>,
    }
    impl sensor_gyro_data {
        #[inline]
        pub fn sgd_x_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(0usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sgd_x_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(0usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sgd_y_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(1usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sgd_y_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(1usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn sgd_z_is_valid(&self) -> u8 {
            unsafe { ::core::mem::transmute(self._bitfield_1.get(2usize, 1u8) as u8) }
        }
        #[inline]
        pub fn set_sgd_z_is_valid(&mut self, val: u8) {
            unsafe {
                let val: u8 = ::core::mem::transmute(val);
                self._bitfield_1.set(2usize, 1u8, val as u64)
            }
        }
        #[inline]
        pub fn new_bitfield_1(
            sgd_x_is_valid: u8,
            sgd_y_is_valid: u8,
            sgd_z_is_valid: u8,
        ) -> __BindgenBitfieldUnit<[u8; 1usize], u8> {
            let mut __bindgen_bitfield_unit: __BindgenBitfieldUnit<[u8; 1usize], u8> =
                Default::default();
            __bindgen_bitfield_unit.set(0usize, 1u8, {
                let sgd_x_is_valid: u8 = unsafe { ::core::mem::transmute(sgd_x_is_valid) };
                sgd_x_is_valid as u64
            });
            __bindgen_bitfield_unit.set(1usize, 1u8, {
                let sgd_y_is_valid: u8 = unsafe { ::core::mem::transmute(sgd_y_is_valid) };
                sgd_y_is_valid as u64
            });
            __bindgen_bitfield_unit.set(2usize, 1u8, {
                let sgd_z_is_valid: u8 = unsafe { ::core::mem::transmute(sgd_z_is_valid) };
                sgd_z_is_valid as u64
            });
            __bindgen_bitfield_unit
        }
    }
    #[repr(C)]
    pub struct _bindgen_ty_1 {
        pub mgr_lock: os_mutex,
        pub mgr_wakeup_callout: os_callout,
        pub mgr_eventq: *mut os_eventq,
        pub mgr_sensor_list: _bindgen_ty_1__bindgen_ty_1,
    }
    #[repr(C)]
    pub struct _bindgen_ty_1__bindgen_ty_1 {
        pub slh_first: *mut sensor,
    }
    impl Default for _bindgen_ty_1__bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    impl Default for _bindgen_ty_1 {
        fn default() -> Self {
            unsafe { ::core::mem::zeroed() }
        }
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        pub static mut sensor_mgr: _bindgen_ty_1;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        pub static mut sensor_base_ts: sensor_timestamp;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        pub static mut sensor_read_event: os_event;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        pub static mut sensor_notify_evt_pool: os_mempool;
    }
    #[mynewt_macros::safe_wrap(attr)] extern "C" {
        pub static mut sensor_notify_evt_area: [os_membuf_t; 60usize];
    }

# Help

## Keyboard Shortcuts

`?`
  Show this help dialog
`S`
  Focus the search field
`↑`
  Move up in search results
`↓`
  Move down in search results
`↹`
  Switch tab
`⏎`
  Go to active search result
`+`
  Expand all sections
`-`
  Collapse all sections

## Search Tricks

Prefix searches with a type followed by a colon (e.g., `fn:`) to restrict the search to a given type.

Accepted types are: `fn`, `mod`, `struct`, `enum`, `trait`, `type`, `macro`, and `const`.

Search functions by type signature (e.g., `vec -> usize` or `* -> vec`)

Search multiple things at once by splitting your query with comma (e.g., `str,u8` or `String,struct:Vec,test`)