# `esp8266`

Mynewt Driver for ESP8266, ported from mbed.  Connecting to WiFi Access Point,
scanning WiFi Access Points and sending UDP packets are working OK.

This driver implements the CoAP transport for the `sensor_coap` library, located in the parent folder.
