<picture>
  <source media="(prefers-color-scheme: dark)" srcset="https://www.uhenry.com/assets/logo-tallytime-full-white.svg">
  <img width="100%" alt="MicroHenry Tallytime Logo" src="https://www.uhenry.com/assets/logo-tallytime-full-black.svg">
</picture>

# Tallytime (Hardware)

An open-source low-cost Tally & Timecode device, powered by RP2040 & LoRa

> [!NOTE]
> This project is WIP and is ongoing active development, expect breaking changes and modifications

## Features

- [ ]  LTC Timecode jam & generation
- [ ]  Wireless sync through LoRa modem
- [ ]  Direct syncing through raw bitstream
- [ ]  Microphone passthrough
- [ ]  Encoder & OLED screen
- [ ]  USB-C & battery charging

## Images

> Top
> ![Top of PCB](https://micro-henry.github.io/tallytime-hardware/top.png)


> Bottom
> ![Bottom of PCB](https://micro-henry.github.io/tallytime-hardware/bottom.png)

PCB renders generated with a modified version (custom fonts) of [linalinn/kicad-render](https://github.com/linalinn/kicad-render)

## Authors

- [@Kelvin-Ziqi-Zhao](https://www.github.com/Kelvin-Ziqi-Zhao)
- [@Treeezheng](https://www.github.com/Treeezheng)
- [@Arom1a](https://www.github.com/Arom1a)
- [@plushugh](https://www.github.com/plushugh)


## License

[CERN-OHL-S-2.0](https://ohwr.org/cern_ohl_s_v2.txt)

