<config configVersion="1.1" device="dsPIC33CK256MP506" coreVersion="4.85.0">
   <usedClasses class="java.util.HashMap">
      <entry>
         <string>System Module</string>
         <string>class com.microchip.mcc.mcu16.systemManager.DefaultSystemManagerMcu16</string>
      </entry>
      <entry>
         <string>Main Manager</string>
         <string>class com.microchip.mcc.mcu16.mainManager.MainManager</string>
      </entry>
      <entry>
         <string>INTERNAL OSCILLATOR</string>
         <string>class com.microchip.mcc.mcu16.systemManager.clk.Clock</string>
      </entry>
      <entry>
         <string>Pin Module</string>
         <string>class com.microchip.mcc.mcu16.pinManager.PinManager</string>
      </entry>
      <entry>
         <string>WATCHDOG</string>
         <string>class com.microchip.mcc.mcu16.systemManager.wdt.Wdt</string>
      </entry>
      <entry>
         <string>DMT</string>
         <string>class com.microchip.mcc.mcu16.systemManager.dmt.DMT</string>
      </entry>
      <entry>
         <string>RESET</string>
         <string>class com.microchip.mcc.mcu16.systemManager.reset.RESET</string>
      </entry>
      <entry>
         <string>ICD</string>
         <string>class com.microchip.mcc.mcu16.systemManager.icd.Icd</string>
      </entry>
      <entry>
         <string>Interrupt Module</string>
         <string>class com.microchip.mcc.mcu16.interruptManager_dsPIC.InterruptManager_dsPIC</string>
      </entry>
      <entry>
         <string>com.microchip.mcc.mcu16.Mcu16PeripheralLibraryLibraryModule</string>
         <string>class com.microchip.mcc.protocolServices.base.modules.librarymodule.LibraryModule</string>
      </entry>
      <entry>
         <string>TMR1</string>
         <string>class com.microchip.mcc.mcu16.modules.tmr.TMR</string>
      </entry>
   </usedClasses>
   <usedLibraries class="java.util.ArrayList">
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.mcu16.Mcu16PeripheralLibrary" version="1.167.0"/>
   </usedLibraries>
   <tokenMap class="java.util.HashMap">
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="122"/>
         <value>122</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="123"/>
         <value>123</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="124"/>
         <value>124</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="125"/>
         <value>125</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="126"/>
         <value>126</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="127"/>
         <value>127</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="128"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="129"/>
         <value>129</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllGraphicsSelect"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="BFRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="120"/>
         <value>120</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="121"/>
         <value>121</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="111"/>
         <value>111</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR16" settingAlias="RP65R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="112"/>
         <value>112</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="113"/>
         <value>113</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="114"/>
         <value>114</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="115"/>
         <value>115</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="116"/>
         <value>116</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="117"/>
         <value>117</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="118"/>
         <value>118</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="119"/>
         <value>119</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB9" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK"/>
         <value>LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="110"/>
         <value>110</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="144"/>
         <value>144</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="145"/>
         <value>145</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="146"/>
         <value>146</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA4" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="147"/>
         <value>147</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="148"/>
         <value>148</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="149"/>
         <value>149</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV"/>
         <value>Divide by 1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.629%"/>
         <value>34</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="140"/>
         <value>140</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="inputMode"/>
         <value>customTmrMode</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="141"/>
         <value>141</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="142"/>
         <value>142</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="143"/>
         <value>143</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="133"/>
         <value>133</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="134"/>
         <value>134</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="135"/>
         <value>135</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="136"/>
         <value>136</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="137"/>
         <value>137</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="138"/>
         <value>138</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="139"/>
         <value>139</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="OFF"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FBTSEQ" settingAlias="IBSEQ"/>
         <value>4095</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="130"/>
         <value>130</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="131"/>
         <value>131</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="132"/>
         <value>132</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="166"/>
         <value>166</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK"/>
         <value>out of lock</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="167"/>
         <value>167</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="168"/>
         <value>168</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="169"/>
         <value>169</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR16" settingAlias="QEIB2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="160"/>
         <value>160</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="161"/>
         <value>161</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="162"/>
         <value>162</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="163"/>
         <value>163</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="combinedTimer"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="164"/>
         <value>164</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="165"/>
         <value>165</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="155"/>
         <value>155</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="156"/>
         <value>156</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="157"/>
         <value>157</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="158"/>
         <value>158</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="159"/>
         <value>159</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="150"/>
         <value>150</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="151"/>
         <value>151</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="152"/>
         <value>152</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="153"/>
         <value>153</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="154"/>
         <value>154</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR14" settingAlias="QEIA1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="188"/>
         <value>188</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="189"/>
         <value>189</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="FRC"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP40R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="180"/>
         <value>180</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="181"/>
         <value>181</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="182"/>
         <value>182</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="183"/>
         <value>183</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="184"/>
         <value>184</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.140%"/>
         <value>43</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="185"/>
         <value>185</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="186"/>
         <value>186</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="187"/>
         <value>187</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="177"/>
         <value>177</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="178"/>
         <value>178</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="179"/>
         <value>179</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefClkOutoutEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS16384"/>
         <value>14336</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="170"/>
         <value>170</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="171"/>
         <value>171</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="172"/>
         <value>172</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="173"/>
         <value>173</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="174"/>
         <value>174</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="175"/>
         <value>175</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="176"/>
         <value>176</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.358%"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="clock failure"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS32"/>
         <value>5120</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR10"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="199"/>
         <value>199</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSwitching"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="OFF"/>
         <value>1792</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ROSEL"/>
         <value>FOSC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS16"/>
         <value>4096</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS" alias="FRC"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="190"/>
         <value>190</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="191"/>
         <value>191</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="192"/>
         <value>192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="193"/>
         <value>193</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="194"/>
         <value>194</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="195"/>
         <value>195</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="196"/>
         <value>196</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="197"/>
         <value>197</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR11"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="198"/>
         <value>198</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Achievable CAN Clock Frequency"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="DIVSWEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR12"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR13"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.815%"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.380%"/>
         <value>57</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS65536"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_USB"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR14"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Switch is Complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF"/>
         <value>no clock failure</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR15"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR11" settingAlias="OCFBR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR1" registerAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="OFF"/>
         <value>112</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR16"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK" alias="FRC"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CAN Clock Source Frequency"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="CNSTYLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR14" settingAlias="RP60R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR17"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="VCODIV" alias="FVCO/4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="VCODIV" alias="FVCO/3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR18"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="VCODIV" alias="FVCO/2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR32" settingAlias="TCKI9R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FVCODIVFreq"/>
         <value>400000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR1" registerAlias="TCON"/>
         <value>33026</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Pll_Dependent_Clock_Switching"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AFVCODIV"/>
         <value>FVCO/4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.869%"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="XT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC7" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1048576"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="DIVSWEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VSS4A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="out of lock"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP35R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VSS3A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.575%"/>
         <value>35</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS2048"/>
         <value>11264</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR49" settingAlias="U2CTSR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VSS2A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VDD1A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CAN Clock Source"/>
         <value>No Clock Selected</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivider"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="CNSTYLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VSS1A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL"/>
         <value>FOSC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VDD2A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FWDT"/>
         <value>864</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC6" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VDD3A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FBTSEQ" settingAlias="BSEQ"/>
         <value>4095</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR9" settingAlias="ICM7R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VDD4A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE"/>
         <value>1:8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdateAuxPostscaler2Options"/>
         <value>[1:2, 1:1]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllPostscaler2"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="WDTWINEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSource"/>
         <value>FRC Oscillator</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR10" settingAlias="RP53R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FBTSEQ"/>
         <value>4095</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.434%"/>
         <value>56</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR19" settingAlias="RP70R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SPI2PIN"/>
         <value>PPS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS" alias="DISABLED"/>
         <value>192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RPCON" settingAlias="IOLOCK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.326%"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="AVCODIV" alias="FVCO/4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="AVCODIV" alias="FVCO/2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="AVCODIV" alias="FVCO/3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA0MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV" alias="1:1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV" alias="1:3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV" alias="1:2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4096"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="C1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.760%"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV" alias="1:5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV" alias="1:4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV" alias="1:7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV" alias="1:6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR20" settingAlias="RP73R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN" alias="OFF"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="100"/>
         <value>100</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="101"/>
         <value>101</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="102"/>
         <value>102</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="103"/>
         <value>103</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="104"/>
         <value>104</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="105"/>
         <value>105</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="106"/>
         <value>106</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="107"/>
         <value>107</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="108"/>
         <value>108</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="109"/>
         <value>109</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR48" settingAlias="OCFDR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS8192"/>
         <value>13312</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BWRP" alias="OFF"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR6" settingAlias="RP45R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="WDTWINEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_PRIMARY"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR17" settingAlias="RP67R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="HIGH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS8"/>
         <value>3072</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS4"/>
         <value>2048</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR1" settingAlias="INT2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR17" settingAlias="QEINDX2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS2"/>
         <value>1024</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR20" settingAlias="RP72R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNAIISRFunction"/>
         <value>ISR_Pin Module_CNAI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="QEIMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR13" settingAlias="PCI11R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1A"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM"/>
         <value>CSECMD</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1B"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR6" settingAlias="ICM4R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCOND" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1C"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCS" alias="External"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TGATE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:8"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="packageId"/>
         <value>TQFP64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1D"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_ENABLE"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE" alias="1:1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSYNC" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet AVDDA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="CNSTYLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR15" settingAlias="RP62R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="DMT" registerAlias="DMTCLR" settingAlias="STEP2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="T1CK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR14" settingAlias="QEIB1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR20" settingAlias="SDI1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.923%"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="AIVTDIS"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="DMT" registerAlias="DMTCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfdivEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR37" settingAlias="OCFCR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_PRESCALER"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1024"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_POSTSCALER2_FREQUENCY"/>
         <value>500000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPrescaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.272%"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="ON_SW"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllfbDivisorClock"/>
         <value>1600000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS262144"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="CNSTYLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="DIVSWEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNSTATD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLPRE"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOTRIMH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RPCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FBSLIM"/>
         <value>8191</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR33" settingAlias="ICM9R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP33R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB4" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR9" settingAlias="RP50R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="customFDMTIVT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR3" settingAlias="ICM1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SPI2PIN" alias="PPS"/>
         <value>8192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSECMD"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSECME"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR15" settingAlias="QEINDX1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_PLL_ENABLE_FREQUENCY"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="PWMMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockSource"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="VREGS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="BIASMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="PWMMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNSTATA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNSTATB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="BFRC"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C1" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNSTATC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.412%"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="customClkOut"/>
         <value>OSC2 is general purpose digital I/O pin</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR30" settingAlias="SS3R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD10" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VSS4A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTBST" alias="DISABLE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR21" settingAlias="RP75R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RPCON" settingAlias="IOLOCK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMDCON" settingAlias="PMDLOCK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.195%"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="PLLKEN"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP8MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS512"/>
         <value>9216</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELD"/>
         <value>11264</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR11" settingAlias="RP55R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDEVOPT"/>
         <value>9272</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllFeedbackDivisor"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB7" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="200"/>
         <value>200</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VSS1A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="DMT" registerAlias="DMTPRECLR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCOND" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELB"/>
         <value>901</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSYNC" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="no clock failure"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELC"/>
         <value>207</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxPll"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR5" settingAlias="RP43R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VSS3A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FICD" settingAlias="NOBTSWP"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS" alias="STNDRD"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="BIASMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB8" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR45" settingAlias="CLCINAR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VSS2A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL"/>
         <value>No Clock Selected</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP8MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELA"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR21" settingAlias="RP74R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB8"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISC"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VDD4A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD10"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VSS2A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISB"/>
         <value>65533</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTIVTH" settingAlias="DMTIVTH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2048"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="CMP3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VDD3A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VSS1A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="OFF"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB9"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VDD2A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR5" settingAlias="TCKI3R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="CNSTYLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR18" settingAlias="RP69R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="CLKSEL" alias="SYSCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISD"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VSS1A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VDD1A"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS4096"/>
         <value>12288</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VSS2A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx1"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTCFG"/>
         <value>G3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VSS3A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.032%"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD11" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV" alias="1:7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISA"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV" alias="1:4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV" alias="1:3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV" alias="1:6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV" alias="1:5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VSS4A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VSS4A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV" alias="1:2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="POST2DIV" alias="1:1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APOST2DIV"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR22" settingAlias="SDI2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="FRCSEL" alias="FRC"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VSS3A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC2"/>
         <value>100000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDMT" settingAlias="DMTDIS" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="CNSTYLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR16" settingAlias="RP64R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscalerOptions"/>
         <value>[1:7, 1:6, 1:5, 1:4, 1:3, 1:2, 1:1]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="OE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.466%"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR9" settingAlias="RP51R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN"/>
         <value>Switch is Complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="BFRC"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8192"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD13"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/256"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="CNSTYLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.272%"/>
         <value>59</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD"/>
         <value>NONE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="ICM5R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.706%"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FRC"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="CM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD11"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSEN" alias="OFF"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 3"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 4"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="timerExtPinSelection"/>
         <value>FALSE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 9"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 7"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 8"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 5"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 6"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="localClockFreq"/>
         <value>100000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD13" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="AFVCO/3"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="AFVCO/2"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_SOURCE"/>
         <value>FRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSDCMD"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD13" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="AFVCO/4"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.466%"/>
         <value>37</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR47" settingAlias="ADCTRGR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB0"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="FRCSEL" alias="Primary Oscillator"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTCNTL" settingAlias="DMTCNTL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR49" settingAlias="U3CTSR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPrescalerClock"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS256"/>
         <value>8192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB1"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR12" settingAlias="RP57R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD11" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR" alias="1:5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR" alias="1:4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR" alias="1:3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR" alias="1:2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR" alias="1:1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR" alias="1:7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR" alias="1:6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB4"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB3"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR4" settingAlias="ICM2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR10" settingAlias="ICM8R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GWRP" alias="OFF"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR22" settingAlias="RP77R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_OE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR38" settingAlias="PCI18R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR19" settingAlias="U2RXR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.217%"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELD" settingAlias="ANSELD10" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.760%"/>
         <value>50</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="FVCO/4"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.652%"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR44" settingAlias="PCI16R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR18" settingAlias="U1RXR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR8" settingAlias="TCKI6R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP41R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR10" settingAlias="RP52R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB7"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CWRP" alias="OFF"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name AVDDA"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="WATCHDOG" registerAlias="WDTCONL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcEnable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="EC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL3"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL4"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1"/>
         <value>125</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL5"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL6"/>
         <value>80</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR22" settingAlias="RP76R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL2"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL7"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNBIISRFunction"/>
         <value>ISR_Pin Module_CNBI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.031%"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllCpuDivScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.326%"/>
         <value>58</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="WATCHDOG" registerAlias="WDTCONH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL4"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL5"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL6"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL7"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL3"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customViewerUpdate"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="OE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="TMR1_TIISRFunction"/>
         <value>ISR_TMR1_TI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="JTAGEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="PR" settingAlias="PR"/>
         <value>9999</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="IPL1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="IPL2"/>
         <value>4096</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="IPL3"/>
         <value>8192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="IPL4"/>
         <value>12288</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="IPL5"/>
         <value>16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="IPL6"/>
         <value>20480</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="IPL7"/>
         <value>24576</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Interrupt Module" name="GlobalInterrupt"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS"/>
         <value>PS1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR12" settingAlias="PCI8R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureUsb"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SCLKPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="NONE"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR17" settingAlias="RP66R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSLP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="IPL2"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="IPL3"/>
         <value>512</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="IPL4"/>
         <value>768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="IPL5"/>
         <value>1024</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="IPL1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSLP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="IPL6"/>
         <value>1280</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT3" alias="IPL7"/>
         <value>1536</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.163%"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscaler"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="SLPDIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FBOOT"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="PTGMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAvcoDivider"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="OE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="AFVCO"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBOOT" settingAlias="BTMODE" alias="SINGLE"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_PRESCALER_FREQUENCY"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="maxPeriod"/>
         <value>0.00065536</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR45" settingAlias="SENT2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="unlocked"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTBST" alias="ENABLE"/>
         <value>4096</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTBST"/>
         <value>ENABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP6MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR29" settingAlias="SDI3R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.597%"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TMWDIS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR2" settingAlias="T1CKR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C1" alias="OFF"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TON"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FVCOFreq"/>
         <value>1600000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR43" settingAlias="PCI14R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS1024"/>
         <value>10240</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.520%"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32768"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C2" alias="OFF"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SPI2PIN" alias="DEDICATED"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS" alias="T1CK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR13" settingAlias="RP59R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 94"/>
         <value>93</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 95"/>
         <value>94</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="clockSourceSelect"/>
         <value>FCY</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 92"/>
         <value>91</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 93"/>
         <value>92</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 98"/>
         <value>97</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 99"/>
         <value>98</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 96"/>
         <value>95</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 97"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS64"/>
         <value>6144</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.815%"/>
         <value>49</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 90"/>
         <value>89</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 91"/>
         <value>90</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 83"/>
         <value>82</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 84"/>
         <value>83</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 81"/>
         <value>80</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.520%"/>
         <value>36</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 82"/>
         <value>81</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 87"/>
         <value>86</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 88"/>
         <value>87</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 85"/>
         <value>84</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 86"/>
         <value>85</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 89"/>
         <value>88</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 80"/>
         <value>79</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 72"/>
         <value>71</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 73"/>
         <value>72</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 70"/>
         <value>69</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 71"/>
         <value>70</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 76"/>
         <value>75</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 77"/>
         <value>76</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="CMP1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 74"/>
         <value>73</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 75"/>
         <value>74</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 78"/>
         <value>77</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 79"/>
         <value>78</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS" alias="FCY"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdateAuxFBDivisorOptions"/>
         <value>[1:200, 1:199, 1:198, 1:197, 1:196, 1:195, 1:194, 1:193, 1:192, 1:191, 1:190, 1:189, 1:188, 1:187, 1:186, 1:185, 1:184, 1:183, 1:182, 1:181, 1:180, 1:179, 1:178, 1:177, 1:176, 1:175, 1:174, 1:173, 1:172, 1:171, 1:170, 1:169, 1:168, 1:167, 1:166, 1:165, 1:164, 1:163, 1:162, 1:161, 1:160, 1:159, 1:158, 1:157, 1:156, 1:155, 1:154, 1:153, 1:152, 1:151, 1:150, 1:149, 1:148, 1:147, 1:146, 1:145, 1:144, 1:143, 1:142, 1:141, 1:140, 1:139, 1:138, 1:137, 1:136, 1:135, 1:134, 1:133, 1:132, 1:131, 1:130, 1:129, 1:128, 1:127, 1:126, 1:125, 1:124, 1:123, 1:122, 1:121, 1:120, 1:119, 1:118, 1:117, 1:116, 1:115, 1:114, 1:113, 1:112, 1:111, 1:110, 1:109, 1:108, 1:107, 1:106, 1:105, 1:104, 1:103, 1:102, 1:101, 1:100, 1:99, 1:98, 1:97, 1:96, 1:95, 1:94, 1:93, 1:92, 1:91, 1:90, 1:89, 1:88, 1:87, 1:86, 1:85, 1:84, 1:83, 1:82, 1:81, 1:80, 1:79, 1:78, 1:77, 1:76, 1:75, 1:74, 1:73, 1:72, 1:71, 1:70, 1:69, 1:68, 1:67, 1:66, 1:65, 1:64, 1:63, 1:62, 1:61, 1:60, 1:59, 1:58, 1:57, 1:56, 1:55, 1:54, 1:53, 1:52, 1:51, 1:50]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 61"/>
         <value>60</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 62"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 60"/>
         <value>59</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 65"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 66"/>
         <value>65</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 63"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 64"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="APSTSCLR"/>
         <value>1:2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 69"/>
         <value>68</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 67"/>
         <value>66</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 68"/>
         <value>67</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLCK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP6MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR23" settingAlias="RP79R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="FPLLO"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 50"/>
         <value>49</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 51"/>
         <value>50</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 54"/>
         <value>53</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 55"/>
         <value>54</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 52"/>
         <value>51</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 53"/>
         <value>52</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 58"/>
         <value>57</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 59"/>
         <value>58</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 56"/>
         <value>55</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 57"/>
         <value>56</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN"/>
         <value>WIN25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR27" settingAlias="U3RXR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 40"/>
         <value>39</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 43"/>
         <value>42</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 44"/>
         <value>43</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 41"/>
         <value>40</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 42"/>
         <value>41</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 47"/>
         <value>46</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 48"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 45"/>
         <value>44</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 46"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 49"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="AIVTDIS" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 32"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 33"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 30"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 31"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 36"/>
         <value>35</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 37"/>
         <value>36</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 34"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 35"/>
         <value>34</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 38"/>
         <value>37</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 39"/>
         <value>38</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_TRIM"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="CMP1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR20" settingAlias="SCK1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK" alias="FCY"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 21"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 22"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 20"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 25"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 26"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 23"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR11" settingAlias="RP54R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 24"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 29"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 27"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 28"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.597%"/>
         <value>53</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 10"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 11"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 14"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 15"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 12"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 13"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 18"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 19"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 16"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 17"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR26" settingAlias="CAN1RXR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="ENHNCD"/>
         <value>2048</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="HS"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN50"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA0MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS"/>
         <value>PS1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR37" settingAlias="PCI17R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK" alias="LPRC"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="tickerFactor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS" alias="HIGH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR23" settingAlias="RP78R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR8" settingAlias="RP48R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="I2C3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN37"/>
         <value>512</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="AFPLLO"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSEN" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FBOOT" settingAlias="BTMODE"/>
         <value>SINGLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBOOT" settingAlias="BTMODE" alias="DUAL"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN25"/>
         <value>768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR11"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FOSCSEL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR10"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC"/>
         <value>FRCDIV</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR16"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureCANFDClock"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:8"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR15"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.575%"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS"/>
         <value>PGx2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscalerClock"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR14"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockTrim"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR18" settingAlias="RP68R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="prescaledFreq"/>
         <value>100000000.00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.163%"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR17" settingAlias="QEIHOM2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR13"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP7MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA0MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTIVTL" settingAlias="DMTIVTL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR12"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="ON"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR19"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="ClockInput"/>
         <value>32000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDMT" settingAlias="DMTDIS" alias="OFF"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA0"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS256"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV"/>
         <value>125</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ICD" name="customICS"/>
         <value>Communicate on PGC2 and PGD2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB4" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTCFG" alias="G2"/>
         <value>2048</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTCFG" alias="G3"/>
         <value>3072</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCS" alias="FOSC/2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTCFG" alias="G0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR18"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="XTCFG" alias="G1"/>
         <value>1024</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN75"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR22" settingAlias="SCK2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR0" settingAlias="INT1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="actualPeriod"/>
         <value>0.0001</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR17"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA1"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscClock"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VDD1A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoOutputPinEnable"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="PTGMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBOOT" settingAlias="BTMODE" alias="DUALPROT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN"/>
         <value>ON_SW</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.358%"/>
         <value>39</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS"/>
         <value>FCY</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS131072"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR42" settingAlias="PCI12R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="I2C2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="PWMMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Requested CAN Clock Frequency"/>
         <value>20000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="minPeriod"/>
         <value>0.00000002</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB8" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="DMT" registerAlias="DMTCLR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="customPR"/>
         <value>9999</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCS"/>
         <value>External</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB7" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VDD4A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP38R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCOND" settingAlias="CNSTYLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockSource"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="DMT" registerAlias="DMTCON" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VDD3A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TMWIP" alias="Write complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSLP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="DISABLED"/>
         <value>3584</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VDD2A"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ENABLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.629%"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscaler2Options"/>
         <value>[1:4, 1:3, 1:2, 1:1]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivSwitch"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR46" settingAlias="CLCINBR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTCNTH" settingAlias="DMTCNTH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureCodeGuard"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="DMT" registerAlias="DMTPRECLR" settingAlias="STEP1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.109%"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="PTGMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_CHANGE"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.652%"/>
         <value>52</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="I2C2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler2"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK"/>
         <value>unlocked</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBOOT" settingAlias="BTMODE" alias="DUALPRIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="locked"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP7MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.543%"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FALTREG"/>
         <value>30583</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllFeedbackDivisorOptions"/>
         <value>[1:50, 1:51, 1:52, 1:53, 1:54, 1:55, 1:56, 1:57, 1:58, 1:59, 1:60, 1:61, 1:62, 1:63, 1:64, 1:65, 1:66, 1:67, 1:68, 1:69, 1:70, 1:71, 1:72, 1:73, 1:74, 1:75, 1:76, 1:77, 1:78, 1:79, 1:80, 1:81, 1:82, 1:83, 1:84, 1:85, 1:86, 1:87, 1:88, 1:89, 1:90, 1:91, 1:92, 1:93, 1:94, 1:95, 1:96, 1:97, 1:98, 1:99, 1:100, 1:101, 1:102, 1:103, 1:104, 1:105, 1:106, 1:107, 1:108, 1:109, 1:110, 1:111, 1:112, 1:113, 1:114, 1:115, 1:116, 1:117, 1:118, 1:119, 1:120, 1:121, 1:122, 1:123, 1:124, 1:125, 1:126, 1:127, 1:128, 1:129, 1:130, 1:131, 1:132, 1:133, 1:134, 1:135, 1:136, 1:137, 1:138, 1:139, 1:140, 1:141, 1:142, 1:143, 1:144, 1:145, 1:146, 1:147, 1:148, 1:149, 1:150, 1:151, 1:152, 1:153, 1:154, 1:155, 1:156, 1:157, 1:158, 1:159, 1:160, 1:161, 1:162, 1:163, 1:164, 1:165, 1:166, 1:167, 1:168, 1:169, 1:170, 1:171, 1:172, 1:173, 1:174, 1:175, 1:176, 1:177, 1:178, 1:179, 1:180, 1:181, 1:182, 1:183, 1:184, 1:185, 1:186, 1:187, 1:188, 1:189, 1:190, 1:191, 1:192, 1:193, 1:194, 1:195, 1:196, 1:197, 1:198, 1:199, 1:200]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNFC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNFB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMDCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNFD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR1" registerAlias="PR"/>
         <value>9999</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSource"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="CMP1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR3" settingAlias="TCKI1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_FBDIVISOR"/>
         <value>1:125</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB9" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP7MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR12" settingAlias="RP56R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNFA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST" alias="1:4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST" alias="1:5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST" alias="1:2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST" alias="1:3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNDIISRFunction"/>
         <value>ISR_Pin Module_CNDI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST" alias="1:6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST" alias="1:7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR21"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS131072"/>
         <value>17408</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR7" settingAlias="RP46R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMT" settingAlias="DMTDIS"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR20"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="SPI3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="DMTMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="VREGS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.977%"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="USEDMT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR12" settingAlias="PCI9R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNCIISRFunction"/>
         <value>ISR_Pin Module_CNCI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST" alias="1:1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="JTAGEN" alias="ON"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.195%"/>
         <value>42</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR26"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="FOSC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.140%"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.217%"/>
         <value>60</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR15" settingAlias="QEIHOM1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FSEC"/>
         <value>36847</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS" alias="STNDRD"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP8MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR23"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR22"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="VCODIV" alias="FVCO"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR6" settingAlias="TCKI4R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="ON"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="VREGS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR29"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS" alias="FOSC"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="CMP2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockChange"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR27"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR27" settingAlias="U3DSRR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS32768"/>
         <value>15360</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="AVCODIV" alias="FVCO"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.054%"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureVcoDivider"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="CLKSEL"/>
         <value>SYSCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP39R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.683%"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet AVSSA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SMBEN" alias="STANDARD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="ENAPLL"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA4" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNCOND"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name NMCLR"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet NMCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNCONC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FPOR"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV"/>
         <value>65</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllPrescaler"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.489%"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNCONB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP9MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="FVCO"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNCONA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA3"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="callBackRate"/>
         <value>0.0001</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS128"/>
         <value>7168</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="90"/>
         <value>90</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="93"/>
         <value>93</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="94"/>
         <value>94</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="91"/>
         <value>91</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Request Switch"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="92"/>
         <value>92</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="86"/>
         <value>86</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="87"/>
         <value>87</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="84"/>
         <value>84</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="85"/>
         <value>85</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP36R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="88"/>
         <value>88</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="89"/>
         <value>89</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc AVDDA"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FOSC"/>
         <value>7491</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSELA4"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="RUNDIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.412%"/>
         <value>38</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="97"/>
         <value>97</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="98"/>
         <value>98</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="95"/>
         <value>95</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="96"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="99"/>
         <value>99</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.706%"/>
         <value>51</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllTwoStagePostScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="71"/>
         <value>71</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="LPRC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="72"/>
         <value>72</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="70"/>
         <value>70</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="64"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="65"/>
         <value>65</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="62"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="63"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="68"/>
         <value>68</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="69"/>
         <value>69</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="66"/>
         <value>66</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="67"/>
         <value>67</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="82"/>
         <value>82</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR48" settingAlias="U1CTSR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="83"/>
         <value>83</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="80"/>
         <value>80</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="81"/>
         <value>81</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="75"/>
         <value>75</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="76"/>
         <value>76</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="73"/>
         <value>73</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="74"/>
         <value>74</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="79"/>
         <value>79</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="77"/>
         <value>77</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="78"/>
         <value>78</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD"/>
         <value>200</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSYNC"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_POSTSCALER_FREQUENCY"/>
         <value>500000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="50"/>
         <value>50</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="42"/>
         <value>42</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="43"/>
         <value>43</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="40"/>
         <value>40</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="41"/>
         <value>41</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="46"/>
         <value>46</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="47"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="44"/>
         <value>44</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="45"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="48"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="49"/>
         <value>49</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONH" settingAlias="RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="60"/>
         <value>60</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="61"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR9" settingAlias="TCKI7R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="53"/>
         <value>53</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="54"/>
         <value>54</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="51"/>
         <value>51</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="52"/>
         <value>52</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="57"/>
         <value>57</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="58"/>
         <value>58</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="55"/>
         <value>55</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR29" settingAlias="SCK3R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="56"/>
         <value>56</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="59"/>
         <value>59</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR47" settingAlias="CLCINDR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center frequency"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="FOSC/2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSELB0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR43" settingAlias="PCI15R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="20"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="21"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="24"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="25"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="22"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="23"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="28"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="29"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="26"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="27"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="CLKSEL" alias="FRC"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="31"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="32"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="30"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="35"/>
         <value>35</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="36"/>
         <value>36</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="33"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="34"/>
         <value>34</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="39"/>
         <value>39</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="37"/>
         <value>37</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="38"/>
         <value>38</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDD" settingAlias="CNPDD15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CRCMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS" alias="HIGH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="QEI2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="BFRC"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC6" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="17"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="18"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="16"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="19"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0D" settingAlias="CNIE0D7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name AVSSA"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="I2C2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.489%"/>
         <value>55</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR13" settingAlias="RP58R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="AIVTDIS" alias="OFF"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1D" settingAlias="CNIE1D14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC7" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR6" settingAlias="RP44R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="20"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="21"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="22"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="16"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="17"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="18"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="19"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="TimerPeriod"/>
         <value>1.000ms</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="200"/>
         <value>200</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS1048576"/>
         <value>20480</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="40"/>
         <value>40</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="41"/>
         <value>41</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="42"/>
         <value>42</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="43"/>
         <value>43</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="44"/>
         <value>44</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="34"/>
         <value>34</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="35"/>
         <value>35</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR33"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="36"/>
         <value>36</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="37"/>
         <value>37</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="prescaleDivisor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="38"/>
         <value>38</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="39"/>
         <value>39</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Maximum frequency deviation"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="OPAMPMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="8"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="30"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="31"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="32"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="33"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="23"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="24"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="25"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="26"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RPCON" settingAlias="IOLOCK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="27"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="28"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="29"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR32"/>
         <value>65280</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="60"/>
         <value>60</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="61"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="62"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="63"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="64"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR21" settingAlias="SS1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="65"/>
         <value>65</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="66"/>
         <value>66</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="56"/>
         <value>56</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="57"/>
         <value>57</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="58"/>
         <value>58</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="59"/>
         <value>59</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR11" settingAlias="OCFAR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureIESOUpdate"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="QEIMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="50"/>
         <value>50</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="51"/>
         <value>51</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="52"/>
         <value>52</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="53"/>
         <value>53</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="54"/>
         <value>54</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="55"/>
         <value>55</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="45"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="46"/>
         <value>46</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="47"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="48"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="49"/>
         <value>49</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR38"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="80"/>
         <value>80</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="81"/>
         <value>81</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="82"/>
         <value>82</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="83"/>
         <value>83</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="84"/>
         <value>84</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="85"/>
         <value>85</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="86"/>
         <value>86</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="87"/>
         <value>87</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="88"/>
         <value>88</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="78"/>
         <value>78</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="79"/>
         <value>79</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR37"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="70"/>
         <value>70</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="71"/>
         <value>71</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="72"/>
         <value>72</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR14" settingAlias="RP61R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="73"/>
         <value>73</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="74"/>
         <value>74</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="75"/>
         <value>75</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOTRIMH" settingAlias="ROTRIM"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="76"/>
         <value>76</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FICD" settingAlias="JTAGEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="77"/>
         <value>77</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="67"/>
         <value>67</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="68"/>
         <value>68</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="69"/>
         <value>69</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV"/>
         <value>FRC/1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.249%"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C3"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN0A"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VDD3A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS65536"/>
         <value>16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="90"/>
         <value>90</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="91"/>
         <value>91</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="92"/>
         <value>92</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="93"/>
         <value>93</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="94"/>
         <value>94</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="95"/>
         <value>95</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="96"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN0B"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="97"/>
         <value>97</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="98"/>
         <value>98</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="99"/>
         <value>99</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV" alias="89"/>
         <value>89</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="FVCO/3"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="FVCO/4"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="DMT" registerAlias="DMTCON" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="FVCO/2"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VDD4A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllClock"/>
         <value>400000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR44" settingAlias="SENT1R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="NONE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN0C"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR21" settingAlias="REFOIR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.054%"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C2"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN0D"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BISTDIS"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePoscErrataWorkaround"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C1"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.923%"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="CLKSEL" alias="LPRC"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.977%"/>
         <value>46</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DMA2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16384"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="REFCLKI"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="QEIMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="clockSourceSelect"/>
         <value>CLOCK_LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TMWIP" alias="Write pending"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC"/>
         <value>FRCPLL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VDD1A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="PRWIP" alias="Write pending"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VDD2A"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON"/>
         <value>33025</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR7"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="ENAPLL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllPostscaler"/>
         <value>1:4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP5MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR6"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TGATE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscalerClock"/>
         <value>400000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR5"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR18" settingAlias="U1DSRR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SMBEN"/>
         <value>SMBUS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR9"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="RESET" registerAlias="RCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="requestedPeriod"/>
         <value>0.00000002</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.249%"/>
         <value>41</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:64"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR8"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR19" settingAlias="RP71R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKSEL" alias="No Clock Selected"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP34R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR2"/>
         <value>65280</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CRCMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BISTDIS" alias="DISABLED"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_PLL_ENABLE"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR1"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_POSTSCALER2"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TGATE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockFBDivisor"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPrescalerOptions"/>
         <value>[1:1]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR23" settingAlias="SS2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR4"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR3"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllPostScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR8" settingAlias="RP49R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="ENAPLL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP5MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR42" settingAlias="PCI13R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR0"/>
         <value>65280</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCONH" settingAlias="WDTCLRKEY"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.543%"/>
         <value>54</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV"/>
         <value>200</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS512"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.434%"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockChange"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR30"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="STNDRD"/>
         <value>3072</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="WDTWINEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATD" settingAlias="CNSTATD0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLDIV1" settingAlias="AVCODIV"/>
         <value>FVCO/4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AFVCOFreq"/>
         <value>1000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUD" settingAlias="CNPUD15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS524288"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV"/>
         <value>12289</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="CNSTYLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR46" settingAlias="CLCINCR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CRCMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="PMPMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR49"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.869%"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR48"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC6"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR10" settingAlias="TCKI8R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP5MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FICD"/>
         <value>32770</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR47"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR46"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.086%"/>
         <value>44</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLCK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FVCODIV"/>
         <value>FVCO/4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_POSTSCALER"/>
         <value>1:2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC"/>
         <value>FRCPLL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC7"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR20"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR13" settingAlias="PCI10R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR4" settingAlias="TCKI2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.109%"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="PLLPOST"/>
         <value>1:4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TMR" settingAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc AVSSA"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR21"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="timerMaxCount"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR15" settingAlias="RP63R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="TimerFrequency"/>
         <value>100000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="DMTMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="CNSTYLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR22"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="PRWIP" alias="Write complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR5" settingAlias="RP42R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:256"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="BIASMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR23"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR9"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BISTDIS" alias="ENABLED"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="DMTMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAutoTune"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS524288"/>
         <value>19456</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR8"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR19" settingAlias="U2DSRR"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="U3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="DMT" registerAlias="DMTCON" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR7"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TMWDIS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR6"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TMWDIS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="PRWIP"/>
         <value>Write complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_DIVSWITCH"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 104"/>
         <value>103</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 105"/>
         <value>104</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 106"/>
         <value>105</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 107"/>
         <value>106</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 108"/>
         <value>107</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 109"/>
         <value>108</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 100"/>
         <value>99</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 101"/>
         <value>100</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 102"/>
         <value>101</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 103"/>
         <value>102</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.380%"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 115"/>
         <value>114</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 116"/>
         <value>115</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 117"/>
         <value>116</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 118"/>
         <value>117</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 119"/>
         <value>118</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 110"/>
         <value>109</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 111"/>
         <value>110</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 112"/>
         <value>111</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR1" settingAlias="INT3R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 113"/>
         <value>112</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCONL" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 114"/>
         <value>113</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 126"/>
         <value>125</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 127"/>
         <value>126</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 128"/>
         <value>127</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 120"/>
         <value>119</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="FRCSEL"/>
         <value>FRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 121"/>
         <value>120</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 122"/>
         <value>121</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 123"/>
         <value>122</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 124"/>
         <value>123</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="ACLKCON" settingAlias="APLLCK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CANCLKCON" settingAlias="CANCLKDIV" alias="Divide by 125"/>
         <value>124</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FailSafe"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSwitching"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_LPRC"/>
         <value>32000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS" alias="DISABLED"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTIVTL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllDisplayScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR19"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="in lock"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR8" settingAlias="ICM6R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ICD" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR16" settingAlias="QEIA2R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTCNTH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP37R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AUXCLK_FBDIVISOR_FREQUENCY"/>
         <value>1000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UI_OSCTUN_SETTING"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFD" settingAlias="CNFD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="196"/>
         <value>196</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="197"/>
         <value>197</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="194"/>
         <value>194</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="195"/>
         <value>195</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT4" alias="OFF"/>
         <value>28672</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="198"/>
         <value>198</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="199"/>
         <value>199</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCOND" settingAlias="CNSTYLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="192"/>
         <value>192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="193"/>
         <value>193</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="190"/>
         <value>190</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR5"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="191"/>
         <value>191</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.303%"/>
         <value>40</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_INPUT_FREQUENCY"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="174"/>
         <value>174</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="175"/>
         <value>175</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="172"/>
         <value>172</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="173"/>
         <value>173</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="178"/>
         <value>178</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="179"/>
         <value>179</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="176"/>
         <value>176</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="177"/>
         <value>177</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet NMCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="TCKI5R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="170"/>
         <value>170</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="171"/>
         <value>171</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODCD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="185"/>
         <value>185</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="customFDMTCNT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="186"/>
         <value>186</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="183"/>
         <value>183</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SMBEN" alias="SMBUS"/>
         <value>1024</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="184"/>
         <value>184</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet AVSSA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="189"/>
         <value>189</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.303%"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTCNTL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="187"/>
         <value>187</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="188"/>
         <value>188</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS262144"/>
         <value>18432</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCOND" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscaler2Clock"/>
         <value>400000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="181"/>
         <value>181</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="182"/>
         <value>182</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="180"/>
         <value>180</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="152"/>
         <value>152</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="153"/>
         <value>153</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="150"/>
         <value>150</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="151"/>
         <value>151</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="156"/>
         <value>156</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="157"/>
         <value>157</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="154"/>
         <value>154</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="155"/>
         <value>155</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR7" settingAlias="RP47R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="158"/>
         <value>158</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="159"/>
         <value>159</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FBSLIM" settingAlias="BSLIM"/>
         <value>8191</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="AFVCODIVFreq"/>
         <value>250000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="163"/>
         <value>163</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="164"/>
         <value>164</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="timerBitMode"/>
         <value>16 Bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="161"/>
         <value>161</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="162"/>
         <value>162</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="167"/>
         <value>167</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="168"/>
         <value>168</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="165"/>
         <value>165</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="166"/>
         <value>166</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="169"/>
         <value>169</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.086%"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC0"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="160"/>
         <value>160</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="130"/>
         <value>130</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc NMCLR"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="131"/>
         <value>131</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="134"/>
         <value>134</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="135"/>
         <value>135</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="132"/>
         <value>132</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="133"/>
         <value>133</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="138"/>
         <value>138</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCONL" settingAlias="ROSEL" alias="Primary Oscillator"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="139"/>
         <value>139</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="136"/>
         <value>136</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="137"/>
         <value>137</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCOND" settingAlias="CNSTYLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="C1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="141"/>
         <value>141</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="142"/>
         <value>142</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="140"/>
         <value>140</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="145"/>
         <value>145</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="146"/>
         <value>146</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="143"/>
         <value>143</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="144"/>
         <value>144</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="149"/>
         <value>149</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC1"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="147"/>
         <value>147</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="148"/>
         <value>148</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP32R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllDivisor"/>
         <value>1:200</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="CM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="112"/>
         <value>112</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="113"/>
         <value>113</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="110"/>
         <value>110</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="111"/>
         <value>111</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="116"/>
         <value>116</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="117"/>
         <value>117</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="C1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="114"/>
         <value>114</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="115"/>
         <value>115</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="118"/>
         <value>118</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="119"/>
         <value>119</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TMWIP"/>
         <value>Write complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR45"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="120"/>
         <value>120</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="123"/>
         <value>123</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="124"/>
         <value>124</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="121"/>
         <value>121</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="122"/>
         <value>122</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="127"/>
         <value>127</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="128"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="125"/>
         <value>125</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="CM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="126"/>
         <value>126</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="129"/>
         <value>129</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR44"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Minimum frequency deviation"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTIVTH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet AVDDA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP6MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR43"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC"/>
         <value>200000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR5" settingAlias="ICM3R"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELC" settingAlias="ANSELC3"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="101"/>
         <value>101</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="102"/>
         <value>102</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="100"/>
         <value>100</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="105"/>
         <value>105</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="106"/>
         <value>106</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLDIV" settingAlias="VCODIV"/>
         <value>FVCO/4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="103"/>
         <value>103</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="104"/>
         <value>104</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="109"/>
         <value>109</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="107"/>
         <value>107</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="APLLFBD1" settingAlias="APLLFBDIV" alias="108"/>
         <value>108</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR42"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdateAuxPrescalerOptions"/>
         <value>[1:1]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TON" alias="enabled"/>
         <value>1</value>
      </entry>
   </tokenMap>
   <generatedFileHashHistoryMap class="java.util.HashMap">
      <entry>
         <file>mcc_generated_files\interrupt_manager.h</file>
         <hash>d413dcac145cc053f9bd2613ef10cba8ac3f0c6daeed38e49cfcadb2170edf47</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.h</file>
         <hash>da11287b3388692edf3d6f8bc0480caf872dee4057749d4c81df8faf03235ba1</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\reset.c</file>
         <hash>3dabec70cc85e6370d989b33443322a05710788c1be70b9acf17bb115f3bdf60</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr1.h</file>
         <hash>b8500e8102a469e585b8da67c2ee03087703cc8a096c7d6253b0dab875f93d7a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.c</file>
         <hash>ff663546bd7d3b2fed558974e75e38d84a14d6bd3f5101d19ef82962cec27ccb</hash>
      </entry>
      <entry>
         <file>main.c</file>
         <hash>add4c1193de9b694593516452ab9d015afe3d5f2f578827a2b55dbd74ebc707f</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.h</file>
         <hash>783790dffb49c792c6fd7632d61bf128852b21c0983f96b00aa391c4c0672e80</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr1.c</file>
         <hash>bf85d4b00773f8d8ed8ab40996faf39952d1805473da32a6661ede1f8ee6e98e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system_types.h</file>
         <hash>5a950eea332589ea6dc66ce9c8aaf27ccaaf2623159a9deaed042055e43c9477</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.c</file>
         <hash>7a64d50b1ff548dc0574f61ded05cb96c27256f7cee6a36fde3b11589b3d9b19</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.h</file>
         <hash>0060fe1fb7298b89c45e013f472a9f4b996184788e2fd4462bf321204ae5163c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.c</file>
         <hash>6786bb8f8ac98a175fa85d7b2389824ac0c37afac965497d53c174820cd29422</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.c</file>
         <hash>cd1b39611258f57371c0aab4cafd68402ef27958b96556ed11638fddf5fc5823</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.h</file>
         <hash>797d91b4866aede3314d66157389699c4119592fa1dc207ac146e0f1f59ba962</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.h</file>
         <hash>67e0b39105fa38a93489aa8dbd59ed289b0d4de610d90d506816d4df1e40e1fa</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\interrupt_manager.c</file>
         <hash>9d43d2327981dd19bf9561d87a9f483b1cc732eb18b85fa762853739c732fa24</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.c</file>
         <hash>23db5b8bbea73f565ab575b145ca07d44d368ec2d7396339bffa729199f90a5e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\reset.h</file>
         <hash>df9c4059c6da70ba157fbfb716835f9253f0c2f16c98c935113c05270e1aa7ab</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\watchdog.h</file>
         <hash>f38cea8509b11e3d7db0337e3b756aaf12217ba5246cb28e732c2a4bf921325d</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\reset_types.h</file>
         <hash>5eaa92f05b14ab22d7298ad9a55b20899d0622f769ec4236335aceefa76eca99</hash>
      </entry>
   </generatedFileHashHistoryMap>
   <mc3libFileHashHistoryMap class="java.util.HashMap"/>
</config>