(Maximum) number of stages
==========================

For a multi-stage design, **multiarm** requires a value for the allowed
(maximum, in the case of a group-sequential design) number of stages,
*J*. Specify your chosen (maximum) number of stages here.
