0 MIPS
Downloading `nothing`

##### Memory

RAM size Megabytes of memory allocated to guest
Video RAM size Megabytes of video memory

##### ROM Images

BIOS image Loads `bios.img` by default. Clear
Video BIOS Loads `vgabios.img` by default. Clear

##### Devices

PCI If checked, simulate a PC with a PCI adapter. Otherwise, simulates an ISA system.
PCI VGA controller Connect the VGA display adapter to the PCI bus. Allows some systems (like ReactOS) to detect more video modes, but is slow and incomplete.
APIC An APIC is integrated with almost every CPU that Halfix can emulate. Should only be disabled if you know what you're doing.
ACPI Required by newer operating systems for timing.
Floppy disk controller Supports the bare minimum of features. Buggy and incomplete.

##### Drives

###### Drive type

Disk image Images are not uploaded to server. Clear

##### Other Settings

Turbo mode If checked, the emulator runs as fast as possible, causing time to become desynchronized.
Work around Windows NT CPUID bug If checked, the reported CPUID level is set to 2. Other functionality isn't compromised.