adc=
adcs=
add11=
add=
addc=
ads=
adx=add immediate value to ACC, skip next on carry
atbp=
atf=output ACC to F
atfc=
atl=
atpl=
atr=
ats=
atx=
bdc=
blta=
cctrl=
cend=
clkhi=
clklo=
comcb=
comcn=
debl=
debm=
decb=
dr=
dta=transfer 1/100s counter to ACC
dtw=
exax=
exbl=
exbla=
exc=
excd=
exci=
exkfa=
exksa=
idiv=reset divider and 1s counter
inbl=
inbm=
incb=
inis=reset 1/100s counter (10ms)
keta=input KE to ACC
kta=
lax=
lb=load BM/BL with 4-bit immediate value (partial)
lbl=load BL
lblx=load BL with 4 bit immediate value
lbmx=load BM with 4 bit immediate value
lda=
mtr=
nop=do nothing
pdtw=
pre=
ptw=
rbm=
rds=reset display enable
rm=
rme=
rmf=
rta=
rtn0=return 0
rtn1=return 1
rtn=return
rtns=return from subroutine
sabl=
sabm=
sbm=
sds=set display enable
skip=
sm=
sme=
smf=
ssr=
str=
t=
ta0=
ta=
tabl=
tal=
tam=
tax=
tb=
tba=
tba=
tc=
tf1=
tf4=
tg=skip next if gamma flag is set, reset it after
tis=
tl=
tls=
tm=
tmel=
tml=
tr=
trs=indirect subroutine call
tw=
wr=
ws=
xbla=
