add comment;?i Comment;CC `ys`
list comments;CC;?ik
change block size;?i block size;b `ys`
analyze all;aa
analyze function;af
analyze preludes;ap
continue process execution;dc;?i
disable colors;e scr.color=0
enable colors (ANSI 16);e scr.color=1
enable colors (256);e scr.color=2
enable colors (16M);e scr.color=3
randomize colors;ecr
hide bytes in disassembly;e asm.bytes=false
show bytes in disassembly;e asm.bytes=true
list imports ;ii;?ik
list sections;iS;?ik
list symbols;is;?ik
list processes;dp*;?ik
run command;?i cmd;`ys`;?ik
seek to entrypoint;s entry0
seek to main;s main
set breakpoint;db;?i new breakpoint address;db `ys`
remove breakpoint ?i delete breakpoint at given address;db-`ys`
show backtrace;dbt;?ik
show bytes in disassembly;e asm.bytes=1
show debugger register values;dr;?ik
show process memory maps;dm;?ik
step instruction;sr PC;pd 1;ds;?ik
step over call;sr PC;pd 1;dso;?ik
write string;?i string;w `ys`
write hexadecimal data in current offset;?i hexpairs;wx `ys`
xor current block with hexpair key;?i hexpair key;wox `ys`
edit eval configuration;Veq
calculator;?i enter math expression;? `ys`;?ik
disassemble 1024 bytes and pipe to less(1);b 1024;pd|less -R
rename function;?i New name;afn `ys`
set flag;?i Flag name;f `ys`
unset flag;?i Flag name to delete;f-`ys`
