
# CR-10S-TH3DFW-Creality ABL


**Table of Contents**

<!-- TOC depthFrom:2 -->

- [CR-10S-TH3DFW-Creality ABL](#cr-10s-th3dfw-creality-abl)
- [BEFORE READING](#before-reading)
- [1.Supported-Model](#supported-model)
- [2. Tested Model](#tested-model)
- [3. How To Flash](#how-to-flash)
- [4. What's New?](#whats-new)

<!-- /TOC -->

## BEFORE READING

Warning!! THIS IS NOT OFFICIAL FIRMWARE BE AWARE OF FLASHING AT YOUR OWN RISK 
------------

## Supported Model

- Creality CR-10S 300X300
- Creality CR-10S 400X400
- Creality CR-10S 500X500


------------


### Tested Model

- Creality CR-10S 300X300

------------

### How To Flash
- 1.Get your printer's Firmware HEX file in [Releases](https://github.com/rlatn1234/CR-10S-TH3DFW-CrealityABL/releases) page.
- 2.Flash your firmware to your printer by Cura or another programs.
- 3.Enjoy your Creality ABL sensor with CR-10S


------------

### What's New?
- New Z offset animation
