Overview
--------
The LS1043A Development System (QDS) is a high-performance computing,
evaluation, and development platform that supports the QorIQ LS1043A
LayerScape Architecture processor. The LS1043AQDS provides SW development
platform for the Freescale LS1043A processor series, with a complete
debugging environment.

LS1043A SoC Overview
--------------------
Please refer arch/arm/cpu/armv8/fsl-layerscape/doc/README.soc for LS1043A
SoC overview.

 LS1043AQDS board Overview
 -----------------------
 - SERDES Connections, 4 lanes supporting:
      - PCI Express - 3.0
      - SGMII, SGMII 2.5
      - QSGMII
      - SATA 3.0
      - 10GBase-R
 - DDR Controller
     - 2GB 40bits (8-bits ECC) DDR4 SDRAM. Support rates of up to 1600MT/s
 -IFC/Local Bus
    - One in-socket 128 MB NOR flash 16-bit data bus
    - One 512 MB NAND flash with ECC support
    - PromJet Port
    - FPGA connection
 - USB 3.0
    - Three high speed USB 3.0 ports
    - First USB 3.0 port configured as Host with Type-A connector
    - The other two USB 3.0 ports configured as OTG with micro-AB connector
 - SDHC port connects directly to an adapter card slot, featuring:
    - Optional clock feedback paths, and optional high-speed voltage translation assistance
    - SD slots for SD, SDHC (1x, 4x, 8x), and/or MMC
    - eMMC memory devices
 - DSPI: Onboard support for three SPI flash memory devices
 - 4 I2C controllers
 - One SATA onboard connectors
 - UART
   - Two 4-pin serial ports at up to 115.2 Kbit/s
   - Two DB9 D-Type connectors supporting one Serial port each
 - ARM JTAG support

Memory map from core's view
----------------------------
Start Address	End Address	Description		Size
0x00_0000_0000	0x00_000F_FFFF	Secure Boot ROM		1MB
0x00_0100_0000	0x00_0FFF_FFFF	CCSRBAR			240MB
0x00_1000_0000	0x00_1000_FFFF	OCRAM0			64KB
0x00_1001_0000	0x00_1001_FFFF	OCRAM1			64KB
0x00_2000_0000	0x00_20FF_FFFF	DCSR			16MB
0x00_6000_0000	0x00_67FF_FFFF	IFC - NOR Flash		128MB
0x00_7E80_0000	0x00_7E80_FFFF	IFC - NAND Flash	64KB
0x00_7FB0_0000	0x00_7FB0_0FFF	IFC - FPGA		4KB
0x00_8000_0000	0x00_FFFF_FFFF	DRAM1			2GB

Booting Options
---------------
a) Promjet Boot
b) NOR boot
c) NAND boot
d) SD boot
e) QSPI boot
