.. SPDX-License-Identifier: GPL-2.0+

U-Boot for ODROID-C4
====================

ODROID-C4 is a single board computer manufactured by Hardkernel
Co. Ltd with the following specifications:

 - Amlogic S905X3 Arm Cortex-A55 quad-core SoC
 - 4GB DDR4 SDRAM
 - Gigabit Ethernet
 - HDMI 2.1 display
 - 40-pin GPIO header
 - 4x USB 3.0 Host
 - 1x USB 2.0 Host/OTG (micro)
 - eMMC, microSD
 - UART serial
 - Infrared receiver

The ODROID-HC4 is a variant with a PCIe-SATA controller, the same commands
applies for HC4.

Schematics are available on the manufacturer website.

U-Boot compilation
------------------

.. code-block:: bash

    $ export CROSS_COMPILE=aarch64-none-elf-
    $ make odroid-c4_defconfig
    $ make

Image creation
--------------

For simplified usage, pleaser refer to :doc:`pre-generated-fip` with codename `odroid-c4` or `odroid-hc4`

Amlogic doesn't provide sources for the firmware and for tools needed
to create the bootloader image, so it is necessary to obtain them from
the git tree published by the board vendor:

.. code-block:: bash

    $ wget https://releases.linaro.org/archive/13.11/components/toolchain/binaries/gcc-linaro-aarch64-none-elf-4.8-2013.11_linux.tar.xz
    $ wget https://releases.linaro.org/archive/13.11/components/toolchain/binaries/gcc-linaro-arm-none-eabi-4.8-2013.11_linux.tar.xz
    $ tar xvfJ gcc-linaro-aarch64-none-elf-4.8-2013.11_linux.tar.xz
    $ tar xvfJ gcc-linaro-arm-none-eabi-4.8-2013.11_linux.tar.xz
    $ export PATH=$PWD/gcc-linaro-aarch64-none-elf-4.8-2013.11_linux/bin:$PWD/gcc-linaro-arm-none-eabi-4.8-2013.11_linux/bin:$PATH

    $ DIR=odroid-c4
    $ git clone --depth 1 \
       https://github.com/hardkernel/u-boot.git -b odroidg12-v2015.01 \
       $DIR

    $ cd odroid-c4
    $ make odroidc4_defconfig
    $ make
    $ export UBOOTDIR=$PWD

Go back to mainline U-Boot source tree then :

.. code-block:: bash

    $ mkdir fip

    $ wget https://github.com/BayLibre/u-boot/releases/download/v2017.11-libretech-cc/blx_fix_g12a.sh -O fip/blx_fix.sh
    $ cp $UBOOTDIR/build/scp_task/bl301.bin fip/
    $ cp $UBOOTDIR/build/board/hardkernel/odroidc4/firmware/acs.bin fip/
    $ cp $UBOOTDIR/fip/g12a/bl2.bin fip/
    $ cp $UBOOTDIR/fip/g12a/bl30.bin fip/
    $ cp $UBOOTDIR/fip/g12a/bl31.img fip/
    $ cp $UBOOTDIR/fip/g12a/ddr3_1d.fw fip/
    $ cp $UBOOTDIR/fip/g12a/ddr4_1d.fw fip/
    $ cp $UBOOTDIR/fip/g12a/ddr4_2d.fw fip/
    $ cp $UBOOTDIR/fip/g12a/diag_lpddr4.fw fip/
    $ cp $UBOOTDIR/fip/g12a/lpddr3_1d.fw fip/
    $ cp $UBOOTDIR/fip/g12a/lpddr4_1d.fw fip/
    $ cp $UBOOTDIR/fip/g12a/lpddr4_2d.fw fip/
    $ cp $UBOOTDIR/fip/g12a/piei.fw fip/
    $ cp $UBOOTDIR/fip/g12a/aml_ddr.fw fip/
    $ cp u-boot.bin fip/bl33.bin

    $ sh fip/blx_fix.sh \
    	fip/bl30.bin \
    	fip/zero_tmp \
    	fip/bl30_zero.bin \
    	fip/bl301.bin \
    	fip/bl301_zero.bin \
    	fip/bl30_new.bin \
    	bl30

    $ sh fip/blx_fix.sh \
    	fip/bl2.bin \
    	fip/zero_tmp \
    	fip/bl2_zero.bin \
    	fip/acs.bin \
    	fip/bl21_zero.bin \
    	fip/bl2_new.bin \
    	bl2

    $ $UBOOTDIR/fip/g12a/aml_encrypt_g12a --bl30sig --input fip/bl30_new.bin \
    					--output fip/bl30_new.bin.g12a.enc \
    					--level v3
    $ $UBOOTDIR/fip/g12a/aml_encrypt_g12a --bl3sig --input fip/bl30_new.bin.g12a.enc \
    					--output fip/bl30_new.bin.enc \
    					--level v3 --type bl30
    $ $UBOOTDIR/fip/g12a/aml_encrypt_g12a --bl3sig --input fip/bl31.img \
    					--output fip/bl31.img.enc \
    					--level v3 --type bl31
    $ $UBOOTDIR/fip/g12a/aml_encrypt_g12a --bl3sig --input fip/bl33.bin --compress lz4 \
    					--output fip/bl33.bin.enc \
    					--level v3 --type bl33 --compress lz4
    $ $UBOOTDIR/fip/g12a/aml_encrypt_g12a --bl2sig --input fip/bl2_new.bin \
    					--output fip/bl2.n.bin.sig
    $ $UBOOTDIR/fip/g12a/aml_encrypt_g12a --bootmk \
    		--output fip/u-boot.bin \
    		--bl2 fip/bl2.n.bin.sig \
    		--bl30 fip/bl30_new.bin.enc \
    		--bl31 fip/bl31.img.enc \
    		--bl33 fip/bl33.bin.enc \
    		--ddrfw1 fip/ddr4_1d.fw \
    		--ddrfw2 fip/ddr4_2d.fw \
    		--ddrfw3 fip/ddr3_1d.fw \
    		--ddrfw4 fip/piei.fw \
    		--ddrfw5 fip/lpddr4_1d.fw \
    		--ddrfw6 fip/lpddr4_2d.fw \
    		--ddrfw7 fip/diag_lpddr4.fw \
    		--ddrfw8 fip/aml_ddr.fw \
    		--ddrfw9 fip/lpddr3_1d.fw \
    		--level v3

and then write the image to SD with:

.. code-block:: bash

    $ DEV=/dev/your_sd_device
    $ dd if=fip/u-boot.bin.sd.bin of=$DEV conv=fsync,notrunc bs=512 skip=1 seek=1
    $ dd if=fip/u-boot.bin.sd.bin of=$DEV conv=fsync,notrunc bs=1 count=444
