Main features of EasyMesh:

- Generates two dimensional, unstructured, Delaunay and constrained Delaunay triangulations in general domains.
- Handles holes in the domain.
- Local refining/coarsening can be achieved easily with different techniques.
- Handles domains composed of more than one material.
- Performs renumeration of nodes, elements and sides in order to decrease the bandwidth of discretized set of equations (wherever you place the unknowns). This renumeration is invoked by default, and cannot be switched off by the command line option.
- Has a built-in function for relaxation of grid, in order to avoid the creation of nodes surrounded with more than 7 and less than 5 elements. The result of this technique, combined with Laplacian smoothing, is a grid of high quality.
- Performs Laplacian smoothing.
- Uses very simple ASCII file as input.
- Creates three different ASCII output files with all the data which a numerical analysist might need.
- If specified by a command line switch, creates a drawing with Delaunay and Voronoi mesh in DXF or `fig` format, so the results of triangulation can be viewed with any graphical tool which supports these formats.

Return to EasyMesh home page.

niceno@univ.trieste.it