iir1

List of all members
Iir::LowPassTransform Class Reference

`#include <PoleFilter.h>`

## Detailed Description

s-plane to z-plane transforms

For pole filters, an analog prototype is created via placement of poles and zeros in the s-plane. The analog prototype is either a halfband low pass or a halfband low shelf. The poles, zeros, and normalization parameters are transformed into the z-plane using variants of the bilinear transformation. low pass to low pass

The documentation for this class was generated from the following files:

- iir/PoleFilter.h
- iir/PoleFilter.cpp