    /*
     * Only necessary when no IMEI device (with any name) is present in the DSDT and a custom device-id
     * is needed to be set via DeviceProperties (some Sandy Bridge or Ivy Bridge configurations).
     */
    DefinitionBlock ("", "SSDT", 2, "ACDT", "IMEI", 0x00000000)
    {
        External (_SB_.PCI0, DeviceObj)

        Scope (_SB.PCI0)
        {
            Device (IMEI)
            {
                Name (_ADR, 0x00160000)  // _ADR: Address
            }
        }
    }

# results matching ""

# No results matching ""