    // PCI0.LPCB-AOACWake
    //
    DefinitionBlock("", "SSDT", 2, "ACDT", "AOACWake", 0)
    {
        External(_SB.PCI0.LPCB, DeviceObj)
        External(_WAK, MethodObj)

        Scope (_SB.PCI0.LPCB)
        {
            If (_OSI ("Darwin"))
            {
                Method (_PS0, 0, Serialized)
                {
                    \_WAK (0x03)
                    //It is possible to customize the power data recovery method
                }

                Method (_PS3, 0, Serialized)
                {

                }
            }
        }
    }
    //EOF

# results matching ""

# No results matching ""