GNU ARM Eclipse plug-ins v1.1.7-201312221905 released | web-jekyll

# GNU ARM Eclipse plug-ins v1.1.7-201312221905 released

Dec 22, 2013 / Liviu Ionescu / gnu, arm, eclipse, segger, j-link, debugging, plug-in

The main change is the addition of the J-Link debugging plug-in, that supports the SEGGER J-Link JTAG/SWD probe, including extra features, like transparent integration of the GDB server, integration of the Serial Wire Viewer (SWV) window as a standard Eclipse console, a functional restart button, and more.

Binary files »

New features:

- [feature-request:#23] the echo command was added to the Cross Build Tools archive to prevent the missing command error that affected the Windows versions of the plug-in when new projects were created
- [feature-request:#22] the STM32F4 template automatically sets the PLL_M definition as HSE_VALUE/1000000.

Bugs fixed:

- [support-requests:#33] the STM32F4 template use of FMC/FSMC was fixed.

Other changes:

- the STM32F4 template includes a conditional definition for Olimex STM32-E407 green led.

Edit