| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Microcontroller Abstraction
Hardware Abstraction Layer » Temperature Feedback

Device analog input pin, register and interrupt vector assignments of temperature feedback signal(s) More...

Collaboration diagram for Microcontroller Abstraction:

#define | _TEMP_ADCInterrupt _ADCAN2Interrupt
| ADC input assignments of temperature feedback signals. More...
#define | _TEMP_ADCISR_IF _ADCAN2IF
| Interrupt Service Routine Flag Bit. More...
#define | TEMP_ANSEL _ANSELB7
| GPIO analog function mode enable bit. More...
#define | TEMP_ADCCORE 8
#define | TEMP_ADCIN 2
#define | TEMP_ADCBUF ADCBUF2
| GPIO analog function mode enable bit. More...
#define | TEMP_ADCTRIG BOOST_PWM_PGxTRIGB
| Register used for trigger placement. More...
#define | TEMP_TRGSRC BOOST_PWM_TRGSRC_TRG2

## Detailed Description

Device analog input pin, register and interrupt vector assignments of temperature feedback signal(s)

## Macro Definition Documentation

## ◆ _TEMP_ADCInterrupt

#define _TEMP_ADCInterrupt _ADCAN2Interrupt

ADC input assignments of temperature feedback signals.

In this section the ADC input channels, related ADC result buffers, trigger sources and interrupt vectors are defined. These settings allow the fast re-assignments of feedback signals in case of hardware changes.Interrupt Service Routine function name

Definition at line 1576 of file dpsk3_hwdescr.h.

## ◆ _TEMP_ADCISR_IF

#define _TEMP_ADCISR_IF _ADCAN2IF

Interrupt Service Routine Flag Bit.

Definition at line 1577 of file dpsk3_hwdescr.h.

## ◆ TEMP_ADCBUF

#define TEMP_ADCBUF ADCBUF2

GPIO analog function mode enable bit.

Definition at line 1582 of file dpsk3_hwdescr.h.

## ◆ TEMP_ADCCORE

#define TEMP_ADCCORE 8

Definition at line 1580 of file dpsk3_hwdescr.h.

## ◆ TEMP_ADCIN

#define TEMP_ADCIN 2

Definition at line 1581 of file dpsk3_hwdescr.h.

## ◆ TEMP_ADCTRIG

#define TEMP_ADCTRIG BOOST_PWM_PGxTRIGB

Register used for trigger placement.

Definition at line 1583 of file dpsk3_hwdescr.h.

## ◆ TEMP_ANSEL

#define TEMP_ANSEL _ANSELB7

GPIO analog function mode enable bit.

Definition at line 1579 of file dpsk3_hwdescr.h.

## ◆ TEMP_TRGSRC

#define TEMP_TRGSRC BOOST_PWM_TRGSRC_TRG2

Definition at line 1584 of file dpsk3_hwdescr.h.