# Make

https://youtu.be/S8NppVT_paw

<br/>
Here's what you need to do to make your soil moisture sensor:

* Connect a nail to the **3V** pin with a croc clip and insert it into the soil.
* Connect the other nail to the **P0** pin with a croc clip and insert it into the soil.

That's it!

## ~button /projects/soil-moisture/code

Code

## ~
