Это автоматический перевод.

## Вставить растровое изображение…

Панель инструментов / значок:
Меню: Начертить > Вставить растровое изображение…
Ярлык: I, M
Команды: insertbitmap | bitmap | im

### Описание

Inserts a raster image (bitmap) into the drawing.
Note that the drawing file which is created when saving the drawing, contains only references to inserted images. It is recommended to keep the image file and the drawing file in the same folder, so QCAD can find the image again when the drawing file is loaded later.
Transparent backgrounds are supported for PNG images.
Note that large bitmaps can cause the drawing display to become very slow.
Usually you will want images to be in the background of other entities. Please refer to the 'Modify' - 'Send to back' tool to learn how to do this.

### Использование

1. Choose the image file which you want to insert.
2. Type a scaling factor in the options tool bar. A factor of 1.0 means that one pixel of the image will be one unit large in the drawing.
3. Type a rotation angle in the options tool bar.
4. Specify the insertion point of the image. That is the left bottom corner of the image.