v2.0.0
Public Member Functions | Data Fields
armv8m_scb_hw_t Struct Reference

## Public Member Functions
| _REG_ (M33_CPUID_OFFSET) io_ro_32 cpuid
| _REG_ (M33_ICSR_OFFSET) io_rw_32 icsr
| _REG_ (M33_VTOR_OFFSET) io_rw_32 vtor
| _REG_ (M33_AIRCR_OFFSET) io_rw_32 aircr
| _REG_ (M33_SCR_OFFSET) io_rw_32 scr
| _REG_ (M33_CCR_OFFSET) io_rw_32 ccr
| _REG_ (M33_SHPR1_OFFSET) io_rw_32 shpr[3]
| _REG_ (M33_SHCSR_OFFSET) io_rw_32 shcsr
| _REG_ (M33_CFSR_OFFSET) io_rw_32 cfsr
| _REG_ (M33_HFSR_OFFSET) io_rw_32 hfsr
| _REG_ (M33_DFSR_OFFSET) io_rw_32 dfsr
| _REG_ (M33_MMFAR_OFFSET) io_rw_32 mmfar
| _REG_ (M33_BFAR_OFFSET) io_rw_32 bfar
| _REG_ (M33_ID_PFR0_OFFSET) io_ro_32 id_pfr[2]
| _REG_ (M33_ID_DFR0_OFFSET) io_ro_32 id_dfr0
| _REG_ (M33_ID_AFR0_OFFSET) io_ro_32 id_afr0
| _REG_ (M33_ID_MMFR0_OFFSET) io_ro_32 id_mmfr[4]
| _REG_ (M33_ID_ISAR0_OFFSET) io_ro_32 id_isar[6]
| _REG_ (M33_CTR_OFFSET) io_ro_32 ctr
| _REG_ (M33_CPACR_OFFSET) io_rw_32 cpacr
| _REG_ (M33_NSACR_OFFSET) io_rw_32 nsacr

## Data Fields
uint32_t | _pad0
uint32_t | _pad1
uint32_t | _pad2 [2]

The documentation for this struct was generated from the following file:

- include/hardware/structs/scb.h