v2.0.0
sysinfo.h
1// THIS HEADER FILE IS AUTOMATICALLY GENERATED -- DO NOT EDIT
2
8#ifndef _HARDWARE_STRUCTS_SYSINFO_H
9#define _HARDWARE_STRUCTS_SYSINFO_H
10
15#include "hardware/address_mapped.h"
16#include "hardware/regs/sysinfo.h"
17
18// Reference to datasheet: https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf#tab-registerlist_sysinfo
19//
20// The _REG_ macro is intended to help make the register navigable in your IDE (for example, using the "Go to Definition" feature)
21// _REG_(x) will link to the corresponding register in hardware/regs/sysinfo.h.
22//
23// Bit-field descriptions are of the form:
24// BITMASK [BITRANGE] FIELDNAME (RESETVALUE) DESCRIPTION
25
26 typedef struct {
27 _REG_(SYSINFO_CHIP_ID_OFFSET) // SYSINFO_CHIP_ID
28 // JEDEC JEP-106 compliant chip identifier
29 // 0xf0000000 [31:28] REVISION (-)
30 // 0x0ffff000 [27:12] PART (-)
31 // 0x00000fff [11:0] MANUFACTURER (-)
32 io_ro_32 chip_id;
33
34 _REG_(SYSINFO_PLATFORM_OFFSET) // SYSINFO_PLATFORM
35 // Platform register
36 // 0x00000002 [1] ASIC (0)
37 // 0x00000001 [0] FPGA (0)
38 io_ro_32 platform;
39
40 uint32_t _pad0[2];
41
42 _REG_(SYSINFO_GITREF_RP2040_OFFSET) // SYSINFO_GITREF_RP2040
43 // Git hash of the chip source
44 // 0xffffffff [31:0] GITREF_RP2040 (-)
45 io_ro_32 gitref_rp2040;
46} sysinfo_hw_t;
47
48#define sysinfo_hw ((sysinfo_hw_t *)SYSINFO_BASE)
49static_assert(sizeof (sysinfo_hw_t) == 0x0014, "");
50
51#endif // _HARDWARE_STRUCTS_SYSINFO_H
52
address_mapped.h
sysinfo_hw_t
Definition: sysinfo.h:26