v2.0.0
tusb_config.h
1/*
2 * The MIT License (MIT)
3 *
4 * Copyright (c) 2020 Raspberry Pi (Trading) Ltd.
5 * Copyright (c) 2020 Damien P. George
6 *
7 * Permission is hereby granted, free of charge, to any person obtaining a copy
8 * of this software and associated documentation files (the "Software"), to deal
9 * in the Software without restriction, including without limitation the rights
10 * to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
11 * copies of the Software, and to permit persons to whom the Software is
12 * furnished to do so, subject to the following conditions:
13 *
14 * The above copyright notice and this permission notice shall be included in
15 * all copies or substantial portions of the Software.
16 *
17 * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
18 * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
19 * FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
20 * AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
21 * LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
22 * OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN
23 * THE SOFTWARE.
24 *
25 */
26
27#ifndef _PICO_STDIO_USB_TUSB_CONFIG_H
28#define _PICO_STDIO_USB_TUSB_CONFIG_H
29
30#include "pico/stdio_usb.h"
31
32#if !defined(LIB_TINYUSB_HOST) && !defined(LIB_TINYUSB_DEVICE)
33#define CFG_TUSB_RHPORT0_MODE (OPT_MODE_DEVICE)
34
35#define CFG_TUD_CDC (1)
36#define CFG_TUD_CDC_RX_BUFSIZE (256)
37#define CFG_TUD_CDC_TX_BUFSIZE (256)
38
39// We use a vendor specific interface but with our own driver
40// Vendor driver only used for Microsoft OS 2.0 descriptor
41#if !PICO_STDIO_USB_RESET_INTERFACE_SUPPORT_MS_OS_20_DESCRIPTOR
42#define CFG_TUD_VENDOR (0)
43#else
44#define CFG_TUD_VENDOR (1)
45#define CFG_TUD_VENDOR_RX_BUFSIZE (256)
46#define CFG_TUD_VENDOR_TX_BUFSIZE (256)
47#endif
48#endif
49
50#endif