v2.0.0
Public Member Functions | Data Fields
otp_hw_t Struct Reference

## Public Member Functions
| _REG_ (OTP_SW_LOCK0_OFFSET) io_rw_32 sw_lock[64]
| _REG_ (OTP_SBPI_INSTR_OFFSET) io_rw_32 sbpi_instr
| _REG_ (OTP_SBPI_WDATA_0_OFFSET) io_rw_32 sbpi_wdata[4]
| _REG_ (OTP_SBPI_RDATA_0_OFFSET) io_ro_32 sbpi_rdata[4]
| _REG_ (OTP_SBPI_STATUS_OFFSET) io_rw_32 sbpi_status
| _REG_ (OTP_USR_OFFSET) io_rw_32 usr
| _REG_ (OTP_DBG_OFFSET) io_rw_32 dbg
| _REG_ (OTP_BIST_OFFSET) io_rw_32 bist
| _REG_ (OTP_CRT_KEY_W0_OFFSET) io_wo_32 crt_key_w[4]
| _REG_ (OTP_CRITICAL_OFFSET) io_ro_32 critical
| _REG_ (OTP_KEY_VALID_OFFSET) io_ro_32 key_valid
| _REG_ (OTP_DEBUGEN_OFFSET) io_rw_32 debugen
| _REG_ (OTP_DEBUGEN_LOCK_OFFSET) io_rw_32 debugen_lock
| _REG_ (OTP_ARCHSEL_OFFSET) io_rw_32 archsel
| _REG_ (OTP_ARCHSEL_STATUS_OFFSET) io_ro_32 archsel_status
| _REG_ (OTP_BOOTDIS_OFFSET) io_rw_32 bootdis
| _REG_ (OTP_INTR_OFFSET) io_rw_32 intr
| _REG_ (OTP_INTE_OFFSET) io_rw_32 inte
| _REG_ (OTP_INTF_OFFSET) io_rw_32 intf
| _REG_ (OTP_INTS_OFFSET) io_ro_32 ints

## Data Fields
uint32_t | _pad0

The documentation for this struct was generated from the following file:

- include/hardware/structs/otp.h