Simulink Model Reference Conversion Advisor Report - dsogi_pll_3ph.slx
Simulink version: 10.7 | Model version: 1.83
System: dsogi_pll_3ph | Current run: 26-May-2024 17:35:16
Treat as Referenced Model: off |

^ Check subsystem content

Check failed
Model 'dsogi_pll_3ph' does not compile due to the following issues:.

- Error due to multiple causes.
  - Cannot solve algebraic loop involving 'dsogi_pll_3ph/pll_dsogi_system/SC/PSC/sum1' because it consists of blocks that cannot be assigned algebraic variables, such as blocks with discrete-valued outputs, blocks with non-double or complex outputs, Stateflow blocks, or nonvirtual subsystems. Consider breaking the algebraic loop. For example, add a delay or a memory block to the loop. To see more details about the loops use the command Simulink.BlockDiagram.getAlgebraicLoops(bdroot)
  - Algebraic loop error with 'dsogi_pll_3ph/pll_dsogi_system/DSOGI/Dsogi alpha/dsogi/alpha_sogi'
  - Algebraic loop error with 'dsogi_pll_3ph/pll_dsogi_system/prl_dco'
  - Algebraic loop error with 'dsogi_pll_3ph/pll_dsogi_system/SC/PSC/a-b1'
  - Algebraic loop error with 'dsogi_pll_3ph/pll_dsogi_system/DSOGI/Dsogi alpha1/Subsystem Reference/alpha_sogi'
  - Algebraic loop error with 'dsogi_pll_3ph/pll_dsogi_system/SC/PSC/sum1'

Note:

- Unable to convert subsystem 'dsogi_pll_3ph/pll_dsogi_system/prl_dco' to a referenced model. Click here to restore the original model.