# Problem Statement

Create a 16-bit wide, 9-to-1 multiplexer. sel=0 chooses a, sel=1 chooses b, etc. For the unused cases (sel=9 to 15), set all output bits to '1'.

> [!TIP]
> With this many options, a case statement may be useful.