# TextToSpeechCloseInMemory

The TextToSpeechCloseInMemory call terminates the speech-to-memory capability and returns to the startup state. The speech samples are then ignored or sent to an audio device, depending on the setting of the dwDeviceOptions parameter in the startup function.

Syntax | MMRESULT TextToSpeechCloseInMemory | (LPTTS_HANDLE_T phTTS)
Parameters | LPTTS_HANDLE_T phTTS | Specifies a text-to-speech handle.
Return Value | This call returns a value of type MMRESULT. The value is zero if the call is successful. The return value is one of the following constants:
Constant | Description
MMSYSERR_NOERROR | Normal successful completion (zero).
MMSYSERR_ERROR | Output to memory not enabled or unable to create a system object.
MMSYSERR_INVALHANDLE | The text-to-speech handle was invalid.
Comments | TextToSpeechOpenInMemory must be called before calling TextToSpeechCloseInMemory.
See Also | TextToSpeechOpenInMemory